// SPDX-License-Identifier: GPL-2.0
/*
 * IPQ5424 RDP466 board device tree source
 *
 * Copyright (c) 2025 The Linux Foundation. All rights reserved.
 */

/ {
	/* Will be removed when SMEM parsing is updated */
	memory@80000000 {
		device_type = "memory";
		reg = <0x0 0x80000000 0x0 0x20000000>;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};
};

	&sdhc {
		sdhci-caps-mask = <0x0 0x04000000>;
		sdhci-caps = <0x0 0x04000000>;	/* SDHCI_CAN_VDD_180 */
		mmc-ddr-1_8v;
		mmc-hs200-1_8v;
		max-frequency = <192000000>;
		bus-width = <4>;
		pinctrl-0 = <&qpic_snand_default_state>;
		pinctrl-names = "default";
		non-removable;

		/*
		 * This reset is needed to clear out the settings done by
		 * previous boot loader. Without this the SDHCI_RESET_ALL
		 * reset done sdhci_init() times out.
		 */
		resets = <&gcc GCC_SDCC_BCR>;

		status = "okay";
	};

