// SPDX-License-Identifier: GPL-2.0+
/*
 * Copyright (C) 2018 Álvaro Fernández Rojas <noltari@gmail.com>
 */

#include <dt-bindings/clock/bcm6318-clock.h>
#include <dt-bindings/dma/bcm6318-dma.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/power-domain/bcm6318-power-domain.h>
#include <dt-bindings/reset/bcm6318-reset.h>
#include "skeleton.dtsi"

/ {
	compatible = "brcm,bcm6318";

	aliases {
		spi0 = &spi;
	};

	cpus {
		reg = <0x10000000 0x4>;
		#address-cells = <1>;
		#size-cells = <0>;
		bootph-all;

		cpu@0 {
			compatible = "brcm,bcm6318-cpu", "mips,mips4Kc";
			device_type = "cpu";
			reg = <0>;
			bootph-all;
		};
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		bootph-all;

		hsspi_pll: hsspi-pll {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <250000000>;
		};

		periph_osc: periph-osc {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <50000000>;
			bootph-all;
		};

		periph_clk: periph-clk {
			compatible = "brcm,bcm6345-clk";
			reg = <0x10000004 0x4>;
			#clock-cells = <1>;
		};

		ubus_clk: ubus-clk {
			compatible = "brcm,bcm6345-clk";
			reg = <0x10000008 0x4>;
			#clock-cells = <1>;
		};
	};

	ubus {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		bootph-all;

		periph_rst: reset-controller@10000010 {
			compatible = "brcm,bcm6345-reset";
			reg = <0x10000010 0x4>;
			#reset-cells = <1>;
		};

		wdt: watchdog@10000068 {
			compatible = "brcm,bcm6345-wdt";
			reg = <0x10000068 0xc>;
			clocks = <&periph_osc>;
		};

		wdt-reboot {
			compatible = "wdt-reboot";
			wdt = <&wdt>;
		};

		pll_cntl: syscon@10000074 {
			compatible = "syscon";
			reg = <0x10000074 0x4>;
		};

		syscon-reboot {
			compatible = "syscon-reboot";
			regmap = <&pll_cntl>;
			offset = <0x0>;
			mask = <0x1>;
		};

		gpio1: gpio-controller@10000080 {
			compatible = "brcm,bcm6345-gpio";
			reg = <0x10000080 0x4>, <0x10000088 0x4>;
			gpio-controller;
			#gpio-cells = <2>;
			ngpios = <18>;

			status = "disabled";
		};

		gpio0: gpio-controller@10000084 {
			compatible = "brcm,bcm6345-gpio";
			reg = <0x10000084 0x4>, <0x1000008c 0x4>;
			gpio-controller;
			#gpio-cells = <2>;

			status = "disabled";
		};

		uart0: serial@10000100 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000100 0x18>;
			clocks = <&periph_osc>;

			status = "disabled";
		};

		leds: led-controller@10000200 {
			compatible = "brcm,bcm6328-leds";
			reg = <0x10000200 0x28>;
			#address-cells = <1>;
			#size-cells = <0>;

			status = "disabled";
		};

		periph_pwr: power-controller@100008e8 {
			compatible = "brcm,bcm6328-power-domain";
			reg = <0x100008e8 0x4>;
			#power-domain-cells = <1>;
		};

		spi: spi@10003000 {
			compatible = "brcm,bcm6328-hsspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x10003000 0x600>;
			clocks = <&periph_clk BCM6318_CLK_HSSPI>, <&hsspi_pll>;
			clock-names = "hsspi", "pll";
			resets = <&periph_rst BCM6318_RST_SPI>;
			spi-max-frequency = <33333334>;
			num-cs = <3>;

			status = "disabled";
		};

		memory-controller@10004000 {
			compatible = "brcm,bcm6318-mc";
			reg = <0x10004000 0x38>;
			bootph-all;
		};

		ehci: usb-controller@10005000 {
			compatible = "brcm,bcm6318-ehci", "generic-ehci";
			reg = <0x10005000 0x100>;
			phys = <&usbh>;
			big-endian;

			status = "disabled";
		};

		ohci: usb-controller@10005100 {
			compatible = "brcm,bcm6318-ohci", "generic-ohci";
			reg = <0x10005100 0x100>;
			phys = <&usbh>;
			big-endian;

			status = "disabled";
		};

		usbh: usb-phy@10005200 {
			compatible = "brcm,bcm6318-usbh";
			reg = <0x10005200 0x30>;
			#phy-cells = <0>;
			clocks = <&periph_clk BCM6318_CLK_USB>;
			clock-names = "usbh";
			power-domains = <&periph_pwr BCM6318_PWR_USB>;
			resets = <&periph_rst BCM6318_RST_USBH>;

			status = "disabled";
		};

		enet: ethernet@10080000 {
			compatible = "brcm,bcm6368-enet";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x10080000 0x8000>;
			clocks = <&periph_clk BCM6318_CLK_ROBOSW250>,
				 <&periph_clk BCM6318_CLK_ROBOSW025>,
				 <&ubus_clk BCM6318_UCLK_ROBOSW>;
			resets = <&periph_rst BCM6318_RST_ENETSW>,
				 <&periph_rst BCM6318_RST_EPHY>;
			dmas = <&iudma BCM6318_DMA_ENETSW_RX>,
			       <&iudma BCM6318_DMA_ENETSW_TX>;
			dma-names = "rx",
				    "tx";
			brcm,num-ports = <5>;

			status = "disabled";
		};

		iudma: dma-controller@10088000 {
			compatible = "brcm,bcm6368-iudma";
			reg = <0x10088000 0x80>,
			      <0x10088200 0x80>,
			      <0x10088400 0x80>;
			reg-names = "dma",
				    "dma-channels",
				    "dma-sram";
			#dma-cells = <1>;
			dma-channels = <8>;
		};
	};
};
