/*
 * at91sam9263.dtsi - Device Tree Include file for AT91SAM9263 family SoC
 *
 *  Copyright (C) 2012 Jean-Christophe PLAGNIOL-VILLARD <plagnioj@jcrosoft.com>
 *
 * Licensed under GPLv2 only.
 */

#include "skeleton.dtsi"
#include <dt-bindings/pinctrl/at91.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/clock/at91.h>

/ {
	model = "Atmel AT91SAM9263 family SoC";
	compatible = "atmel,at91sam9263";
	interrupt-parent = <&aic>;

	aliases {
		serial0 = &dbgu;
		serial1 = &usart0;
		serial2 = &usart1;
		serial3 = &usart2;
		gpio0 = &pioA;
		gpio1 = &pioB;
		gpio2 = &pioC;
		gpio3 = &pioD;
		gpio4 = &pioE;
		tcb0 = &tcb0;
		i2c0 = &i2c0;
		ssc0 = &ssc0;
		ssc1 = &ssc1;
		pwm0 = &pwm0;
		spi0 = &spi0;
	};

	cpus {
		cpu {
			compatible = "arm,arm926ej-s";
			device_type = "cpu";
		};
	};

	memory {
		reg = <0x20000000 0x08000000>;
	};

	clocks {
		main_xtal: main_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		slow_xtal: slow_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
	};

	sram0: sram@00300000 {
		compatible = "mmio-sram";
		reg = <0x00300000 0x14000>;
	};

	sram1: sram@00500000 {
		compatible = "mmio-sram";
		reg = <0x00500000 0x4000>;
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		bootph-all;

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			bootph-all;

			aic: interrupt-controller@fffff000 {
				#interrupt-cells = <3>;
				compatible = "atmel,at91rm9200-aic";
				interrupt-controller;
				reg = <0xfffff000 0x200>;
				atmel,external-irqs = <30 31>;
			};

			pmc: pmc@fffffc00 {
				compatible = "atmel,at91rm9200-pmc", "syscon";
				reg = <0xfffffc00 0x100>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				interrupt-controller;
				#address-cells = <1>;
				#size-cells = <0>;
				#interrupt-cells = <1>;
				bootph-all;

				main_osc: main_osc {
					compatible = "atmel,at91rm9200-clk-main-osc";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_MOSCS>;
					clocks = <&main_xtal>;
				};

				main: mainck {
					compatible = "atmel,at91rm9200-clk-main";
					#clock-cells = <0>;
					clocks = <&main_osc>;
				};

				plla: pllack@0 {
					compatible = "atmel,at91rm9200-clk-pll";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_LOCKA>;
					clocks = <&main>;
					reg = <0>;
					atmel,clk-input-range = <1000000 32000000>;
					#atmel,pll-clk-output-range-cells = <4>;
					atmel,pll-clk-output-ranges = <80000000 200000000 0 1>,
								<190000000 240000000 2 1>;
				};

				pllb: pllbck@1 {
					compatible = "atmel,at91rm9200-clk-pll";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_LOCKB>;
					clocks = <&main>;
					reg = <1>;
					atmel,clk-input-range = <1000000 32000000>;
					#atmel,pll-clk-output-range-cells = <4>;
					atmel,pll-clk-output-ranges = <80000000 200000000 0 1>,
								<190000000 240000000 2 1>;
				};

				mck: masterck {
					compatible = "atmel,at91rm9200-clk-master";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_MCKRDY>;
					clocks = <&slow_xtal>, <&main>, <&plla>, <&pllb>;
					atmel,clk-output-range = <0 120000000>;
					atmel,clk-divisors = <1 2 4 0>;
					bootph-all;
				};

				usb: usbck {
					compatible = "atmel,at91rm9200-clk-usb";
					#clock-cells = <0>;
					atmel,clk-divisors = <1 2 4 0>;
					clocks = <&pllb>;
				};

				prog: progck {
					compatible = "atmel,at91rm9200-clk-programmable";
					#address-cells = <1>;
					#size-cells = <0>;
					interrupt-parent = <&pmc>;
					clocks = <&slow_xtal>, <&main>, <&plla>, <&pllb>;

					prog0: prog@0 {
						#clock-cells = <0>;
						reg = <0>;
						interrupts = <AT91_PMC_PCKRDY(0)>;
					};

					prog1: prog@1 {
						#clock-cells = <0>;
						reg = <1>;
						interrupts = <AT91_PMC_PCKRDY(1)>;
					};

					prog2: prog@2 {
						#clock-cells = <0>;
						reg = <2>;
						interrupts = <AT91_PMC_PCKRDY(2)>;
					};

					prog3: prog@3 {
						#clock-cells = <0>;
						reg = <3>;
						interrupts = <AT91_PMC_PCKRDY(3)>;
					};
				};

				systemck {
					compatible = "atmel,at91rm9200-clk-system";
					#address-cells = <1>;
					#size-cells = <0>;

					uhpck: uhpck@6 {
						#clock-cells = <0>;
						reg = <6>;
						clocks = <&usb>;
					};

					udpck: udpck@7 {
						#clock-cells = <0>;
						reg = <7>;
						clocks = <&usb>;
					};

					pck0: pck0@8 {
						#clock-cells = <0>;
						reg = <8>;
						clocks = <&prog0>;
					};

					pck1: pck1@9 {
						#clock-cells = <0>;
						reg = <9>;
						clocks = <&prog1>;
					};

					pck2: pck2@10 {
						#clock-cells = <0>;
						reg = <10>;
						clocks = <&prog2>;
					};

					pck3: pck3@11 {
						#clock-cells = <0>;
						reg = <11>;
						clocks = <&prog3>;
					};
				};

				periphck {
					compatible = "atmel,at91rm9200-clk-peripheral";
					#address-cells = <1>;
					#size-cells = <0>;
					clocks = <&mck>;
					bootph-all;

					pioA_clk: pioA_clk@2 {
						#clock-cells = <0>;
						reg = <2>;
						bootph-all;
					};

					pioB_clk: pioB_clk@3 {
						#clock-cells = <0>;
						reg = <3>;
						bootph-all;
					};

					pioCDE_clk: pioCDE_clk@4 {
						#clock-cells = <0>;
						reg = <4>;
						bootph-all;
					};

					usart0_clk: usart0_clk@7 {
						#clock-cells = <0>;
						reg = <7>;
					};

					usart1_clk: usart1_clk@8 {
						#clock-cells = <0>;
						reg = <8>;
					};

					usart2_clk: usart2_clk@9 {
						#clock-cells = <0>;
						reg = <9>;
					};

					mci0_clk: mci0_clk@10 {
						#clock-cells = <0>;
						reg = <10>;
					};

					mci1_clk: mci1_clk@11 {
						#clock-cells = <0>;
						reg = <11>;
					};

					can_clk: can_clk@12 {
						#clock-cells = <0>;
						reg = <12>;
					};

					twi0_clk: twi0_clk@13 {
						#clock-cells = <0>;
						reg = <13>;
					};

					spi0_clk: spi0_clk@14 {
						#clock-cells = <0>;
						reg = <14>;
					};

					spi1_clk: spi1_clk@15 {
						#clock-cells = <0>;
						reg = <15>;
					};

					ssc0_clk: ssc0_clk@16 {
						#clock-cells = <0>;
						reg = <16>;
					};

					ssc1_clk: ssc1_clk@17 {
						#clock-cells = <0>;
						reg = <17>;
					};

					ac97_clk: ac97_clk@18 {
						#clock-cells = <0>;
						reg = <18>;
					};

					tcb_clk: tcb_clk@19 {
						#clock-cells = <0>;
						reg = <19>;
					};

					pwm_clk: pwm_clk@20 {
						#clock-cells = <0>;
						reg = <20>;
					};

					macb0_clk: macb0_clk@21 {
						#clock-cells = <0>;
						reg = <21>;
					};

					g2de_clk: g2de_clk@23 {
						#clock-cells = <0>;
						reg = <23>;
					};

					udc_clk: udc_clk@24 {
						#clock-cells = <0>;
						reg = <24>;
					};

					isi_clk: isi_clk@25 {
						#clock-cells = <0>;
						reg = <25>;
					};

					lcd_clk: lcd_clk@26 {
						#clock-cells = <0>;
						reg = <26>;
					};

					dma_clk: dma_clk@27 {
						#clock-cells = <0>;
						reg = <27>;
					};

					ohci_clk: ohci_clk@29 {
						#clock-cells = <0>;
						reg = <29>;
					};
				};
			};

			ramc0: ramc@ffffe200 {
				compatible = "atmel,at91sam9260-sdramc";
				reg = <0xffffe200 0x200>;
			};

			ramc1: ramc@ffffe800 {
				compatible = "atmel,at91sam9260-sdramc";
				reg = <0xffffe800 0x200>;
			};

			pit: timer@fffffd30 {
				compatible = "atmel,at91sam9260-pit";
				reg = <0xfffffd30 0xf>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&mck>;
			};

			tcb0: timer@fff7c000 {
				compatible = "atmel,at91rm9200-tcb";
				reg = <0xfff7c000 0x100>;
				interrupts = <19 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&tcb_clk>, <&slow_xtal>;
				clock-names = "t0_clk", "slow_clk";
			};

			rstc@fffffd00 {
				compatible = "atmel,at91sam9260-rstc";
				reg = <0xfffffd00 0x10>;
				clocks = <&slow_xtal>;
			};

			shdwc@fffffd10 {
				compatible = "atmel,at91sam9260-shdwc";
				reg = <0xfffffd10 0x10>;
				clocks = <&slow_xtal>;
			};

			pinctrl@fffff200 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "atmel,at91rm9200-pinctrl", "simple-bus";
				ranges = <0xfffff200 0xfffff200 0xa00>;

				atmel,mux-mask = <
				      /*    A         B     */
				       0xfffffffb 0xffffe07f  /* pioA */
				       0x0007ffff 0x39072fff  /* pioB */
				       0xffffffff 0x3ffffff8  /* pioC */
				       0xfffffbff 0xffffffff  /* pioD */
				       0xffe00fff 0xfbfcff00  /* pioE */
				      >;

				/* shared pinctrl settings */
				dbgu {
					pinctrl_dbgu: dbgu-0 {
						atmel,pins =
							<AT91_PIOC 30 AT91_PERIPH_A AT91_PINCTRL_PULL_UP
							 AT91_PIOC 31 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};
				};

				usart0 {
					pinctrl_usart0: usart0-0 {
						atmel,pins =
							<AT91_PIOA 26 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA26 periph A with pullup */
							 AT91_PIOA 27 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA27 periph A */
					};

					pinctrl_usart0_rts: usart0_rts-0 {
						atmel,pins =
							<AT91_PIOA 28 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA28 periph A */
					};

					pinctrl_usart0_cts: usart0_cts-0 {
						atmel,pins =
							<AT91_PIOA 29 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA29 periph A */
					};
				};

				usart1 {
					pinctrl_usart1: usart1-0 {
						atmel,pins =
							<AT91_PIOD 0 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD0 periph A with pullup */
							 AT91_PIOD 1 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD1 periph A */
					};

					pinctrl_usart1_rts: usart1_rts-0 {
						atmel,pins =
							<AT91_PIOD 7 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PD7 periph B */
					};

					pinctrl_usart1_cts: usart1_cts-0 {
						atmel,pins =
							<AT91_PIOD 8 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PD8 periph B */
					};
				};

				usart2 {
					pinctrl_usart2: usart2-0 {
						atmel,pins =
							<AT91_PIOD 2 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD2 periph A with pullup */
							 AT91_PIOD 3 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD3 periph A */
					};

					pinctrl_usart2_rts: usart2_rts-0 {
						atmel,pins =
							<AT91_PIOD 5 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PD5 periph B */
					};

					pinctrl_usart2_cts: usart2_cts-0 {
						atmel,pins =
							<AT91_PIOD 6 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PD6 periph B */
					};
				};

				nand {
					pinctrl_nand: nand-0 {
						atmel,pins =
							<AT91_PIOA 22 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP	/* PA22 gpio RDY pin pull_up*/
							 AT91_PIOD 15 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP>;	/* PD15 gpio enable pin pull_up */
					};
				};

				macb {
					pinctrl_macb_rmii: macb_rmii-0 {
						atmel,pins =
							<AT91_PIOC 25 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC25 periph B */
							 AT91_PIOE 21 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE21 periph A */
							 AT91_PIOE 23 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE23 periph A */
							 AT91_PIOE 24 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE24 periph A */
							 AT91_PIOE 25 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE25 periph A */
							 AT91_PIOE 26 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE26 periph A */
							 AT91_PIOE 27 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE27 periph A */
							 AT91_PIOE 28 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE28 periph A */
							 AT91_PIOE 29 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE29 periph A */
							 AT91_PIOE 30 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PE30 periph A */
					};

					pinctrl_macb_rmii_mii: macb_rmii_mii-0 {
						atmel,pins =
							<AT91_PIOC 20 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC20 periph B */
							 AT91_PIOC 21 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC21 periph B */
							 AT91_PIOC 22 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC22 periph B */
							 AT91_PIOC 23 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC23 periph B */
							 AT91_PIOC 24 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC24 periph B */
							 AT91_PIOC 25 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC25 periph B */
							 AT91_PIOC 27 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC27 periph B */
							 AT91_PIOE 22 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PE22 periph B */
					};
				};

				mmc0 {
					pinctrl_mmc0_clk: mmc0_clk-0 {
						atmel,pins =
							<AT91_PIOA 12 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA12 periph A */
					};

					pinctrl_mmc0_slot0_cmd_dat0: mmc0_slot0_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 1 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA1 periph A with pullup */
							 AT91_PIOA 0 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA0 periph A with pullup */
					};

					pinctrl_mmc0_slot0_dat1_3: mmc0_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 3 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA3 periph A with pullup */
							 AT91_PIOA 4 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA4 periph A with pullup */
							 AT91_PIOA 5 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA5 periph A with pullup */
					};

					pinctrl_mmc0_slot1_cmd_dat0: mmc0_slot1_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 16 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA16 periph A with pullup */
							 AT91_PIOA 17 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA17 periph A with pullup */
					};

					pinctrl_mmc0_slot1_dat1_3: mmc0_slot1_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 18 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA18 periph A with pullup */
							 AT91_PIOA 19 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA19 periph A with pullup */
							 AT91_PIOA 20 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA20 periph A with pullup */
					};
				};

				mmc1 {
					pinctrl_mmc1_clk: mmc1_clk-0 {
						atmel,pins =
							<AT91_PIOA 6 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA6 periph A */
					};

					pinctrl_mmc1_slot0_cmd_dat0: mmc1_slot0_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 7 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA7 periph A with pullup */
							 AT91_PIOA 8 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA8 periph A with pullup */
					};

					pinctrl_mmc1_slot0_dat1_3: mmc1_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 9 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA9 periph A with pullup */
							 AT91_PIOA 10 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA10 periph A with pullup */
							 AT91_PIOA 11 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA11 periph A with pullup */
					};

					pinctrl_mmc1_slot1_cmd_dat0: mmc1_slot1_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 21 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA21 periph A with pullup */
							 AT91_PIOA 22 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA22 periph A with pullup */
					};

					pinctrl_mmc1_slot1_dat1_3: mmc1_slot1_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 23 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA23 periph A with pullup */
							 AT91_PIOA 24 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA24 periph A with pullup */
							 AT91_PIOA 25 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA25 periph A with pullup */
					};
				};

				ssc0 {
					pinctrl_ssc0_tx: ssc0_tx-0 {
						atmel,pins =
							<AT91_PIOB 0 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB0 periph B */
							 AT91_PIOB 1 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB1 periph B */
							 AT91_PIOB 2 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB2 periph B */
					};

					pinctrl_ssc0_rx: ssc0_rx-0 {
						atmel,pins =
							<AT91_PIOB 3 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB3 periph B */
							 AT91_PIOB 4 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB4 periph B */
							 AT91_PIOB 5 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB5 periph B */
					};
				};

				ssc1 {
					pinctrl_ssc1_tx: ssc1_tx-0 {
						atmel,pins =
							<AT91_PIOB 6 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB6 periph A */
							 AT91_PIOB 7 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB7 periph A */
							 AT91_PIOB 8 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB8 periph A */
					};

					pinctrl_ssc1_rx: ssc1_rx-0 {
						atmel,pins =
							<AT91_PIOB 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB9 periph A */
							 AT91_PIOB 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB10 periph A */
							 AT91_PIOB 11 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB11 periph A */
					};
				};

				spi0 {
					pinctrl_spi0: spi0-0 {
						atmel,pins =
							<AT91_PIOA 0 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA0 periph B SPI0_MISO pin */
							 AT91_PIOA 1 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA1 periph B SPI0_MOSI pin */
							 AT91_PIOA 2 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA2 periph B SPI0_SPCK pin */
					};
				};

				spi1 {
					pinctrl_spi1: spi1-0 {
						atmel,pins =
							<AT91_PIOB 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB12 periph A SPI1_MISO pin */
							 AT91_PIOB 13 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB13 periph A SPI1_MOSI pin */
							 AT91_PIOB 14 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB14 periph A SPI1_SPCK pin */
					};
				};

				tcb0 {
					pinctrl_tcb0_tclk0: tcb0_tclk0-0 {
						atmel,pins = <AT91_PIOB 28 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk1: tcb0_tclk1-0 {
						atmel,pins = <AT91_PIOC 28 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk2: tcb0_tclk2-0 {
						atmel,pins = <AT91_PIOA 15 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa0: tcb0_tioa0-0 {
						atmel,pins = <AT91_PIOE 18 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa1: tcb0_tioa1-0 {
						atmel,pins = <AT91_PIOE 8 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa2: tcb0_tioa2-0 {
						atmel,pins = <AT91_PIOB 17 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob0: tcb0_tiob0-0 {
						atmel,pins = <AT91_PIOE 19 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob1: tcb0_tiob1-0 {
						atmel,pins = <AT91_PIOE 9 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob2: tcb0_tiob2-0 {
						atmel,pins = <AT91_PIOB 18 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};
				};

				fb {
					pinctrl_fb: fb-0 {
						atmel,pins =
							<AT91_PIOC 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC1 periph A */
							 AT91_PIOC 2 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC2 periph A */
							 AT91_PIOC 3 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC3 periph A */
							 AT91_PIOB 9 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB9 periph B */
							 AT91_PIOC 6 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC6 periph A */
							 AT91_PIOC 7 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC7 periph A */
							 AT91_PIOC 8 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC8 periph A */
							 AT91_PIOC 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC9 periph A */
							 AT91_PIOC 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC10 periph A */
							 AT91_PIOC 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC11 periph A */
							 AT91_PIOC 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC14 periph A */
							 AT91_PIOC 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC15 periph A */
							 AT91_PIOC 16 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC16 periph A */
							 AT91_PIOC 12 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC12 periph B */
							 AT91_PIOC 18 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC18 periph A */
							 AT91_PIOC 19 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC19 periph A */
							 AT91_PIOC 22 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC22 periph A */
							 AT91_PIOC 23 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC23 periph A */
							 AT91_PIOC 24 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC24 periph A */
							 AT91_PIOC 17 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC17 periph B */
							 AT91_PIOC 26 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC26 periph A */
							 AT91_PIOC 27 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PC27 periph A */
					};
				};

				can {
					pinctrl_can_rx_tx: can_rx_tx {
						atmel,pins =
							<AT91_PIOA 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* CANRX, conflicts with IRQ0 */
							 AT91_PIOA 13 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* CANTX, conflicts with PCK0 */
					};
				};

				ac97 {
					pinctrl_ac97: ac97-0 {
						atmel,pins =
							<AT91_PIOB 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB12 periph A AC97FS pin */
							 AT91_PIOB 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB13 periph A AC97CK pin */
							 AT91_PIOB 2 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB14 periph A AC97TX pin */
							 AT91_PIOB 3 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB14 periph A AC97RX pin */
					};
				};

				pioA: gpio@fffff200 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff200 0x200>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioA_clk>;
					bootph-all;
				};

				pioB: gpio@fffff400 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff400 0x200>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioB_clk>;
					bootph-all;
				};

				pioC: gpio@fffff600 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff600 0x200>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioCDE_clk>;
					bootph-all;
				};

				pioD: gpio@fffff800 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff800 0x200>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioCDE_clk>;
					bootph-all;
				};

				pioE: gpio@fffffa00 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffffa00 0x200>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioCDE_clk>;
					bootph-all;
				};
			};

			dbgu: serial@ffffee00 {
				compatible = "atmel,at91sam9260-dbgu", "atmel,at91sam9260-usart";
				reg = <0xffffee00 0x200>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_dbgu>;
				clocks = <&mck>;
				clock-names = "usart";
				status = "disabled";
			};

			usart0: serial@fff8c000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff8c000 0x200>;
				interrupts = <7 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart0>;
				clocks = <&usart0_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart1: serial@fff90000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff90000 0x200>;
				interrupts = <8 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart1>;
				clocks = <&usart1_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart2: serial@fff94000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff94000 0x200>;
				interrupts = <9 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart2>;
				clocks = <&usart2_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			ssc0: ssc@fff98000 {
				compatible = "atmel,at91rm9200-ssc";
				reg = <0xfff98000 0x4000>;
				interrupts = <16 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc0_tx &pinctrl_ssc0_rx>;
				clocks = <&ssc0_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			ssc1: ssc@fff9c000 {
				compatible = "atmel,at91rm9200-ssc";
				reg = <0xfff9c000 0x4000>;
				interrupts = <17 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc1_tx &pinctrl_ssc1_rx>;
				clocks = <&ssc1_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			ac97: sound@fffa0000 {
				compatible = "atmel,at91sam9263-ac97c";
				reg = <0xfffa0000 0x4000>;
				interrupts = <18 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ac97>;
				clocks = <&ac97_clk>;
				clock-names = "ac97_clk";
				status = "disabled";
			};

			macb0: ethernet@fffbc000 {
				compatible = "cdns,at91sam9260-macb", "cdns,macb";
				reg = <0xfffbc000 0x100>;
				interrupts = <21 IRQ_TYPE_LEVEL_HIGH 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_macb_rmii>;
				clocks = <&macb0_clk>, <&macb0_clk>;
				clock-names = "hclk", "pclk";
				status = "disabled";
			};

			usb1: gadget@fff78000 {
				compatible = "atmel,at91sam9263-udc";
				reg = <0xfff78000 0x4000>;
				interrupts = <24 IRQ_TYPE_LEVEL_HIGH 2>;
				clocks = <&udc_clk>, <&udpck>;
				clock-names = "pclk", "hclk";
				status = "disabled";
			};

			i2c0: i2c@fff88000 {
				compatible = "atmel,at91sam9260-i2c";
				reg = <0xfff88000 0x100>;
				interrupts = <13 IRQ_TYPE_LEVEL_HIGH 6>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi0_clk>;
				status = "disabled";
			};

			mmc0: mmc@fff80000 {
				compatible = "atmel,hsmci";
				reg = <0xfff80000 0x600>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH 0>;
				pinctrl-names = "default";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci0_clk>;
				clock-names = "mci_clk";
				status = "disabled";
			};

			mmc1: mmc@fff84000 {
				compatible = "atmel,hsmci";
				reg = <0xfff84000 0x600>;
				interrupts = <11 IRQ_TYPE_LEVEL_HIGH 0>;
				pinctrl-names = "default";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci1_clk>;
				clock-names = "mci_clk";
				status = "disabled";
			};

			watchdog@fffffd40 {
				compatible = "atmel,at91sam9260-wdt";
				reg = <0xfffffd40 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&slow_xtal>;
				atmel,watchdog-type = "hardware";
				atmel,reset-type = "all";
				atmel,dbg-halt;
				status = "disabled";
			};

			spi0: spi@fffa4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xfffa4000 0x200>;
				interrupts = <14 IRQ_TYPE_LEVEL_HIGH 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi0>;
				clocks = <&spi0_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			spi1: spi@fffa8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xfffa8000 0x200>;
				interrupts = <15 IRQ_TYPE_LEVEL_HIGH 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi1>;
				clocks = <&spi1_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			pwm0: pwm@fffb8000 {
				compatible = "atmel,at91sam9rl-pwm";
				reg = <0xfffb8000 0x300>;
				interrupts = <20 IRQ_TYPE_LEVEL_HIGH 4>;
				#pwm-cells = <3>;
				clocks = <&pwm_clk>;
				clock-names = "pwm_clk";
				status = "disabled";
			};

			can: can@fffac000 {
				compatible = "atmel,at91sam9263-can";
				reg = <0xfffac000 0x300>;
				interrupts = <12 IRQ_TYPE_LEVEL_HIGH 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_can_rx_tx>;
				clocks = <&can_clk>;
				clock-names = "can_clk";
			};

			rtc@fffffd20 {
				compatible = "atmel,at91sam9260-rtt";
				reg = <0xfffffd20 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&slow_xtal>;
				status = "disabled";
			};

			rtc@fffffd50 {
				compatible = "atmel,at91sam9260-rtt";
				reg = <0xfffffd50 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&slow_xtal>;
				status = "disabled";
			};

			gpbr: syscon@fffffd60 {
				compatible = "atmel,at91sam9260-gpbr", "syscon";
				reg = <0xfffffd60 0x50>;
				status = "disabled";
			};
		};

		fb0: fb@0x00700000 {
			compatible = "atmel,at91sam9263-lcdc";
			reg = <0x00700000 0x1000>;
			interrupts = <26 IRQ_TYPE_LEVEL_HIGH 3>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_fb>;
			clocks = <&lcd_clk>, <&lcd_clk>;
			clock-names = "lcdc_clk", "hclk";
			status = "disabled";
		};

		nand0: nand@40000000 {
			compatible = "atmel,at91rm9200-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40000000 0x10000000
			       0xffffe000 0x200
			      >;
			atmel,nand-addr-offset = <21>;
			atmel,nand-cmd-offset = <22>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;
			gpios = <&pioA 22 GPIO_ACTIVE_HIGH
				 &pioD 15 GPIO_ACTIVE_HIGH
				 0
				>;
			status = "disabled";
		};

		usb0: ohci@00a00000 {
			compatible = "atmel,at91rm9200-ohci", "usb-ohci";
			reg = <0x00a00000 0x100000>;
			interrupts = <29 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&ohci_clk>, <&ohci_clk>, <&uhpck>;
			clock-names = "ohci_clk", "hclk", "uhpck";
			status = "disabled";
		};
	};

	i2c-gpio-0 {
		compatible = "i2c-gpio";
		gpios = <&pioB 4 GPIO_ACTIVE_HIGH /* sda */
			 &pioB 5 GPIO_ACTIVE_HIGH /* scl */
			>;
		i2c-gpio,sda-open-drain;
		i2c-gpio,scl-open-drain;
		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};
};
