// SPDX-License-Identifier: GPL-2.0+
/*
 * Skeleton device tree; the bare minimum needed to boot; just include and
 * add a compatible value.  The bootloader will typically populate the memory
 * node.
 */

/ {
	#address-cells = <1>;
	#size-cells = <1>;

	chosen {
	};

	aliases {
	};

	memory {
		device_type = "memory";
		reg = <0 0>;
	};
};
