// SPDX-License-Identifier: BSD-3-Clause
/*
 * Copyright (c) 2024 Linaro Ltd.
 */
/ {
	/* When running as the primary bootloader there is no prior
	 * stage to populate the memory layout for us. We *should*
	 * have two nodes here, but ABL does NOT like that.
	 * sooo we're stuck with this.
	 */
	memory@80000000 {
		device_type = "memory";
		reg = <0 0x80000000 0 0x3A800000>,
		      <0 0xC0000000 0 0x01800000>,
		      <0 0xC3400000 0 0x3CC00000>,
		      <1 0x00000000 1 0x00000000>;
	};
};

// RAM Entry 0 : Base 0x0080000000  Size 0x003A800000
// RAM Entry 1 : Base 0x00C0000000  Size 0x0001800000
// RAM Entry 2 : Base 0x00C3400000  Size 0x003CC00000
// RAM Entry 3 : Base 0x0100000000  Size 0x0100000000
