/*
 * Copyright (C) 2017 Jelle van der Waa <jelle@vdwaa.nl>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun8i-h3.dtsi"
#include "sunxi-common-regulators.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	model = "FriendlyARM NanoPi NEO Air";
	compatible = "friendlyarm,nanopi-neo-air", "allwinner,sun8i-h3";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "nanopi:green:pwr";
			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>; /* PL10 */
			default-state = "on";
		};

		led-1 {
			label = "nanopi:blue:status";
			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>; /* PA10 */
		};
	};

	wifi_pwrseq: pwrseq {
		compatible = "mmc-pwrseq-simple";
		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
	status = "okay";
};

&mmc1 {
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc3v3>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	brcmf: wifi@1 {
		reg = <1>;
		compatible = "brcm,bcm4329-fmac";
		interrupt-parent = <&pio>;
		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10 / EINT10 */
		interrupt-names = "host-wake";
	};
};

&mmc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc2_8bit_pins>;
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc3v3>;
	bus-width = <8>;
	non-removable;
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pa_pins>;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart3_pins>, <&uart3_rts_cts_pins>;
	uart-has-rtscts;
	status = "okay";

	bluetooth {
		compatible = "brcm,bcm43438-bt";
		clocks = <&rtc CLK_OSC32K_FANOUT>;
		clock-names = "lpo";
		vbat-supply = <&reg_vcc3v3>;
		vddio-supply = <&reg_vcc3v3>;
		device-wakeup-gpios = <&pio 0 8 GPIO_ACTIVE_HIGH>; /* PA8 */
		host-wakeup-gpios = <&pio 0 7 GPIO_ACTIVE_HIGH>; /* PA7 */
		shutdown-gpios = <&pio 6 13 GPIO_ACTIVE_HIGH>; /* PG13 */
	};
};

&usbphy {
	/* USB VBUS is always on */
	status = "okay";
};
