// SPDX-License-Identifier: GPL-2.0+ OR X11
/*
 * NXP lx2160a SOC common device tree source
 *
 * Copyright 2018-2021, 2023 NXP
 *
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>

/ {
	compatible = "fsl,lx2160a";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	memory@80000000 {
		device_type = "memory";
		reg = <0x00000000 0x80000000 0 0x80000000>;
		      /* DRAM space - 1, size : 2 GB DRAM */
	};

	sysclk: sysclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "sysclk";
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		dma-ranges = <0x0 0x0 0x0 0x0 0x10000 0x00000000>;

		uart0: serial@21c0000 {
			compatible = "arm,sbsa-uart","arm,pl011";
			reg = <0x0 0x21c0000 0x0 0x1000>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
			current-speed = <115200>;
			status = "disabled";
			bootph-all;
		};

		uart1: serial@21d0000 {
			compatible = "arm,sbsa-uart","arm,pl011";
			reg = <0x0 0x21d0000 0x0 0x1000>;
			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
			current-speed = <115200>;
			status = "disabled";
			bootph-all;
		};

		uart2: serial@21e0000 {
			compatible = "arm,sbsa-uart","arm,pl011";
			reg = <0x0 0x21e0000 0x0 0x1000>;
			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
			current-speed = <115200>;
			status = "disabled";
			bootph-all;
		};

		uart3: serial@21f0000 {
			compatible = "arm,sbsa-uart","arm,pl011";
			reg = <0x0 0x21f0000 0x0 0x1000>;
			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
			current-speed = <115200>;
			status = "disabled";
			bootph-all;
		};
	};

	crypto: crypto@8000000 {
		compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
		fsl,sec-era = <10>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x0 0x00 0x8000000 0x100000>;
		reg = <0x00 0x8000000 0x0 0x100000>;
		interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
		dma-coherent;

		sec_jr0: jr@10000 {
			compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg        = <0x10000 0x10000>;
			interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
		};

		sec_jr1: jr@20000 {
			compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg        = <0x20000 0x10000>;
			interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
		};

		sec_jr2: jr@30000 {
			compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg        = <0x30000 0x10000>;
			interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
		};

		sec_jr3: jr@40000 {
			compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg        = <0x40000 0x10000>;
			interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
		};
	};

	clockgen: clocking@1300000 {
		compatible = "fsl,ls2080a-clockgen";
		reg = <0 0x1300000 0 0xa0000>;
		#clock-cells = <2>;
		clocks = <&sysclk>;
	};

	gic: interrupt-controller@6000000 {
		compatible = "arm,gic-v3";
		reg = <0x0 0x06000000 0 0x10000>, /* GIC Dist */
		      <0x0 0x06200000 0 0x100000>; /* GICR */
		#interrupt-cells = <3>;
		interrupt-controller;
		interrupts = <1 9 0x4>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <1 13 0x8>, /* Physical Secure PPI, active-low */
			     <1 14 0x8>, /* Physical NS PPI, active-low */
			     <1 11 0x8>, /* Virtual PPI, active-low */
			     <1 10 0x8>; /* Hypervisor PPI, active-low */
	};

	fspi: spi@20c0000 {
		compatible = "nxp,lx2160a-fspi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x20c0000 0x0 0x10000>,
			<0x0 0x20000000 0x0 0x10000000>;
		reg-names = "fspi_base", "fspi_mmap";
		clocks = <&clockgen 4 3>, <&clockgen 4 3>;
		clock-names = "fspi_en", "fspi";
		interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
		status = "disabled";
	};

	i2c0: i2c@2000000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2000000 0x0 0x10000>;
		interrupts = <0 34 4>;
		scl-gpio = <&gpio2 15 0>;
		status = "disabled";
	};

	i2c1: i2c@2010000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2010000 0x0 0x10000>;
		interrupts = <0 34 4>;
		status = "disabled";
	};

	i2c2: i2c@2020000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2020000 0x0 0x10000>;
		interrupts = <0 35 4>;
		status = "disabled";
	};

	i2c3: i2c@2030000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2030000 0x0 0x10000>;
		interrupts = <0 35 4>;
		status = "disabled";
	};

	i2c4: i2c@2040000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2040000 0x0 0x10000>;
		interrupts = <0 74 4>;
		scl-gpio = <&gpio2 16 0>;
		status = "disabled";
	};

	i2c5: i2c@2050000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2050000 0x0 0x10000>;
		interrupts = <0 74 4>;
		status = "disabled";
	};

	i2c6: i2c@2060000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2060000 0x0 0x10000>;
		interrupts = <0 75 4>;
		status = "disabled";
	};

	i2c7: i2c@2070000 {
		compatible = "fsl,vf610-i2c";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2070000 0x0 0x10000>;
		interrupts = <0 75 4>;
		status = "disabled";
	};

	dspi0: spi@2100000 {
		compatible = "fsl,vf610-dspi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2100000 0x0 0x10000>;
		interrupts = <0 26 0x4>; /* Level high type */
		spi-num-chipselects = <6>;
	};

	dspi1: spi@2110000 {
		compatible = "fsl,vf610-dspi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2110000 0x0 0x10000>;
		interrupts = <0 26 0x4>; /* Level high type */
		spi-num-chipselects = <6>;
	};

	dspi2: spi@2120000 {
		compatible = "fsl,vf610-dspi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x0 0x2120000 0x0 0x10000>;
		interrupts = <0 241 0x4>; /* Level high type */
		spi-num-chipselects = <6>;
	};

	gpio0: gpio@2300000 {
		compatible = "fsl,qoriq-gpio";
		reg = <0x0 0x2300000 0x0 0x10000>;
		interrupts = <0 36 4>;
		gpio-controller;
		little-endian;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio1: gpio@2310000 {
		compatible = "fsl,qoriq-gpio";
		reg = <0x0 0x2310000 0x0 0x10000>;
		interrupts = <0 36 4>;
		gpio-controller;
		little-endian;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio2: gpio@2320000 {
		compatible = "fsl,qoriq-gpio";
		reg = <0x0 0x2320000 0x0 0x10000>;
		interrupts = <0 37 4>;
		gpio-controller;
		little-endian;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio3: gpio@2330000 {
		compatible = "fsl,qoriq-gpio";
		reg = <0x0 0x2330000 0x0 0x10000>;
		interrupts = <0 37 4>;
		gpio-controller;
		little-endian;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	wdt0: watchdog@23a0000 {
		compatible = "arm,sbsa-gwdt";
		reg = <0x0 0x23a0000 0 0x1000>,
		      <0x0 0x2390000 0 0x1000>;
		timeout-sec = <30>;
	};

	usb0: usb3@3100000 {
		compatible = "fsl,layerscape-dwc3";
		reg = <0x0 0x3100000 0x0 0x10000>;
		interrupts = <0 80 0x4>; /* Level high type */
		dr_mode = "host";
	};

	usb1: usb3@3110000 {
		compatible = "fsl,layerscape-dwc3";
		reg = <0x0 0x3110000 0x0 0x10000>;
		interrupts = <0 81 0x4>; /* Level high type */
		dr_mode = "host";
	};

	esdhc0: esdhc@2140000 {
		compatible = "fsl,esdhc";
		reg = <0x0 0x2140000 0x0 0x10000>;
		interrupts = <0 28 0x4>; /* Level high type */
		clocks = <&clockgen 4 1>;
		voltage-ranges = <1800 1800 3300 3300>;
		sdhci,auto-cmd12;
		little-endian;
		bus-width = <4>;
		status = "disabled";
	};

	esdhc1: esdhc@2150000 {
		compatible = "fsl,esdhc";
		reg = <0x0 0x2150000 0x0 0x10000>;
		interrupts = <0 63 0x4>; /* Level high type */
		clocks = <&clockgen 4 1>;
		voltage-ranges = <1800 1800 3300 3300>;
		sdhci,auto-cmd12;
		non-removable;
		little-endian;
		bus-width = <4>;
		status = "disabled";
	};

	sata0: sata@3200000 {
			compatible = "fsl,ls2080a-ahci";
			reg = <0x0 0x3200000 0x0 0x10000>;
			interrupts = <0 133 4>;
			clocks = <&clockgen 4 3>;
			status = "disabled";

	};

	sata1: sata@3210000 {
			compatible = "fsl,ls2080a-ahci";
			reg = <0x0 0x3210000 0x0 0x10000>;
			interrupts = <0 136 4>;
			clocks = <&clockgen 4 3>;
			status = "disabled";

	};

	sata2: sata@3220000 {
			compatible = "fsl,ls2080a-ahci";
			reg = <0x0 0x3220000 0x0 0x10000>;
			interrupts = <0 97 4>;
			clocks = <&clockgen 4 3>;
			status = "disabled";

	};

	sata3: sata@3230000 {
			compatible = "fsl,ls2080a-ahci";
			reg = <0x0 0x3230000 0x0 0x10000>;
			interrupts = <0 100 4>;
			clocks = <&clockgen 4 3>;
			status = "disabled";

	};

	pcie1: pcie@3400000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03400000 0x0 0x80000   /* PAB registers */
		       0x00 0x03480000 0x0 0x40000   /* LUT registers */
		       0x00 0x034c0000 0x0 0x40000   /* PF control registers */
		       0x80 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0x80 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0x80 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	pcie2: pcie@3500000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03500000 0x0 0x80000   /* PAB registers */
		       0x00 0x03580000 0x0 0x40000   /* LUT registers */
		       0x00 0x035c0000 0x0 0x40000   /* PF control registers */
		       0x88 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		num-lanes = <2>;
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0x88 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0x88 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	pcie3: pcie@3600000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03600000 0x0 0x80000   /* PAB registers */
		       0x00 0x03680000 0x0 0x40000   /* LUT registers */
		       0x00 0x036c0000 0x0 0x40000   /* PF control registers */
		       0x90 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0x90 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0x90 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	pcie4: pcie@3700000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03700000 0x0 0x80000   /* PAB registers */
		       0x00 0x03780000 0x0 0x40000   /* LUT registers */
		       0x00 0x037c0000 0x0 0x40000   /* PF control registers */
		       0x98 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0x98 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0x98 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	pcie5: pcie@3800000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03800000 0x0 0x80000   /* PAB registers */
		       0x00 0x03880000 0x0 0x40000   /* LUT registers */
		       0x00 0x038c0000 0x0 0x40000   /* PF control registers */
		       0xa0 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0xa0 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0xa0 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	pcie6: pcie@3900000 {
		compatible = "fsl,lx2160a-pcie";
		reg = <0x00 0x03900000 0x0 0x80000   /* PAB registers */
		       0x00 0x03980000 0x0 0x40000   /* LUT registers */
		       0x00 0x039c0000 0x0 0x40000   /* PF control registers */
		       0xa8 0x00000000 0x0 0x2000>; /* configuration space */
		reg-names = "ccsr", "lut", "pf_ctrl", "config";
		#address-cells = <3>;
		#size-cells = <2>;
		device_type = "pci";
		bus-range = <0x0 0xff>;
		ranges = <0x81000000 0x0 0x00000000 0xa8 0x00020000 0x0 0x00010000   /* downstream I/O */
			  0x82000000 0x0 0x40000000 0xa8 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
	};

	fsl_mc: fsl-mc@80c000000 {
		compatible = "fsl,qoriq-mc", "simple-mfd";
		reg = <0x00000008 0x0c000000 0 0x40>,
		      <0x00000000 0x08340000 0 0x40000>;
		#address-cells = <3>;
		#size-cells = <1>;

		/*
		 * Region type 0x0 - MC portals
		 * Region type 0x1 - QBMAN portals
		 */
		ranges = <0x0 0x0 0x0 0x8 0x0c000000 0x4000000
			  0x1 0x0 0x0 0x8 0x18000000 0x8000000>;

		dpmacs {
			compatible = "simple-mfd";
			#address-cells = <1>;
			#size-cells = <0>;

			dpmac1: dpmac@1 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x1>;
				status = "disabled";
			};

			dpmac2: dpmac@2 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x2>;
				status = "disabled";
			};

			dpmac3: dpmac@3 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x3>;
				status = "disabled";
			};

			dpmac4: dpmac@4 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x4>;
				status = "disabled";
			};

			dpmac5: dpmac@5 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x5>;
				status = "disabled";
			};

			dpmac6: dpmac@6 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x6>;
				status = "disabled";
			};

			dpmac7: dpmac@7 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x7>;
				status = "disabled";
			};

			dpmac8: dpmac@8 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x8>;
				status = "disabled";
			};

			dpmac9: dpmac@9 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x9>;
				status = "disabled";
			};

			dpmac10: dpmac@a {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xa>;
				status = "disabled";
			};

			dpmac11: dpmac@b {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xb>;
				status = "disabled";
			};

			dpmac12: dpmac@c {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xc>;
				status = "disabled";
			};

			dpmac13: dpmac@d {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xd>;
				status = "disabled";
			};

			dpmac14: dpmac@e {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xe>;
				status = "disabled";
			};

			dpmac15: dpmac@f {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0xf>;
				status = "disabled";
			};

			dpmac16: dpmac@10 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x10>;
				status = "disabled";
			};

			dpmac17: dpmac@11 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x11>;
				status = "disabled";
			};

			dpmac18: dpmac@12 {
				compatible = "fsl,qoriq-mc-dpmac";
				reg = <0x12>;
				status = "disabled";
			};
		};
	};

	/* LX2160ARM Chapter 28 ("Thermal Monitoring Unit") */
	tmu: tmu@1f80000 {
		compatible = "fsl,qoriq-tmu";
		reg = <0x0 0x1f80000 0x0 0x10000>;
		interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
		fsl,tmu-range = <0x800000e6 0x8001017d>;
		fsl,tmu-calibration = <0x00000000 0x00000035
				       0x00000001 0x00000154>;
		little-endian;
		#thermal-sensor-cells = <1>;
		label = "lx2160a-tmu"; /* explicit naming */
	};

	/* explicit thermal-zones names per LX2160ARM Table 323 */
	thermal-zones {
		cluster67-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 0>;
		};

		ddr1-cluster5-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 1>;
		};

		wriop-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 2>;
		};

		dce-qbman-hsio2-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 3>;
		};

		ccn-dpaa-tbu-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 4>;
		};

		cluster4-hsio3-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 5>;
		};

		cluster23-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 6>;
		};
	};

	/* WRIOP0: 0x8b8_0000, E-MDIO1: 0x1_6000 */
	emdio1: mdio@8b96000 {
		compatible = "fsl,ls-mdio";
		reg = <0x0 0x8b96000 0x0 0x1000>;
		interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	/* WRIOP0: 0x8b8_0000, E-MDIO2: 0x1_7000 */
	emdio2: mdio@8b97000 {
		compatible = "fsl,ls-mdio";
		reg = <0x0 0x8b97000 0x0 0x1000>;
		interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};
	firmware {
		optee {
			compatible = "linaro,optee-tz";
			method = "smc";
		};
	};
};
