// SPDX-License-Identifier: GPL-2.0+ OR X11
/*
 * Device tree fragment for RCW SCH-28021 card
 *
 * Copyright 2019-2021 NXP
 */

/*
 * SCH-28021 is a QSGMII add-on card used with various FSL QDS boards.
 * It integrates a VSC8514 quad PHY which supports 4 interfaces muxed on a
 * single QSGMII lane.
 * PHY addresses are 0x08 - 0x0b.
 * On the card the first port is the top port (farthest from PEX connector).
 */
phy@8 {
	reg = <0x08>;
};

phy@9 {
	reg = <0x09>;
};

phy@a {
	reg = <0x0a>;
};

phy@b {
	reg = <0x0b>;
};
