// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/input/input.h>
#include "tegra30.dtsi"

/ {
	model = "Microsoft Surface RT Tablet";
	compatible = "microsoft,surface-rt", "nvidia,tegra30";

	chosen {
		stdout-path = &uarta;
	};

	aliases {
		i2c0 = &pwr_i2c;

		mmc0 = &sdmmc4; /* eMMC */
		mmc1 = &sdmmc1; /* uSD slot */

		rtc0 = &pmic;
		rtc1 = "/rtc@7000e000";

		spi0 = &spi4;

		usb0 = &usb1;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x80000000>;
	};

	host1x@50000000 {
		dc@54200000 {
			rgb {
				status = "okay";

				nvidia,panel = <&panel>;
			};
		};
	};

	gpio@6000d000 {
		/* in case usb vbus is on for some reason */
		usb-vbus-hog {
			gpio-hog;
			gpios = <TEGRA_GPIO(DD, 6) GPIO_ACTIVE_HIGH>;
			output-low;
		};
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			/* SDMMC1 pinmux */
			sdmmc1-clk {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1-cmd {
				nvidia,pins = "sdmmc1_dat3_py4",
						"sdmmc1_dat2_py5",
						"sdmmc1_dat1_py6",
						"sdmmc1_dat0_py7",
						"sdmmc1_cmd_pz1";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* SDMMC3 pinmux */
			sdmmc3-clk {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3-cmd {
				nvidia,pins = "sdmmc3_cmd_pa7",
						"sdmmc3_dat3_pb4",
						"sdmmc3_dat2_pb5",
						"sdmmc3_dat1_pb6",
						"sdmmc3_dat0_pb7",
						"sdmmc3_dat5_pd0";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* SDMMC4 pinmux */
			sdmmc4-clk {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			sdmmc4-cmd {
				nvidia,pins = "sdmmc4_cmd_pt7",
						"sdmmc4_dat0_paa0",
						"sdmmc4_dat1_paa1",
						"sdmmc4_dat2_paa2",
						"sdmmc4_dat3_paa3",
						"sdmmc4_dat4_paa4",
						"sdmmc4_dat5_paa5",
						"sdmmc4_dat6_paa6",
						"sdmmc4_dat7_paa7",
						"sdmmc4_rst_n_pcc3";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			cam-mclk {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* I2C pinmux */
			gen1-i2c {
				nvidia,pins = "gen1_i2c_scl_pc4",
						"gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};
			gen2-i2c {
				nvidia,pins = "gen2_i2c_scl_pt5",
						"gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};
			cam-i2c {
				nvidia,pins = "cam_i2c_scl_pbb1",
						"cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};
			ddc-i2c {
				nvidia,pins = "ddc_scl_pv4",
						"ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};
			pwr-i2c {
				nvidia,pins = "pwr_i2c_scl_pz6",
						"pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			/* HDMI pinmux */
			hdmi-cec {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			hdmi-hpd {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,function = "hdmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* UART-A */
			ulpi-data0-po1 {
				nvidia,pins = "ulpi_data0_po1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi-data1-po2 {
				nvidia,pins = "ulpi_data1_po2";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi-data2-po3 {
				nvidia,pins = "ulpi_data2_po3",
						"ulpi_data3_po4";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* UART-B */
			uartb-txd-rxd {
				nvidia,pins = "uart2_txd_pc2",
						"uart2_rxd_pc3";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uartb-cts-rts {
				nvidia,pins = "uart2_cts_n_pj5",
						"uart2_rts_n_pj6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* UART-C */
			uartc-rxd-cts {
				nvidia,pins = "uart3_cts_n_pa1",
						"uart3_rxd_pw7";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uartc-txd-rts {
				nvidia,pins = "uart3_rts_n_pc0",
						"uart3_txd_pw6";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* I2S pinmux */
			dap-i2s0-out {
				nvidia,pins = "dap1_fs_pn0",
						"dap1_sclk_pn3";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap-i2s0-in {
				nvidia,pins = "dap1_din_pn1",
						"dap1_dout_pn2";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap-i2s1 {
				nvidia,pins = "dap2_fs_pa2",
						"dap2_sclk_pa3",
						"dap2_din_pa4",
						"dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap-i2s2 {
				nvidia,pins = "dap3_fs_pp0",
						"dap3_din_pp1",
						"dap3_dout_pp2",
						"dap3_sclk_pp3";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap-i2s3 {
				nvidia,pins = "dap4_fs_pp4",
						"dap4_din_pp5",
						"dap4_dout_pp6",
						"dap4_sclk_pp7";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb0 {
				nvidia,pins = "pbb0", "pbb7";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pcc1 {
				nvidia,pins = "pcc1";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pcc2 {
				nvidia,pins = "pcc2";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PCI-e pinmux */
			pex-l2-rst-n {
				nvidia,pins = "pex_l2_rst_n_pcc6",
						"pex_wake_n_pdd3",
						"pex_l1_rst_n_pdd5";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pex-l2-clkreq-n {
				nvidia,pins = "pex_l2_clkreq_n_pcc7",
						"pex_l0_prsnt_n_pdd0",
						"pex_l0_rst_n_pdd1",
						"pex_l0_clkreq_n_pdd2",
						"pex_l1_prsnt_n_pdd4",
						"pex_l1_clkreq_n_pdd6",
						"pex_l2_prsnt_n_pdd7";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* SPI pinmux */
			spi1-miso {
				nvidia,pins = "spi1_miso_px7";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi-clk {
				nvidia,pins = "ulpi_clk_py0",
						"ulpi_dir_py1",
						"ulpi_nxt_py2",
						"ulpi_stp_py3";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi-data7 {
				nvidia,pins = "ulpi_data7_po0",
						"ulpi_data4_po5",
						"ulpi_data5_po6",
						"ulpi_data6_po7",
						"spi1_mosi_px4",
						"spi1_sck_px5",
						"spi1_cs0_n_px6";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			spi2-cs1-n {
				nvidia,pins = "spi2_cs1_n_pw2";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			spi2-cs2-n {
				nvidia,pins = "spi2_cs2_n_pw3";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-a17 {
				nvidia,pins = "gmi_a17_pb0",
						"gmi_a18_pb1",
						"gmi_a16_pj7",
						"gmi_a19_pk7";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			spi2-sck {
				nvidia,pins = "spi2_sck_px2";
				nvidia,function = "spi6";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Display A pinmux */
			lcd-pclk {
				nvidia,pins = "lcd_pclk_pb3",
						"lcd_dc1_pd2",
						"lcd_d0_pe0",
						"lcd_d1_pe1",
						"lcd_d2_pe2",
						"lcd_d3_pe3",
						"lcd_d4_pe4",
						"lcd_d5_pe5",
						"lcd_d6_pe6",
						"lcd_d7_pe7",
						"lcd_d8_pf0",
						"lcd_d9_pf1",
						"lcd_d10_pf2",
						"lcd_d11_pf3",
						"lcd_d12_pf4",
						"lcd_d13_pf5",
						"lcd_d14_pf6",
						"lcd_d15_pf7",
						"lcd_de_pj1",
						"lcd_d16_pm0",
						"lcd_d17_pm1",
						"lcd_d18_pm2",
						"lcd_d19_pm3",
						"lcd_d20_pm4",
						"lcd_d21_pm5",
						"lcd_d22_pm6",
						"lcd_d23_pm7",
						"lcd_sdout_pn5",
						"lcd_dc0_pn6",
						"lcd_m1_pw1",
						"lcd_sdin_pz2",
						"lcd_sck_pz4";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd-pwr1 {
				nvidia,pins = "lcd_pwr1_pc1",
						"lcd_pwr2_pc6";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd-hsync {
				nvidia,pins = "lcd_hsync_pj3",
						"lcd_vsync_pj4",
						"lcd_cs0_n_pn4",
						"lcd_cs1_n_pw0",
						"lcd_wr_n_pz3";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd-pwr0 {
				nvidia,pins = "lcd_pwr0_pb2";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			crt-hsync-pv6 {
				nvidia,pins = "crt_hsync_pv6",
						"crt_vsync_pv7";
				nvidia,function = "crt";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			blink {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,function = "blink";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* KBC keys */
			kb-col0 {
				nvidia,pins = "kb_col0_pq0",
						"kb_col1_pq1",
						"kb_col2_pq2",
						"kb_col3_pq3",
						"kb_col4_pq4",
						"kb_col5_pq5",
						"kb_col6_pq6",
						"kb_col7_pq7",
						"kb_row12_ps4";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb-row0 {
				nvidia,pins = "kb_row0_pr0",
						"kb_row1_pr1",
						"kb_row5_pr5";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb-row2 {
				nvidia,pins = "kb_row2_pr2",
						"kb_row3_pr3",
						"kb_row6_pr6",
						"kb_row7_pr7",
						"kb_row11_ps3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb-row4 {
				nvidia,pins = "kb_row4_pr4",
						"kb_row9_ps1";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb-row8 {
				nvidia,pins = "kb_row8_ps0",
						"kb_row10_ps2";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb-row13 {
				nvidia,pins = "kb_row13_ps5",
						"kb_row14_ps6",
						"kb_row15_ps7";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* SPDIF pinmux */
			spdif-pins {
				nvidia,pins = "spdif_out_pk5",
						"spdif_in_pk6";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3-dat6 {
				nvidia,pins = "sdmmc3_dat6_pd3",
						"sdmmc3_dat7_pd4";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			jtag-rtck {
				nvidia,pins = "jtag_rtck_pu7";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GMI pinmux */
			gmi-wp-n {
				nvidia,pins = "gmi_wp_n_pc7",
						"gmi_cs7_n_pi6";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3-dat4 {
				nvidia,pins = "sdmmc3_dat4_pd1",
						"gmi_ad9_ph1";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi-ad0-pg0 {
				nvidia,pins = "gmi_ad0_pg0",
						"gmi_ad1_pg1",
						"gmi_ad2_pg2",
						"gmi_ad3_pg3",
						"gmi_ad4_pg4",
						"gmi_ad5_pg5",
						"gmi_ad6_pg6",
						"gmi_ad7_pg7",
						"gmi_ad15_ph7";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-ad8 {
				nvidia,pins = "gmi_ad8_ph0";
				nvidia,function = "pwm0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi-ad10 {
				nvidia,pins = "gmi_ad10_ph2",
						"gmi_ad11_ph3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-ad12 {
				nvidia,pins = "gmi_ad12_ph4",
						"gmi_ad13_ph5",
						"gmi_iordy_pi5",
						"gmi_cs0_n_pj0",
						"pu1",
						"pu2",
						"pv1",
						"pv2",
						"pv3";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-wr-n {
				nvidia,pins = "gmi_wr_n_pi0",
						"gmi_oe_n_pi1",
						"gmi_adv_n_pk0",
						"gmi_clk_pk1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-dqs {
				nvidia,pins = "gmi_dqs_pi2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-wait {
				nvidia,pins = "gmi_wait_pi7",
						"gmi_cs2_n_pk3",
						"gmi_cs3_n_pk4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-cs4-n {
				nvidia,pins = "gmi_cs4_n_pk2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi-ad14-ph6 {
				nvidia,pins = "gmi_ad14_ph6";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* VI pinmux */
			vi-d1-pd5 {
				nvidia,pins = "vi_d1_pd5",
						"vi_vsync_pd6",
						"vi_d2_pl0",
						"vi_d4_pl2",
						"vi_d5_pl3",
						"vi_d6_pl4",
						"vi_pclk_pt0",
						"vi_d10_pt2",
						"vi_d0_pt4";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			vi-d3-pl1 {
				nvidia,pins = "vi_d3_pl1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			vi-hsync-pd7 {
				nvidia,pins = "vi_hsync_pd7",
						"vi_d7_pl5",
						"vi_d8_pl6",
						"vi_d9_pl7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			vi-mclk-pt1 {
				nvidia,pins = "vi_mclk_pt1";
				nvidia,function = "vi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};
			vi-d11-pt3 {
				nvidia,pins = "vi_d11_pt3";
				nvidia,function = "ddr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
				nvidia,io-reset = <TEGRA_PIN_DISABLE>;
			};

			/* PORT U */
			pu0 {
				nvidia,pins = "pu0";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu3 {
				nvidia,pins = "pu3";
				nvidia,function = "pwm0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu4 {
				nvidia,pins = "pu4";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu5 {
				nvidia,pins = "pu5";
				nvidia,function = "pwm2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu6 {
				nvidia,pins = "pu6";
				nvidia,function = "pwm3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PORT V */
			pv0 {
				nvidia,pins = "pv0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PORT BB */
			pbb3 {
				nvidia,pins = "pbb3";
				nvidia,function = "vgp3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb4 {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pbb5 {
				nvidia,pins = "pbb5";
				nvidia,function = "vgp5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb6 {
				nvidia,pins = "pbb6";
				nvidia,function = "vgp6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* CLK pinmux */
			clk1-out-pw4 {
				nvidia,pins = "clk1_out_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2-out-pw5 {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "extperiph2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2-req-pcc5 {
				nvidia,pins = "clk2_req_pcc5",
						"clk1_req_pee2";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk3-out-pee0 {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk3-req-pee1 {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "dev3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sys-clk-req-pz5 {
				nvidia,pins = "sys_clk_req_pz5";
				nvidia,function = "sysclk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			owr {
				nvidia,pins = "owr";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GPIO power/drive control */
			drive-sdio1 {
				nvidia,pins = "drive_sdio1",
						"drive_sdio3";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <46>;
				nvidia,pull-up-strength = <42>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FAST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FAST>;
			};
		};
	};

	uarta: serial@70006000 {
		status = "okay";
	};

	pwm: pwm@7000a000 {
		status = "okay";
	};

	pwr_i2c: i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		/* Texas Instruments TPS659110 PMIC */
		pmic: tps65911@2d {
			compatible = "ti,tps65911";
			reg = <0x2d>;

			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			#interrupt-cells = <2>;
			interrupt-controller;

			ti,system-power-controller;

			#gpio-cells = <2>;
			gpio-controller;

			regulators {
				vdd_1v8_vio: vddio {
					regulator-name = "vdd_1v8_gen";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vddio_usd: ldo5 {
					regulator-name = "vddio_usd";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
					regulator-boot-on;
				};
			};
		};
	};

	spi4: spi@7000da00 {
		status = "okay";
		spi-max-frequency = <25000000>;

		spi-flash@1 {
			compatible = "winbond,w25q32", "jedec,spi-nor";
			reg = <1>;
			spi-max-frequency = <20000000>;
		};
	};

	sdmmc1: mmc@78000000 {
		status = "okay";
		bus-width = <4>;

		cd-gpios = <&gpio TEGRA_GPIO(I, 5) GPIO_ACTIVE_LOW>;

		vmmc-supply = <&vdd_usd>;
		vqmmc-supply = <&vddio_usd>;
	};

	sdmmc4: mmc@78000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;

		vmmc-supply = <&vdd_3v3_sys>;
		vqmmc-supply = <&vdd_1v8_vio>;
	};

	/* Main USB port */
	usb1: usb@7d000000 {
		status = "okay";
		dr_mode = "otg";
		nvidia,vbus-gpio = <&gpio TEGRA_GPIO(DD, 6) GPIO_ACTIVE_HIGH>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";

		enable-gpios = <&gpio TEGRA_GPIO(DD, 0) GPIO_ACTIVE_HIGH>;
		pwms = <&pwm 0 50000>;

		brightness-levels = <1 35 70 105 140 175 210 255>;
		default-brightness-level = <5>;
	};

	/* PMIC has a built-in 32KHz oscillator which is used by PMC */
	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "pmic-oscillator";
	};

	extcon-keys {
		compatible = "gpio-keys";

		switch-hall-sensor {
			label = "Hall Sensor";
			gpios = <&gpio TEGRA_GPIO(L, 1) GPIO_ACTIVE_HIGH>;
			linux,code = <SW_LID>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(V, 0) GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_CANCEL>;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio TEGRA_GPIO(S, 6) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_DOWN>;
		};

		key-volume-up {
			label = "Volume Up";
			gpios = <&gpio TEGRA_GPIO(S, 7) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_UP>;
		};

		key-windows-button {
			label = "Windows Button";
			gpios = <&gpio TEGRA_GPIO(S, 5) GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_ENTER>;
		};
	};

	panel: panel {
		compatible = "simple-panel";

		power-supply = <&vdd_pnl_reg>;
		enable-gpios = <&gpio TEGRA_GPIO(B, 2) GPIO_ACTIVE_HIGH>;

		backlight = <&backlight>;

		display-timings {
			timing@0 {
				/* 1366x768@60Hz */
				clock-frequency = <71980000>;

				hactive = <1366>;
				hfront-porch = <56>;
				hback-porch = <106>;
				hsync-len = <14>;

				vactive = <768>;
				vfront-porch = <3>;
				vback-porch = <6>;
				vsync-len = <1>;
			};
		};
	};

	vdd_3v3_sys: regulator-3v {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v3_sys";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_usd: regulator-usd {
		compatible = "regulator-fixed";
		regulator-name = "vdd_usd";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio TEGRA_GPIO(D, 7) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vdd_pnl_reg: regulator-pnl {
		compatible = "regulator-fixed";
		regulator-name = "vdd_panel";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio TEGRA_GPIO(DD, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};
