// SPDX-License-Identifier: GPL-2.0+
/*
 * Devicetree file for running sandbox tests
 *
 * This includes lots of extra devices used by various tests.
 *
 * Note that SPL use the main sandbox.dts file
 */

/dts-v1/;

#include <config.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/gpio/sandbox-gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/pinctrl/sandbox-pinmux.h>
#include <dt-bindings/mux/mux.h>
#include <dt-bindings/phy/phy.h>

/ {
	model = "sandbox";
	compatible = "sandbox";
	#address-cells = <1>;
	#size-cells = <1>;

	aliases {
		console = &uart0;
		ethernet0 = "/eth@10002000";
		ethernet2 = &swp_0;
		ethernet3 = &eth_3;
		ethernet4 = &dsa_eth0;
		ethernet5 = &eth_5;
		ethernet6 = "/eth@10004000";
		ethernet7 = &swp_1;
		ethernet8 = &phy_eth0;
		gpio1 = &gpio_a;
		gpio2 = &gpio_b;
		gpio3 = &gpio_c;
		i2c0 = "/i2c@0";
		mmc0 = "/mmc0";
		mmc1 = "/mmc1";
		mmc2 = "/mmc2";
		mmc3 = "/mmc3";
		mmc4 = "/mmc4";
		mmc5 = "/mmc5";
		mmc6 = "/mmc6";
		mmc7 = "/mmc7";
		mmc8 = "/mmc8";
		mmc9 = "/mmc9";
		mmc10 = "/mmc10";
		pci0 = &pci0;
		pci1 = &pci1;
		pci2 = &pci2;
		remoteproc0 = &rproc_1;
		remoteproc1 = &rproc_2;
		rtc0 = &rtc_0;
		rtc1 = &rtc_1;
		spi0 = "/spi@0";
		testfdt6 = "/e-test";
		testbus3 = "/some-bus";
		testfdt0 = "/some-bus/c-test@0";
		testfdt12 = "/some-bus/c-test@1";
		testfdt3 = "/b-test";
		testfdt5 = "/some-bus/c-test@5";
		testfdt8 = "/a-test";
		testfdtm1 = &testfdtm1;
		fdt-dummy0 = "/translation-test@8000/dev@0,0";
		fdt-dummy1 = "/translation-test@8000/dev@1,100";
		fdt-dummy2 = "/translation-test@8000/dev@2,200";
		fdt-dummy3 = "/translation-test@8000/noxlatebus@3,300/dev@42";
		usb0 = &usb_0;
		usb1 = &usb_1;
		usb2 = &usb_2;
		axi0 = &axi;
		osd0 = "/osd";
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		event_log: tcg_event_log {
			no-map;
			reg = <(CFG_SYS_SDRAM_BASE + 0x100000) 0x2000>;
		};
	};

	binman: binman {
	};

	config {
		testing-bool;
		testing-int = <123>;
		testing-str = "testing";
		environment {
			from_fdt = "yes";
			fdt_env_path = "";
		};
	};

	options {
		u-boot {
			compatible = "u-boot,config";
			bootscr-ram-offset = /bits/ 64 <0x12345678>;
			bootscr-flash-offset = /bits/ 64 <0>;
			bootscr-flash-size = /bits/ 64 <0x2000>;
			boot-led = <&sandbox_led_green>;
			activity-led = <&sandbox_led_red>;
			testing-bool;
			testing-int = <123>;
			testing-str = "testing";
			testing-phandle = <&phandle_node_1>;
		};
	};

	bootstd {
		bootph-verify;
		compatible = "u-boot,boot-std";

		filename-prefixes = "/", "/boot/";
		bootdev-order = "mmc2", "mmc1";

		extlinux {
			compatible = "u-boot,extlinux";
		};

		efi {
			compatible = "u-boot,distro-efi";
		};

		theme {
			font-size = <30>;
			menu-inset = <3>;
			menuitem-gap-y = <1>;
			white-on-black;
		};

		cedit-theme {
			font-size = <30>;
			menu-inset = <3>;
			menuitem-gap-y = <1>;
		};

		/*
		 * This is used for the VBE OS-request tests. A FAT filesystem
		 * created in a partition with the VBE information appearing
		 * before the partition starts
		 */
		firmware0 {
			bootph-verify;
			compatible = "fwupd,vbe-simple";
			storage = "mmc1";
			skip-offset = <0x200>;
			area-start = <0x400>;
			area-size = <0x1000>;
			state-offset = <0x400>;
			state-size = <0x40>;
			version-offset = <0x800>;
			version-size = <0x100>;
		};

		/*
		 * This is used for the VBE VPL tests. The MMC device holds the
		 * binman image.bin file. The test progresses through each phase
		 * of U-Boot, loading each in turn from MMC.
		 *
		 * Note that the test enables this node (and mmc3) before
		 * running U-Boot
		 */
		firmware1 {
			bootph-verify;
			status = "disabled";
			compatible = "fwupd,vbe-simple";
			storage = "mmc3";
			skip-offset = <0x800000>;
			area-start = <0>;
			area-size = <0x2000000>;
			state-offset = <0xdffc00>;
			state-size = <0x40>;
			version-offset = <0xdffe00>;
			version-size = <0x100>;
		};
	};

	cedit: cedit {
	};

	fuzzing-engine {
		compatible = "sandbox,fuzzing-engine";
	};

	reboot-mode0 {
		compatible = "reboot-mode-gpio";
		gpios = <&gpio_c 0 GPIO_ACTIVE_HIGH>, <&gpio_c 1 GPIO_ACTIVE_HIGH>;
		u-boot,env-variable = "bootstatus";
		mode-test = <0x01>;
		mode-download = <0x03>;
	};

	reboot_mode1: reboot-mode@14 {
		compatible = "reboot-mode-rtc";
		rtc = <&rtc_0>;
		reg = <0x30 4>;
		u-boot,env-variable = "bootstatus";
		big-endian;
		mode-test = <0x21969147>;
		mode-download = <0x51939147>;
	};

	audio: audio-codec {
		compatible = "sandbox,audio-codec";
		#sound-dai-cells = <1>;
	};

	buttons {
		compatible = "gpio-keys";

		btn1 {
			gpios = <&gpio_a 3 0>;
			label = "button1";
			linux,code = <BTN_1>;
		};

		btn2 {
			gpios = <&gpio_a 4 0>;
			label = "button2";
			linux,code = <BTN_2>;
		};
	};

	buttons2 {
		compatible = "adc-keys";
		io-channels = <&adc 3>;
		keyup-threshold-microvolt = <3000000>;

		button-up {
			label = "button3";
			linux,code = <KEY_F3>;
			press-threshold-microvolt = <1500000>;
		};

		button-down {
			label = "button4";
			linux,code = <KEY_F4>;
			press-threshold-microvolt = <1000000>;
		};

		button-enter {
			label = "button5";
			linux,code = <KEY_F5>;
			press-threshold-microvolt = <500000>;
		};
	};

	cros_ec: cros-ec {
		reg = <0 0>;
		compatible = "google,cros-ec-sandbox";

		/*
		 * This describes the flash memory within the EC. Note
		 * that the STM32L flash erases to 0, not 0xff.
		 */
		flash {
			image-pos = <0x08000000>;
			size = <0x20000>;
			erase-value = <0>;

			/* Information for sandbox */
			ro {
				image-pos = <0>;
				size = <0xf000>;
			};
			wp-ro {
				image-pos = <0xf000>;
				size = <0x1000>;
				used = <0x884>;
				compress = "lz4";
				uncomp-size = <0xcf8>;
				hash {
					algo = "sha256";
					value = [00 01 02 03 04 05 06 07
						08 09 0a 0b 0c 0d 0e 0f
						10 11 12 13 14 15 16 17
						18 19 1a 1b 1c 1d 1e 1f];
				};
			};
			rw {
				image-pos = <0x10000>;
				size = <0x10000>;
			};
		};

		cros_ec_pwm: cros-ec-pwm {
			compatible = "google,cros-ec-pwm";
			#pwm-cells = <1>;
		};

	};

	dsi_host: dsi_host {
		compatible = "sandbox,dsi-host";
	};

	phandle_node_1: phandle-node-1 {
	};

	phandle_node_2: phandle-node-2 {
	};

	a-test {
		reg = <0 1>;
		compatible = "denx,u-boot-fdt-test";
		ping-expect = <0>;
		ping-add = <0>;
		bootph-all;
		test-gpios = <&gpio_a 1>, <&gpio_a 4>,
			<&gpio_b 5 GPIO_ACTIVE_HIGH 3 2 1>,
			<0>, <&gpio_a 12>;
		test2-gpios = <&gpio_a 1>, <&gpio_a 4>,
			<&gpio_b 6 GPIO_ACTIVE_LOW 3 2 1>,
			<&gpio_b 7 GPIO_IN 3 2 1>,
			<&gpio_b 8 GPIO_OUT 3 2 1>,
			<&gpio_b 9 (GPIO_OUT|GPIO_OUT_ACTIVE) 3 2 1>;
		test3-gpios =
			<&gpio_c 0 (GPIO_OUT|GPIO_OPEN_DRAIN)>,
			<&gpio_c 1 (GPIO_OUT|GPIO_OPEN_SOURCE)>,
			<&gpio_c 2 GPIO_OUT>,
			<&gpio_c 3 (GPIO_IN|GPIO_PULL_UP)>,
			<&gpio_c 4 (GPIO_IN|GPIO_PULL_DOWN)>,
			<&gpio_c 5 GPIO_IN>,
			<&gpio_c 6 (GPIO_ACTIVE_LOW|GPIO_OUT|GPIO_OPEN_DRAIN)>,
			<&gpio_c 7 (GPIO_ACTIVE_LOW|GPIO_OUT|GPIO_OPEN_SOURCE)>;
		test4-gpios = <&gpio_a 14>, <&gpio_b 4 1 3 2 1>;
		test5-gpios = <&gpio_a 19>;

		bool-value;
		int8-value = /bits/ 8 <0x12>;
		int16-value = /bits/ 16 <0x1234>;
		int-value = <1234>;
		uint-value = <(-1234)>;
		int64-value = /bits/ 64 <0x1111222233334444>;
		int-array = <5678 9123 4567>;
		int64-array = /bits/ 64 <0x1111222233334444 0x4444333322221111>;
		str-value = "test string";
		interrupts-extended = <&irq 3 0>;
		acpi,name = "GHIJ";
		phandle-value = <&gpio_c 10>, <0xFFFFFFFF 20>, <&gpio_a 30>;
		phandle-nodes = <&phandle_node_1>, <&phandle_node_2>;

		mux-controls = <&muxcontroller0 0>, <&muxcontroller0 1>,
			       <&muxcontroller0 2>, <&muxcontroller0 3>,
			       <&muxcontroller1>;
		mux-control-names = "mux0", "mux1", "mux2", "mux3", "mux4";
		mux-syscon = <&syscon3>;
		display-timings {
			timing0: 240x320 {
				clock-frequency = <6500000>;
				hactive = <240>;
				vactive = <320>;
				hfront-porch = <6>;
				hback-porch = <7>;
				hsync-len = <1>;
				vback-porch = <5>;
				vfront-porch = <8>;
				vsync-len = <2>;
				hsync-active = <1>;
				vsync-active = <0>;
				de-active = <1>;
				pixelclk-active = <1>;
				interlaced;
				doublescan;
				doubleclk;
			};
			timing1: 480x800 {
				clock-frequency = <9000000>;
				hactive = <480>;
				vactive = <800>;
				hfront-porch = <10>;
				hback-porch = <59>;
				hsync-len = <12>;
				vback-porch = <15>;
				vfront-porch = <17>;
				vsync-len = <16>;
				hsync-active = <0>;
				vsync-active = <1>;
				de-active = <0>;
				pixelclk-active = <0>;
			};
			timing2: 800x480 {
				clock-frequency = <33500000>;
				hactive = <800>;
				vactive = <480>;
				hback-porch = <89>;
				hfront-porch = <164>;
				vback-porch = <23>;
				vfront-porch = <10>;
				hsync-len = <11>;
				vsync-len = <13>;
			};
		};
		panel-timing {
			clock-frequency = <6500000>;
			hactive = <240>;
			vactive = <320>;
			hfront-porch = <6>;
			hback-porch = <7>;
			hsync-len = <1>;
			vback-porch = <5>;
			vfront-porch = <8>;
			vsync-len = <2>;
			hsync-active = <1>;
			vsync-active = <0>;
			de-active = <1>;
			pixelclk-active = <1>;
			interlaced;
			doublescan;
			doubleclk;
		};
	};

	junk {
		reg = <1 1>;
		compatible = "not,compatible";
	};

	no-compatible {
		reg = <2 1>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		enable-gpios = <&gpio_a 1>;
		power-supply = <&ldo_1>;
		pwms = <&pwm 0 1000>;
		default-brightness-level = <5>;
		brightness-levels = <0 16 32 64 128 170 202 234 255>;
	};

	bind-test {
		compatible = "simple-bus";
		bind-test-child1 {
			compatible = "sandbox,phy";
			#phy-cells = <1>;
		};

		bind-test-child2 {
			compatible = "simple-bus";
		};
	};

	b-test {
		reg = <3 1>;
		compatible = "denx,u-boot-fdt-test";
		ping-expect = <3>;
		ping-add = <3>;

		mux-controls = <&muxcontroller0 0>;
		mux-control-names = "mux0";
	};

	multimatch-test {
		compatible = "sandbox,multimatch-test";
	};

	phy_provider0: gen_phy@0 {
		compatible = "sandbox,phy";
		#phy-cells = <1>;
	};

	phy_provider1: gen_phy@1 {
		compatible = "sandbox,phy";
		#phy-cells = <0>;
		broken;
	};

	phy_provider2: gen_phy@2 {
		compatible = "sandbox,phy";
		#phy-cells = <0>;
	};

	phy_provider3: gen_phy@3 {
		compatible = "sandbox,phy";
		#phy-cells = <2>;
	};

	gen_phy_user: gen_phy_user {
		compatible = "simple-bus";
		phys = <&phy_provider0 0>, <&phy_provider0 1>, <&phy_provider1>;
		phy-names = "phy1", "phy2", "phy3";
	};

	gen_phy_user1: gen_phy_user1 {
		compatible = "simple-bus";
		phys = <&phy_provider0 0>, <&phy_provider2>;
		phy-names = "phy1", "phy2";
	};

	gen_phy_user2: gen_phy_user2 {
		compatible = "simple-bus";
		phys = <&phy_provider3 0 0>;
		phy-names = "phy1";
	};

	/* PHY common props test nodes */
	phy_common_props_missing: phy-common-props-missing {
		/* empty: no rx-polarity or tx-polarity properties */
	};

	phy_common_props_more_values: phy-common-props-more-values {
		/* 3 values but only 2 names => count mismatch */
		rx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT PHY_POL_NORMAL>;
		rx-polarity-names = "sgmii", "2500base-x";
		tx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT PHY_POL_NORMAL>;
		tx-polarity-names = "sgmii", "2500base-x";
	};

	phy_common_props_single: phy-common-props-single {
		/* 1 value, no names array => value applies to all modes */
		rx-polarity = <PHY_POL_INVERT>;
		tx-polarity = <PHY_POL_INVERT>;
	};

	phy_common_props_more_names: phy-common-props-more-names {
		/* 2 values but 3 names => count mismatch */
		rx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		rx-polarity-names = "sgmii", "2500base-x", "1000base-x";
		tx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		tx-polarity-names = "sgmii", "2500base-x", "1000base-x";
	};

	phy_common_props_find_by_name: phy-common-props-find-by-name {
		/* valid 3-element arrays, lookup by mode name */
		rx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT PHY_POL_AUTO>;
		rx-polarity-names = "sgmii", "2500base-x", "usb-ss";
		tx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT PHY_POL_NORMAL>;
		tx-polarity-names = "sgmii", "2500base-x", "1000base-x";
	};

	phy_common_props_no_default: phy-common-props-no-default {
		/* name not in array, no "default" entry => -EINVAL */
		rx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		rx-polarity-names = "2500base-x", "1000base-x";
		tx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		tx-polarity-names = "2500base-x", "1000base-x";
	};

	phy_common_props_with_default: phy-common-props-with-default {
		/* name not in array, but "default" entry exists */
		rx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		rx-polarity-names = "2500base-x", "default";
		tx-polarity = <PHY_POL_NORMAL PHY_POL_INVERT>;
		tx-polarity-names = "2500base-x", "default";
	};

	phy_common_props_unsupported: phy-common-props-unsupported {
		/* PHY_POL_AUTO is not supported for manual-only modes */
		rx-polarity = <PHY_POL_AUTO>;
		rx-polarity-names = "sgmii";
		tx-polarity = <PHY_POL_AUTO>;
		tx-polarity-names = "sgmii";
	};

	some-bus {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "denx,u-boot-test-bus";
		reg = <3 1>;
		ping-expect = <4>;
		ping-add = <4>;
		c-test@5 {
			compatible = "denx,u-boot-fdt-test";
			reg = <5>;
			ping-expect = <5>;
			ping-add = <5>;
		};
		c-test@0 {
			compatible = "denx,u-boot-fdt-test";
			reg = <0>;
			ping-expect = <6>;
			ping-add = <6>;
		};
		c-test@1 {
			compatible = "denx,u-boot-fdt-test";
			reg = <1>;
			ping-expect = <7>;
			ping-add = <7>;
		};
	};

	d-test {
		reg = <3 1>;
		ping-expect = <6>;
		ping-add = <6>;
		compatible = "google,another-fdt-test";
	};

	e-test {
		reg = <3 1>;
		ping-expect = <6>;
		ping-add = <6>;
		compatible = "google,another-fdt-test";
	};

	f-test {
		#interrupt-cells = <2>;
		interrupt-parent = <&irq>;
		interrupts = <4 0>;
		compatible = "denx,u-boot-fdt-test";
	};

	g-test {
		compatible = "denx,u-boot-fdt-test";
	};

	h-test {
		compatible = "denx,u-boot-fdt-test1";
	};

	i-test {
		compatible = "mediatek,u-boot-fdt-test";
		#address-cells = <1>;
		#size-cells = <0>;

		subnode@0 {
			reg = <0>;
		};

		subnode@1 {
			reg = <1>;
		};

		subnode@2 {
			reg = <2>;
		};
	};

	devres-test {
		compatible = "denx,u-boot-devres-test";
	};

	another-test {
		reg = <0 2>;
		compatible = "denx,u-boot-fdt-test";
		test4-gpios = <&gpio_a 14>, <&gpio_b 4 1 3 2 1>;
		test5-gpios = <&gpio_a 19>;
	};

	mmio-bus@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "denx,u-boot-test-bus";
		dma-ranges = <0x10000000 0x00000000 0x00040000>;

		subnode@0 {
			compatible = "denx,u-boot-fdt-test";
		};
	};

	mmio-bus@1 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "denx,u-boot-test-bus";

		subnode@0 {
			compatible = "denx,u-boot-fdt-test";
		};
	};

	acpi_test1: acpi-test {
		compatible = "denx,u-boot-acpi-test";
		acpi-ssdt-test-data = "ab";
		acpi-dsdt-test-data = "hi";
		child {
			compatible = "denx,u-boot-acpi-test";
		};
	};

	acpi_test2: acpi-test2 {
		compatible = "denx,u-boot-acpi-test";
		acpi-ssdt-test-data = "cd";
		acpi-dsdt-test-data = "jk";
	};

	clocks {
		clk_fixed: clk-fixed {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <1234>;
		};

		clk_fixed_factor: clk-fixed-factor {
			compatible = "fixed-factor-clock";
			#clock-cells = <0>;
			clock-div = <3>;
			clock-mult = <2>;
			clocks = <&clk_fixed>;
		};

		osc {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <20000000>;
		};
	};

	clk_sandbox: clk-sbox {
		compatible = "sandbox,clk";
		#clock-cells = <1>;
		assigned-clocks = <&clk_sandbox 3>;
		assigned-clock-rates = <321>;
	};

	clk-test {
		compatible = "sandbox,clk-test";
		clocks = <&clk_fixed>,
			 <&clk_sandbox 1>,
			 <&clk_sandbox 0>,
			 <&ccf 11>,
			 <&clk_sandbox 3>,
			 <&clk_sandbox 2>;
		clock-names = "fixed", "i2c", "spi", "i2c_root", "uart2", "uart1";
	};

	clk-test2 {
		compatible = "sandbox,clk-test";
		assigned-clock-rates = <321>;
	};

	clk-test3 {
		compatible = "sandbox,clk-test";
		assigned-clocks = <&clk_sandbox 1>;
	};

	clk-test4 {
		compatible = "sandbox,clk-test";
		assigned-clock-rates = <654>, <321>;
		assigned-clocks = <&clk_sandbox 1>;
	};

	ccf: clk-ccf {
		compatible = "sandbox,clk-ccf";
		#clock-cells = <1>;
	};

	efi-media {
		compatible = "sandbox,efi-media";
	};

	eth@10002000 {
		compatible = "sandbox,eth";
		reg = <0x10002000 0x1000>;
	};

	eth_5: eth@10003000 {
		compatible = "sandbox,eth";
		reg = <0x10003000 0x1000>;
		nvmem-cells = <&eth5_addr>;
		nvmem-cell-names = "mac-address";
	};

	eth_3: sbe5 {
		compatible = "sandbox,eth";
		reg = <0x10005000 0x1000>;
		nvmem-cells = <&eth3_addr>;
		nvmem-cell-names = "mac-address";
	};

	eth@10004000 {
		compatible = "sandbox,eth";
		reg = <0x10004000 0x1000>;
	};

	phy_eth0: phy-test-eth {
		compatible = "sandbox,eth";
		reg = <0x10007000 0x1000>;
		mac-address = [ 02 00 11 22 33 49 ];
		phy-handle = <&ethphy1>;
		phy-mode = "2500base-x";
	};

	dsa_eth0: dsa-test-eth {
		compatible = "sandbox,eth";
		reg = <0x10006000 0x1000>;
		nvmem-cells = <&eth4_addr>;
		nvmem-cell-names = "mac-address";
	};

	dsa-test {
		compatible = "sandbox,dsa";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;
			swp_0: port@0 {
				reg = <0>;
				label = "lan0";
				phy-mode = "rgmii-rxid";

				fixed-link {
					speed = <100>;
					full-duplex;
				};
			};

			swp_1: port@1 {
				reg = <1>;
				label = "lan1";
				phy-mode = "rgmii-txid";
				fixed-link = <0 1 100 0 0>;
			};

			port@2 {
				reg = <2>;
				ethernet = <&dsa_eth0>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};
	};

	firmware {
		sandbox_firmware: sandbox-firmware {
			compatible = "sandbox,firmware";
		};

		scmi {
			compatible = "sandbox,scmi-agent";
			#address-cells = <1>;
			#size-cells = <0>;

			pwrdom_scmi: protocol@11 {
				reg = <0x11>;
				#power-domain-cells = <1>;
			};

			clk_scmi: protocol@14 {
				reg = <0x14>;
				#clock-cells = <1>;
				linaro,sandbox-channel-id = <0x14>;
			};

			reset_scmi: protocol@16 {
				reg = <0x16>;
				#reset-cells = <1>;
			};

			protocol@17 {
				reg = <0x17>;

				regulators {
					#address-cells = <1>;
					#size-cells = <0>;

					regul0_scmi: reg@0 {
						reg = <0>;
						regulator-name = "sandbox-voltd0";
						regulator-min-microvolt = <1100000>;
						regulator-max-microvolt = <3300000>;
					};
					regul1_scmi: reg@1 {
						reg = <0x1>;
						regulator-name = "sandbox-voltd1";
						regulator-min-microvolt = <1800000>;
					};
				};
			};
		};

		sm: secure-monitor {
			compatible = "sandbox,sm";
		};
	};

	fpga {
		compatible = "sandbox,fpga";
	};

	pinctrl-gpio {
		compatible = "sandbox,pinctrl-gpio";

		gpio_a: base-gpios {
			compatible = "sandbox,gpio";
			gpio-controller;
			#gpio-cells = <1>;
			gpio-bank-name = "a";
			sandbox,gpio-count = <25>;
			gpio-line-names = "", "eth1-reset", "rtc-irq";
			hog_input_active_low {
				gpio-hog;
				input;
				gpios = <10 GPIO_ACTIVE_LOW>;
			};
			hog_input_active_high {
				gpio-hog;
				input;
				gpios = <11 GPIO_ACTIVE_HIGH>;
			};
			hog_output_low {
				gpio-hog;
				output-low;
				gpios = <12 GPIO_ACTIVE_HIGH>;
			};
			hog_output_high {
				gpio-hog;
				output-high;
				gpios = <13 GPIO_ACTIVE_HIGH>;
			};
		};

		gpio_b: extra-gpios {
			compatible = "sandbox,gpio";
			gpio-controller;
			#gpio-cells = <5>;
			gpio-bank-name = "b";
			sandbox,gpio-count = <10>;
			gpio-line-names = "factory-reset";
		};

		gpio_c: pinmux-gpios {
			compatible = "sandbox,gpio";
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank-name = "c";
			sandbox,gpio-count = <10>;
		};
	};

	icc0: interconnect-0 {
		compatible = "sandbox,interconnect0";
		#interconnect-cells = <1>;
	};

	icc1: interconnect-1 {
		compatible = "sandbox,interconnect1";
		#interconnect-cells = <1>;
	};

	icc2: interconnect-2 {
		compatible = "sandbox,interconnect2";
		#interconnect-cells = <1>;
	};

	icc3: interconnect-3 {
		compatible = "sandbox,interconnect3";
		#interconnect-cells = <1>;
	};

	icc4: interconnect-4 {
		compatible = "sandbox,interconnect4";
		#interconnect-cells = <1>;
	};

	interconnect-test-0 {
		compatible = "sandbox,interconnect-test";
		interconnects = <&icc0 0 &icc3 0>;
	};

	interconnect-test-1 {
		compatible = "sandbox,interconnect-test";
		interconnects = <&icc1 0 &icc4 0>;
		interconnect-names = "icc-path";
	};

	i2c@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0 1>;
		compatible = "sandbox,i2c";
		clock-frequency = <100000>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_i2c0_pins>;

		eeprom@2c {
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x2c>;
			compatible = "i2c-eeprom";
			sandbox,emul = <&emul_eeprom>;
			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;
				bootcount_i2c: bootcount@10 {
					reg = <10 2>;
				};
			};

			eth3_addr: mac-address@24 {
				reg = <24 6>;
			};
		};

		rtc_0: rtc@43 {
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x43>;
			compatible = "sandbox-rtc";
			sandbox,emul = <&emul0>;

			eth4_addr: mac-address@40 {
				reg = <0x40 6>;
			};
		};

		rtc_1: rtc@61 {
			reg = <0x61>;
			compatible = "sandbox-rtc";
			sandbox,emul = <&emul1>;
		};

		i2c_emul: emul@7f {
			reg = <0x7f>;
			compatible = "sandbox,i2c-emul-parent";
			emul_eeprom: emul-eeprom {
				compatible = "sandbox,i2c-eeprom";
				sandbox,filename = "i2c.bin";
				sandbox,size = <256>;
			};
			emul0: emul0 {
				compatible = "sandbox,i2c-rtc-emul";
			};
			emul1: emull {
				compatible = "sandbox,i2c-rtc-emul";
			};
			emul_pmbus: emul-pmbus {
				compatible = "sandbox,i2c-pmbus";
			};
		};

		sandbox_pmic: sandbox_pmic@40 {
			reg = <0x40>;
			sandbox,emul = <&emul_pmic0>;
		};

		mc34708: pmic@41 {
			reg = <0x41>;
			sandbox,emul = <&emul_pmic1>;
		};

		pmbus@70 {
			reg = <0x70>;
			compatible = "pmbus";
			regulator-name = "sandbox-pmbus-vout";
			sandbox,emul = <&emul_pmbus>;
		};
	};

	i3c0 {
		compatible = "sandbox,i3c";
	};

	i3c1 {
		compatible = "sandbox,i3c";
	};

	bootcount@0 {
		compatible = "u-boot,bootcount-rtc";
		rtc = <&rtc_1>;
		offset = <0x13>;
	};

	bootcount {
		compatible = "u-boot,bootcount-i2c-eeprom";
		i2c-eeprom = <&bootcount_i2c>;
	};

	bootcount_4@0 {
		compatible = "u-boot,bootcount-syscon";
		syscon = <&syscon0>;
		reg = <0x0 0x04>, <0x0 0x04>;
		reg-names = "syscon_reg", "offset";
	};

	bootcount_2@0 {
		compatible = "u-boot,bootcount-syscon";
		syscon = <&syscon0>;
		reg = <0x0 0x04>, <0x0 0x02> ;
		reg-names = "syscon_reg", "offset";
	};

	adc: adc@0 {
		compatible = "sandbox,adc";
		#io-channel-cells = <1>;
		vdd-supply = <&buck2>;
		vss-microvolts = <0>;
	};

	iommu: iommu@0 {
		compatible = "sandbox,iommu";
		#iommu-cells = <0>;
	};

	irq: irq {
		compatible = "sandbox,irq";
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	lcd {
		bootph-all;
		compatible = "sandbox,lcd-sdl";
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_lcd_pins>;
		xres = <1366>;
		yres = <768>;
	};

	leds {
		compatible = "gpio-leds";

		sandbox_led_red: iracibble {
			gpios = <&gpio_a 1 0>;
			label = "sandbox:red";
		};

		sandbox_led_green: martinet {
			gpios = <&gpio_a 2 0>;
			label = "sandbox:green";
		};

		default_on {
			gpios = <&gpio_a 5 0>;
			label = "sandbox:default_on";
			default-state = "on";
		};

		default_off {
			gpios = <&gpio_a 6 0>;
			/* label intentionally omitted */
			default-state = "off";
		};

		led-20 {
			gpios = <&gpio_a 20 0>;
			/* label intentionally omitted */
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_RED>;
			function-enumerator = <20>;
		};

		led-21 {
			gpios = <&gpio_a 21 0>;
			/* label intentionally omitted */
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
		};

		led-22 {
			gpios = <&gpio_a 22 0>;
			/* label intentionally omitted */
			function = LED_FUNCTION_STATUS;
		};

		led-23 {
			gpios = <&gpio_a 23 0>;
			/* label intentionally omitted */
			color = <LED_COLOR_ID_GREEN>;
		};

		led-24 {
			gpios = <&gpio_a 24 0>;
			label = "sandbox:function";
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
		};
	};

	lvds-encoder {
		compatible = "lvds-encoder";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				bridge_input: endpoint {
					/* link to output */
				};
			};

			port@1 {
				reg = <1>;

				bridge_output: endpoint {
					remote-endpoint = <&panel_input>;
				};
			};
		};
	};

	wdt-gpio-toggle {
		gpios = <&gpio_a 8 0>;
		compatible = "linux,wdt-gpio";
		hw_margin_ms = <100>;
		hw_algo = "toggle";
		always-running;
	};

	wdt-gpio-level {
		gpios = <&gpio_a 7 0>;
		compatible = "linux,wdt-gpio";
		hw_margin_ms = <100>;
		hw_algo = "level";
		always-running;
	};

	mbox: mbox {
		compatible = "sandbox,mbox";
		#mbox-cells = <1>;
	};

	mbox-test {
		compatible = "sandbox,mbox-test";
		mboxes = <&mbox 100>, <&mbox 1>;
		mbox-names = "other", "test";
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		timebase-frequency = <2000000>;
		cpu1: cpu@1 {
			device_type = "cpu";
			reg = <0x1>;
			timebase-frequency = <3000000>;
			compatible = "sandbox,cpu_sandbox";
			bootph-all;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			reg = <0x2>;
			compatible = "sandbox,cpu_sandbox";
			bootph-all;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			reg = <0x3>;
			compatible = "sandbox,cpu_sandbox";
			bootph-all;
		};
	};

	chipid: chipid {
		compatible = "sandbox,soc";
	};

	i2s: i2s {
		compatible = "sandbox,i2s";
		#sound-dai-cells = <1>;
		sandbox,silent;	/* Don't emit sounds while testing */
	};

	nop-test_0 {
		compatible = "sandbox,nop_sandbox1";
		nop-test_1 {
			compatible = "sandbox,nop_sandbox2";
			bind = "True";
		};
		nop-test_2 {
			compatible = "sandbox,nop_sandbox2";
			bind = "False";
		};
	};

	memory-controller {
		compatible = "sandbox,memory";
	};

	misc-test {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "sandbox,misc_sandbox";

		eth5_addr: mac-address@10 {
			reg = <0x10 6>;
		};
	};

	mmc2 {
		compatible = "sandbox,mmc";
		non-removable;
	};

	/* This is used for the bootdev tests */
	mmc1 {
		compatible = "sandbox,mmc";
		filename = "mmc1.img";
	};

	/* This is used for the fastboot tests */
	mmc0: mmc0 {
		compatible = "sandbox,mmc";
	};

	/* This is used for VBE VPL tests */
	mmc3 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "image.bin";
		non-removable;
	};

	/* This is used for bootstd bootmenu tests */
	mmc4 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc4.img";
	};

	/* This is used for ChromiumOS tests */
	mmc5 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc5.img";
	};

	/* This is used for mbr tests */
	mmc6 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc6.img";
	};

	/* This is used for Android boot image v4 tests */
	mmc7 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc7.img";
	};

	/* This is used for Android boot image v2 tests. */
	mmc8 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc8.img";
	};

	/* This is used for zip/unzip/gzwrite tests. */
	mmc9 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc9.img";
	};

	/* This is used for RAUC boot tests */
	mmc10 {
		status = "disabled";
		compatible = "sandbox,mmc";
		filename = "mmc10.img";
	};

	pch {
		compatible = "sandbox,pch";
	};

	pci0: pci@0 {
		compatible = "sandbox,pci";
		device_type = "pci";
		bus-range = <0x00 0xff>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges = <0x02000000 0 0x10000000 0x10000000 0 0x2000000
				0x01000000 0 0x20000000 0x20000000 0 0x2000>;
		iommu-map = <0x0010 &iommu 0 1>;
		iommu-map-mask = <0xfffffff8>;
		pci@0,0 {
			compatible = "pci-generic";
			reg = <0x0000 0 0 0 0>;
			sandbox,emul = <&swap_case_emul0_0>;
		};
		pci@1,0 {
			compatible = "pci-generic";
			/* reg 0 is at 0x14, using FDT_PCI_SPACE_MEM32 */
			reg = <0x02000814 0 0 0x80 0
			       0x01000810 0 0 0xc0 0>;
			sandbox,emul = <&swap_case_emul0_1>;
		};
		p2sb-pci@2,0 {
			compatible = "sandbox,p2sb";
			reg = <0x02001010 0 0 0 0>;
			sandbox,emul = <&p2sb_emul>;

			adder {
				intel,p2sb-port-id = <3>;
				compatible = "sandbox,adder";
			};
		};
		pci@1e,0 {
			compatible = "sandbox,pmc";
			reg = <0xf000 0 0 0 0>;
			sandbox,emul = <&pmc_emul1e>;
			acpi-base = <0x400>;
			gpe0-dwx-mask = <0xf>;
			gpe0-dwx-shift-base = <4>;
			gpe0-dw = <6 7 9>;
			gpe0-sts = <0x20>;
			gpe0-en = <0x30>;
		};
		pci@1f,0 {
			compatible = "pci-generic";
			/* reg 0 is at 0x10, using FDT_PCI_SPACE_IO */
			reg = <0x0100f810 0 0 0x100 0>;
			sandbox,emul = <&swap_case_emul0_1f>;
		};
	};

	pci-emul0 {
		compatible = "sandbox,pci-emul-parent";
		swap_case_emul0_0: emul0@0,0 {
			compatible = "sandbox,swap-case";
		};
		swap_case_emul0_1: emul0@1,0 {
			compatible = "sandbox,swap-case";
			use-ea;
		};
		swap_case_emul0_1f: emul0@1f,0 {
			compatible = "sandbox,swap-case";
		};
		p2sb_emul: emul@2,0 {
			compatible = "sandbox,p2sb-emul";
		};
		pmc_emul1e: emul@1e,0 {
			compatible = "sandbox,pmc-emul";
		};
	};

	pci1: pci@1 {
		compatible = "sandbox,pci";
		device_type = "pci";
		bus-range = <0x00 0xff>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges = <0x02000000 0 0x30000000 0x30000000 0 0x2000 // MEM0
			  0x02000000 0 0x31000000 0x3e000000 0 0x2000 // MEM1
			  0x01000000 0 0x40000000 0x40000000 0 0x2000>;
		sandbox,dev-info = <0x08 0x00 0x1234 0x5678
				    0x0c 0x00 0x1234 0x5678
				    0x10 0x00 0x1234 0x5678>;
		pci@10,0 {
			reg = <0x8000 0 0 0 0>;
		};
	};

	pci2: pci@2 {
		compatible = "sandbox,pci";
		device_type = "pci";
		bus-range = <0x00 0xff>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges = <0x02000000 0 0x50000000 0x50000000 0 0x2000
				0x01000000 0 0x60000000 0x60000000 0 0x2000>;
		sandbox,dev-info = <0x08 0x00 0x1234 0x5678>;
		pci@1f,0 {
			compatible = "pci-generic";
			reg = <0xf800 0 0 0 0>;
			sandbox,emul = <&swap_case_emul2_1f>;
		};
	};

	pci-emul2 {
		compatible = "sandbox,pci-emul-parent";
		swap_case_emul2_1f: emul2@1f,0 {
			compatible = "sandbox,swap-case";
		};
	};

	pci_ep: pci_ep {
		compatible = "sandbox,pci_ep";
	};

	probing {
		compatible = "simple-bus";
		test1 {
			compatible = "denx,u-boot-probe-test";
		};

		test2 {
			compatible = "denx,u-boot-probe-test";
		};

		test3 {
			compatible = "denx,u-boot-probe-test";
		};

		test4 {
			compatible = "denx,u-boot-probe-test";
			first-syscon = <&syscon0>;
			second-sys-ctrl = <&another_system_controller>;
			third-syscon = <&syscon2>;
		};
	};

	pwrdom: power-domain {
		compatible = "sandbox,power-domain";
		#power-domain-cells = <1>;
	};

	power-domain-test {
		compatible = "sandbox,power-domain-test";
		power-domains = <&pwrdom 2>;
	};

	pwm: pwm {
		compatible = "sandbox,pwm";
		#pwm-cells = <2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_pwm_pins>;
	};

	pwm2 {
		compatible = "sandbox,pwm";
		#pwm-cells = <2>;
	};

	ram {
		compatible = "sandbox,ram";
	};

	reset@0 {
		compatible = "sandbox,warm-reset";
		bootph-some-ram;
	};

	reset@1 {
		compatible = "sandbox,reset";
		bootph-some-ram;
	};

	resetc: reset-ctl {
		compatible = "sandbox,reset-ctl";
		#reset-cells = <1>;
	};

	resetc_fb: reset-ctl-fallback {
		compatible = "sandbox,reset-ctl-fallback-only";
		#reset-cells = <1>;
	};

	reset-ctl-test {
		compatible = "sandbox,reset-ctl-test";
		resets = <&resetc 100>, <&resetc 2>, <&resetc 20>, <&resetc 40>,
			 <&resetc_fb 5>;
		reset-names = "other", "test", "test2", "test3", "fallback";
	};

	rng {
		compatible = "sandbox,sandbox-rng";
	};

	rproc_1: rproc@1 {
		compatible = "sandbox,test-processor";
		remoteproc-name = "remoteproc-test-dev1";
	};

	rproc_2: rproc@2 {
		compatible = "sandbox,test-processor";
		internal-memory-mapped;
		remoteproc-name = "remoteproc-test-dev2";
	};

	panel {
		compatible = "simple-panel";
		backlight = <&backlight 0 100>;

		display-timings {
			timing@0 {
				/* 1280x800@60Hz */
				clock-frequency = <68000000>;
				hactive = <1280>;
				hfront-porch = <48>;
				hback-porch = <18>;
				hsync-len = <30>;
				vactive = <800>;
				vfront-porch = <3>;
				vback-porch = <12>;
				vsync-len = <5>;
			};
		};

		port {
			panel_input: endpoint {
				remote-endpoint = <&bridge_output>;
			};
		};
	};

	scsi {
		compatible = "sandbox,scsi";
		sandbox,filepath = "scsi.img";
	};

	smem@0 {
		compatible = "sandbox,smem";
	};

	sound {
		compatible = "sandbox,sound";
		cpu {
			sound-dai = <&i2s 0>;
		};

		codec {
			sound-dai = <&audio 0>;
		};
	};

	spi@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0 1>;
		compatible = "sandbox,spi";
		cs-gpios = <0>, <0>, <&gpio_a 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_spi0_pins>;

		spi.bin@0 {
			reg = <0>;
			compatible = "spansion,m25p16", "jedec,spi-nor";
			spi-max-frequency = <40000000>;
			sandbox,filename = "spi.bin";
		};
		spi.bin@1 {
			reg = <1>;
			compatible = "spansion,m25p16", "jedec,spi-nor";
			spi-max-frequency = <50000000>;
			sandbox,filename = "spi.bin";
			spi-cpol;
			spi-cpha;
		};
	};

	syscon0: syscon@0 {
		compatible = "sandbox,syscon0";
		reg = <0x10 16>;
	};

	another_system_controller: syscon@1 {
		compatible = "sandbox,syscon1";
		reg = <0x20 5
			0x28 6
			0x30 7
			0x38 8>;
	};

	syscon2: syscon@2 {
		compatible = "simple-mfd", "syscon";
		reg = <0x40 5
			0x48 6
			0x50 7
			0x58 8>;
	};

	syscon3: syscon@3 {
		compatible = "simple-mfd", "syscon";
		reg = <0x000100 0x10>;

		muxcontroller0: a-mux-controller {
			compatible = "mmio-mux";
			#mux-control-cells = <1>;

			mux-reg-masks = <0x0 0x30>, /* 0: reg 0x0, bits 5:4 */
					<0xc 0x1E>, /* 1: reg 0xc, bits 4:1 */
					<0x4 0xFF>; /* 2: reg 0x4, bits 7:0 */
			idle-states = <MUX_IDLE_AS_IS>, <0x02>, <0x73>;
			u-boot,mux-autoprobe;
		};
	};

	muxcontroller1: emul-mux-controller {
		compatible = "mux-emul";
		#mux-control-cells = <0>;
		u-boot,mux-autoprobe;
		idle-state = <0xabcd>;
	};

	testfdtm0 {
		compatible = "denx,u-boot-fdtm-test";
	};

	testfdtm1: testfdtm1 {
		compatible = "denx,u-boot-fdtm-test";
	};

	testfdtm2 {
		compatible = "denx,u-boot-fdtm-test";
	};

	timer@0 {
		compatible = "sandbox,timer";
		clock-frequency = <1000000>;
	};

	timer@1 {
		compatible = "sandbox,timer";
		sandbox,timebase-frequency-fallback;
	};

	tpm2 {
		compatible = "sandbox,tpm2";
		memory-region = <&event_log>;
	};

	tpm {
		compatible = "google,sandbox-tpm";
	};

	uart0: serial {
		compatible = "sandbox,serial";
		bootph-all;
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_uart0_pins>;
	};

	usb_0: usb@0 {
		compatible = "sandbox,usb";
		status = "disabled";
		hub {
			compatible = "sandbox,usb-hub";
			#address-cells = <1>;
			#size-cells = <0>;
			flash-stick {
				reg = <0>;
				compatible = "sandbox,usb-flash";
			};
		};
	};

	usb_1: usb@1 {
		compatible = "sandbox,usb";
		iommus = <&iommu>;
		hub {
			compatible = "usb-hub";
			usb,device-class = <9>;
			#address-cells = <1>;
			#size-cells = <0>;
			hub-emul {
				compatible = "sandbox,usb-hub";
				#address-cells = <1>;
				#size-cells = <0>;
				flash-stick@0 {
					reg = <0>;
					compatible = "sandbox,usb-flash";
					sandbox,filepath = "testflash.bin";
				};

				flash-stick@1 {
					reg = <1>;
					compatible = "sandbox,usb-flash";
					sandbox,filepath = "flash1.img";
				};

				flash-stick@2 {
					reg = <2>;
					compatible = "sandbox,usb-flash";
					sandbox,filepath = "testflash2.bin";
				};

				keyb@3 {
					reg = <3>;
					compatible = "sandbox,usb-keyb";
				};

			};

			usbstor@1 {
				reg = <1>;
			};
			usbstor@3 {
				reg = <3>;
			};
		};
	};

	usb_2: usb@2 {
		compatible = "sandbox,usb";
		status = "disabled";
	};

	spmi: spmi@0 {
		compatible = "sandbox,spmi";
		#address-cells = <0x1>;
		#size-cells = <0x1>;
		ranges;
		pm8916@0 {
			compatible = "qcom,spmi-pmic";
			reg = <0x0 0x1>;
			#address-cells = <0x1>;
			#size-cells = <0x1>;
			ranges;

			spmi_gpios: gpios@c000 {
				compatible = "qcom,pm8916-gpio";
				reg = <0xc000 0x400>;
				gpio-ranges = <&spmi_gpios 0 0 4>;
				gpio-controller;
				gpio-count = <4>;
				#gpio-cells = <2>;
			};
		};
	};

	wdt0: wdt@0 {
		compatible = "sandbox,wdt";
		hw_margin_ms = <200>;
	};

	axi: axi@0 {
		compatible = "sandbox,axi";
		#address-cells = <0x1>;
		#size-cells = <0x1>;
		store@0 {
			compatible = "sandbox,sandbox_store";
			reg = <0x0 0x400>;
		};
	};

	chosen {
		#address-cells = <1>;
		#size-cells = <1>;
		setting = "sunrise ohoka";
		other-node = "/some-bus/c-test@5";
		int-values = <0x1937 72993>;
		u-boot,acpi-ssdt-order = <&acpi_test2 &acpi_test1>;
		stdout-path = "serial0:115200n8";
		chosen-test {
			compatible = "denx,u-boot-fdt-test";
			reg = <9 1>;
		};
	};

	translation-test@8000 {
		compatible = "simple-bus";
		reg = <0x8000 0x4000>;

		#address-cells = <0x2>;
		#size-cells = <0x1>;

		ranges = <0 0x0 0x8000 0x1000
			  1 0x100 0x9000 0x1000
			  2 0x200 0xA000 0x1000
			  3 0x300 0xB000 0x1000
			 >;

		dma-ranges = <0 0x000 0x10000000 0x1000
			      1 0x100 0x20000000 0x1000
			     >;

		dev@0,0 {
			compatible = "denx,u-boot-fdt-dummy";
			reg = <0 0x0 0x1000>;
			reg-names = "sandbox-dummy-0";
		};

		dev@1,100 {
			compatible = "denx,u-boot-fdt-dummy";
			reg = <1 0x100 0x1000>;

		};

		dev@2,200 {
			compatible = "denx,u-boot-fdt-dummy";
			reg = <2 0x200 0x1000>;
		};


		noxlatebus@3,300 {
			compatible = "simple-bus";
			reg = <3 0x300 0x1000>;

			#address-cells = <0x1>;
			#size-cells = <0x0>;

			dev@42 {
				compatible = "denx,u-boot-fdt-dummy";
				reg = <0x42>;
			};
		};
	};

	ofnode-foreach {
		compatible = "foreach";

		first {
			prop1 = <1>;
			prop2 = <2>;
		};

		second {
			prop1 = <1>;
			prop2 = <2>;
		};
	};

	osd {
		compatible = "sandbox,sandbox_osd";
	};

	sandbox_tee {
		compatible = "sandbox,tee";
	};

	sandbox_virtio1 {
		compatible = "sandbox,virtio1";
		virtio-type = <4>;	/* rng */
	};

	sandbox_virtio2 {
		compatible = "sandbox,virtio2";
	};

	sandbox-virtio-blk {
		compatible = "sandbox,virtio1";
		virtio-type = <2>;	/* block */
	};

	sandbox_scmi {
		compatible = "sandbox,scmi-devices";
		power-domains = <&pwrdom_scmi 2>;
		clocks = <&clk_scmi 2>, <&clk_scmi 0>;
		resets = <&reset_scmi 3>;
		regul0-supply = <&regul0_scmi>;
		regul1-supply = <&regul1_scmi>;
	};

	pinctrl {
		compatible = "sandbox,pinctrl";

		pinctrl-names = "default", "alternate";
		pinctrl-0 = <&pinctrl_gpios>, <&pinctrl_i2s>;
		pinctrl-1 = <&pinctrl_spi>, <&pinctrl_i2c>;

		pinctrl_gpios: pins-gpios {
			gpio0 {
				pins = "P5";
				function = "GPIO";
				bias-pull-up;
				input-disable;
			};
			gpio1 {
				pins = "P6";
				function = "GPIO";
				output-high;
				drive-open-drain;
			};
			gpio2 {
				pinmux = <SANDBOX_PINMUX(7, SANDBOX_PINMUX_GPIO)>;
				bias-pull-down;
				input-enable;
			};
			gpio3 {
				pinmux = <SANDBOX_PINMUX(8, SANDBOX_PINMUX_GPIO)>;
				bias-disable;
			};
		};

		pinctrl_i2c: pins-i2c {
			groups {
				groups = "I2C_UART";
				function = "I2C";
			};

			pins {
				pins = "P0", "P1";
				drive-open-drain;
			};
		};

		pinctrl_i2s: pins-i2s {
			groups = "SPI_I2S";
			function = "I2S";
		};

		pinctrl_spi: pins-spi {
			groups = "SPI_I2S";
			function = "SPI";

			cs {
				pinmux = <SANDBOX_PINMUX(5, SANDBOX_PINMUX_CS)>,
					 <SANDBOX_PINMUX(6, SANDBOX_PINMUX_CS)>;
			};
		};
	};

	pinctrl-single-no-width {
		compatible = "pinctrl-single";
		reg = <0x0000 0x238>;
		#pinctrl-cells = <1>;
		pinctrl-single,function-mask = <0x7f>;
	};

	pinctrl-single-pins {
		compatible = "pinctrl-single";
		reg = <0x0000 0x238>;
		#pinctrl-cells = <1>;
		pinctrl-single,register-width = <32>;
		pinctrl-single,function-mask = <0x7f>;

		pinmux_pwm_pins: pinmux_pwm_pins {
			pinctrl-single,pins = < 0x48 0x06 >;
		};

		pinmux_spi0_pins: pinmux_spi0_pins {
			pinctrl-single,pins = <
				0x190 0x0c
				0x194 0x0c
				0x198 0x23
				0x19c 0x0c
			>;
		};

		pinmux_uart0_pins: pinmux_uart0_pins {
			pinctrl-single,pins = <
				0x70 0x30
				0x74 0x00
			>;
		};
	};

	pinctrl-single-bits {
		compatible = "pinctrl-single";
		reg = <0x0000 0x50>;
		#pinctrl-cells = <2>;
		pinctrl-single,bit-per-mux;
		pinctrl-single,register-width = <32>;
		pinctrl-single,function-mask = <0xf>;

		pinmux_i2c0_pins: pinmux_i2c0_pins {
			pinctrl-single,bits = <
				0x10 0x00002200 0x0000ff00
			>;
		};

		pinmux_lcd_pins: pinmux_lcd_pins {
			pinctrl-single,bits = <
				0x40 0x22222200 0xffffff00
				0x44 0x22222222 0xffffffff
				0x48 0x00000022 0x000000ff
				0x48 0x02000000 0x0f000000
				0x4c 0x02000022 0x0f0000ff
			>;
		};
	};

	hwspinlock@0 {
		compatible = "sandbox,hwspinlock";
	};

	dma: dma {
		compatible = "sandbox,dma";
		#dma-cells = <1>;

		dmas = <&dma 0>, <&dma 1>, <&dma 2>;
		dma-names = "m2m", "tx0", "rx0";
	};

	/*
	 * keep mdio-mux ahead of mdio so that the mux is removed first at the
	 * end of the test.  If parent mdio is removed first, clean-up of the
	 * mux will trigger a 2nd probe of parent-mdio, leaving parent-mdio
	 * active at the end of the test.  That it turn doesn't allow the mdio
	 * class to be destroyed, triggering an error.
	 */
	mdio-mux-test {
		compatible = "sandbox,mdio-mux";
		#address-cells = <1>;
		#size-cells = <0>;
		mdio-parent-bus = <&mdio>;

		mdio-ch-test@0 {
			reg = <0>;
		};
		mdio-ch-test@1 {
			reg = <1>;
		};
	};

	mdio: mdio-test {
		compatible = "sandbox,mdio";
		#address-cells = <1>;
		#size-cells = <0>;

		ethphy1: ethernet-phy@1 {
			reg = <1>;
		};
	};

	pm-bus-test {
		compatible = "simple-pm-bus";
		clocks = <&clk_sandbox 4>;
		power-domains = <&pwrdom 1>;
	};

	resetc2: syscon-reset {
		compatible = "syscon-reset";
		#reset-cells = <1>;
		regmap = <&syscon0>;
		offset = <1>;
		mask = <0x27FFFFFF>;
		assert-high = <0>;
	};

	syscon-reset-test {
		compatible = "sandbox,misc_sandbox";
		resets = <&resetc2 15>, <&resetc2 30>, <&resetc2 60>;
		reset-names = "valid", "no_mask", "out_of_range";
	};

	sysinfo {
		compatible = "sandbox,sysinfo-sandbox";
	};

	sysinfo-gpio {
		compatible = "gpio-sysinfo";
		gpios = <&gpio_a 15>, <&gpio_a 16>, <&gpio_a 17>;
		revisions = <19>, <5>;
		names = "rev_a", "foo";
	};

	some_regmapped-bus {
		#address-cells = <0x1>;
		#size-cells = <0x1>;

		ranges = <0x0 0x0 0x10>;
		compatible = "simple-bus";

		regmap-test_0 {
			reg = <0 0x10>;
			compatible = "sandbox,regmap_test";
		};
	};

	thermal {
		compatible = "sandbox,thermal";
	};

	fwu-mdata {
		compatible = "u-boot,fwu-mdata-gpt";
		fwu-mdata-store = <&mmc0>;
	};

	nvmxip-qspi1@08000000 {
		compatible = "nvmxip,qspi";
		reg = <0x08000000 0x00200000>;
		lba_shift = <9>;
		lba = <4096>;
	};

	nvmxip-qspi2@08200000 {
		compatible = "nvmxip,qspi";
		reg = <0x08200000 0x00100000>;
		lba_shift = <9>;
		lba = <2048>;
	};

	extcon {
		compatible = "sandbox,extcon";
	};

	arm-ffa-emul {
		compatible = "sandbox,arm-ffa-emul";

		sandbox-arm-ffa {
				compatible = "sandbox,arm-ffa";
		};
	};

	nand-controller {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "sandbox,nand";

		nand@0 {
			reg = <0>;
			nand-ecc-mode = "soft";
			sandbox,id = [00 e3];
			sandbox,erasesize = <(8 * 1024)>;
			sandbox,oobsize = <16>;
			sandbox,pagesize = <512>;
			sandbox,pages = <0x2000>;
			sandbox,err-count = <1>;
			sandbox,err-step-size = <512>;
		};

		/* MT29F64G08AKABA */
		nand@1 {
			reg = <1>;
			nand-ecc-mode = "soft_bch";
			sandbox,id = [2C 48 00 26 89 00 00 00];
			sandbox,onfi = [
				4f 4e 46 49 0e 00 5a 00
				ff 01 00 00 00 00 03 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				4d 49 43 52 4f 4e 20 20
				20 20 20 20 4d 54 32 39
				46 36 34 47 30 38 41 4b
				41 42 41 43 35 20 20 20
				2c 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 10 00 00 e0 00 00 02
				00 00 1c 00 80 00 00 00
				00 10 00 00 02 23 01 50
				00 01 05 01 00 00 04 00
				04 01 1e 00 00 00 00 00
				00 00 00 00 00 00 00 00
				0e 1f 00 1f 00 f4 01 ac
				0d 19 00 c8 00 00 00 00
				00 00 00 00 00 00 0a 07
				19 00 00 00 00 00 00 00
				00 00 00 00 01 00 01 00
				00 00 04 10 01 81 04 02
				02 01 1e 90 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 00 00 00
				00 00 00 00 00 03 20 7d
			];
			sandbox,erasesize = <(512 * 1024)>;
			sandbox,oobsize = <224>;
			sandbox,pagesize = <4096>;
			sandbox,pages = <0x200000>;
			sandbox,err-count = <3>;
			sandbox,err-step-size = <512>;
		};
	};

	graph1 {
		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				#address-cells = <1>;
				#size-cells = <0>;

				reg = <0>;

				endpoint@0 {
					reg = <0>;
				};

				endpoint@1 {
					reg = <1>;
				};
			};

			port@1 {
				reg = <1>;

				endpoint {
					test-property-0;
				};
			};

			port@2 {
				#address-cells = <1>;
				#size-cells = <0>;

				reg = <2>;

				graph2_link: endpoint@0 {
					reg = <0>;
					test-property-1;
					remote-endpoint = <&graph1_link>;
				};

				endpoint@1 {
					reg = <1>;
				};
			};
		};
	};

	graph2 {
		port {
			graph1_link: endpoint {
				remote-endpoint = <&graph2_link>;
			};
		};
	};

	aes-engine {
		compatible = "software-aes-engine";
	};
};

#include "sandbox_pmic.dtsi"
#include "cros-ec-keyboard.dtsi"

#ifdef CONFIG_SANDBOX_VPL
#include "sandbox_vpl.dtsi"
#endif

#if IS_ENABLED(CONFIG_EFI_HAVE_CAPSULE_SUPPORT)
#include "sandbox_capsule.dtsi"
#endif

#include "cedit.dtsi"
