/* SPDX-License-Identifier: GPL-2.0+ */
/*
 * Copyright (C) 2011 Marek Vasut <marek.vasut@gmail.com>
 * on behalf of DENX Software Engineering GmbH
 *
 * January 2004 - Changed to support H4 device
 * Copyright (c) 2004-2008 Texas Instruments
 *
 * (C) Copyright 2002
 * Gary Jennejohn, DENX Software Engineering, <garyj@denx.de>
 */

OUTPUT_FORMAT("elf32-littlearm", "elf32-littlearm", "elf32-littlearm")
OUTPUT_ARCH(arm)
ENTRY(_start)
SECTIONS
{
	. = IMAGE_TEXT_BASE;

	. = ALIGN(4);
	.text	:
	{
		*(.vectors)
		arch/arm/cpu/arm926ejs/mxs/start.o	(.text*)
		*(.text*)
	}

	. = ALIGN(4);
	.rodata : { *(SORT_BY_ALIGNMENT(SORT_BY_NAME(.rodata*))) }

	. = ALIGN(4);
	.data : {
		*(.data*)
	}

	.bss : {
		. = ALIGN(4);
		__bss_start = .;
		*(.bss*)
		. = ALIGN(8);
		__bss_end = .;
	}

	_end = .;
	_image_binary_end = .;

	.dynsym _image_binary_end : { *(.dynsym) }
	.dynbss : { *(.dynbss) }
	.dynstr : { *(.dynstr*) }
	.dynamic : { *(.dynamic*) }
	.hash : { *(.hash*) }
	.plt : { *(.plt*) }
	.interp : { *(.interp*) }
	.gnu : { *(.gnu*) }
	.ARM.exidx : { *(.ARM.exidx*) }
}

ASSERT(_image_binary_end % 8 == 0, \
       "_image_binary_end must be 8-byte aligned for device tree");
