// SPDX-License-Identifier: GPL-2.0+

/ {
	/* When running as a first-stage bootloader this isn't filled in automatically */
	memory@80000000 {
		device_type = "memory";
		reg = <0x0 0x80000000 0x0 0x20000000>;
	};
};

#include "an7581-u-boot.dtsi"

&gdm1 {
	status = "okay";
};

&gdm2 {
	status = "okay";

	managed = "in-band-status";
	phy-mode = "10gbase-r";
};

&gdm4 {
	status = "okay";

	managed = "in-band-status";
	phy-mode = "usxgmii";
};
