/*
 * Samsung's Exynos4x12 SoCs device tree source
 *
 * Copyright (c) 2012 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 *
 * Samsung's Exynos4x12 SoCs device nodes are listed in this file. Exynos4x12
 * based board files can include this file and provide values for board specfic
 * bindings.
 *
 * Note: This file does not include device nodes for all the controllers in
 * Exynos4x12 SoC. As device tree coverage for Exynos4x12 increases, additional
 * nodes can be added to this file.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
` * published by the Free Software Foundation.
*/

#include "exynos4.dtsi"
#include "exynos4x12-pinctrl.dtsi"
#include "exynos4x12-pinctrl-uboot.dtsi"

/ {
	aliases {
		pinctrl0 = &pinctrl_0;
		pinctrl1 = &pinctrl_1;
		pinctrl2 = &pinctrl_2;
		pinctrl3 = &pinctrl_3;
	};

	pd_isp: isp-power-domain@10023CA0 {
		compatible = "samsung,exynos4210-pd";
		reg = <0x10023CA0 0x20>;
	};

	clock: clock-controller@10030000 {
		compatible = "samsung,exynos4412-clock";
		reg = <0x10030000 0x20000>;
		#clock-cells = <1>;
	};

	mct@10050000 {
		compatible = "samsung,exynos4412-mct";
		reg = <0x10050000 0x800>;
		interrupt-parent = <&mct_map>;
		interrupts = <0>, <1>, <2>, <3>, <4>;
		clocks = <&clock 3>, <&clock 344>;
		clock-names = "fin_pll", "mct";

		mct_map: mct-map {
			#interrupt-cells = <1>;
			#address-cells = <0>;
			#size-cells = <0>;
			interrupt-map = <0 &gic 0 57 0>,
					<1 &combiner 12 5>,
					<2 &combiner 12 6>,
					<3 &combiner 12 7>,
					<4 &gic 1 12 0>;
		};
	};

	pinctrl_0: pinctrl@11400000 {
		compatible = "samsung,exynos4x12-pinctrl";
		reg = <0x11400000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 47 0>;
	};

	pinctrl_1: pinctrl@11000000 {
		compatible = "samsung,exynos4x12-pinctrl";
		reg = <0x11000000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 46 0>;

		wakup_eint: wakeup-interrupt-controller {
			compatible = "samsung,exynos4210-wakeup-eint";
			interrupt-parent = <&gic>;
			interrupts = <0 32 0>;
		};
	};

	pinctrl_2: pinctrl@03860000 {
		compatible = "samsung,exynos4x12-pinctrl";
		reg = <0x03860000 0x1000>;
		interrupt-parent = <&combiner>;
		interrupts = <10 0>;
	};

	pinctrl_3: pinctrl@106E0000 {
		compatible = "samsung,exynos4x12-pinctrl";
		reg = <0x106E0000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 72 0>;
	};

	g2d@10800000 {
		compatible = "samsung,exynos4212-g2d";
		reg = <0x10800000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 89 0>;
		clocks = <&clock 177>, <&clock 277>;
		clock-names = "sclk_fimg2d", "fimg2d";
		status = "disabled";
	};
};
