/*
 * sama5d3.dtsi - Device Tree Include file for SAMA5D3 family SoC
 *                applies to SAMA5D31, SAMA5D33, SAMA5D34, SAMA5D35, SAMA5D36 SoC
 *
 *  Copyright (C) 2013 Atmel,
 *                2013 Ludovic Desroches <ludovic.desroches@atmel.com>
 *
 * Licensed under GPLv2 or later.
 */

#include "skeleton.dtsi"
#include <dt-bindings/dma/at91.h>
#include <dt-bindings/pinctrl/at91.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/clock/at91.h>

/ {
	model = "Atmel SAMA5D3 family SoC";
	compatible = "atmel,sama5d3", "atmel,sama5";
	interrupt-parent = <&aic>;

	aliases {
		serial0 = &dbgu;
		serial1 = &usart0;
		serial2 = &usart1;
		serial3 = &usart2;
		serial4 = &usart3;
		serial5 = &uart0;
		gpio0 = &pioA;
		gpio1 = &pioB;
		gpio2 = &pioC;
		gpio3 = &pioD;
		gpio4 = &pioE;
		tcb0 = &tcb0;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		ssc0 = &ssc0;
		ssc1 = &ssc1;
		pwm0 = &pwm0;
	};
	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a5";
			reg = <0x0>;
		};
	};

	pmu {
		compatible = "arm,cortex-a5-pmu";
		interrupts = <46 IRQ_TYPE_LEVEL_HIGH 0>;
	};

	memory {
		reg = <0x20000000 0x8000000>;
	};

	clocks {
		slow_xtal: slow_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		main_xtal: main_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		adc_op_clk: adc_op_clk{
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <1000000>;
		};
	};

	sram: sram@00300000 {
		compatible = "mmio-sram";
		reg = <0x00300000 0x20000>;
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		bootph-all;

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			bootph-all;

			mmc0: mmc@f0000000 {
				compatible = "atmel,hsmci";
				reg = <0xf0000000 0x600>;
				interrupts = <21 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(0)>;
				dma-names = "rxtx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mmc0_clk_cmd_dat0 &pinctrl_mmc0_dat1_3 &pinctrl_mmc0_dat4_7>;
				status = "disabled";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci0_clk>;
				clock-names = "mci_clk";
			};

			spi0: spi@f0004000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xf0004000 0x100>;
				interrupts = <24 IRQ_TYPE_LEVEL_HIGH 3>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(1)>,
				       <&dma0 2 AT91_DMA_CFG_PER_ID(2)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi0>;
				clocks = <&spi0_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			ssc0: ssc@f0008000 {
				compatible = "atmel,at91sam9g45-ssc";
				reg = <0xf0008000 0x4000>;
				interrupts = <38 IRQ_TYPE_LEVEL_HIGH 4>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(13)>,
				       <&dma0 2 AT91_DMA_CFG_PER_ID(14)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc0_tx &pinctrl_ssc0_rx>;
				clocks = <&ssc0_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			tcb0: timer@f0010000 {
				compatible = "atmel,at91sam9x5-tcb";
				reg = <0xf0010000 0x100>;
				interrupts = <26 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&tcb0_clk>, <&clk32k>;
				clock-names = "t0_clk", "slow_clk";
			};

			i2c0: i2c@f0014000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf0014000 0x4000>;
				interrupts = <18 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(7)>,
				       <&dma0 2 AT91_DMA_CFG_PER_ID(8)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c0>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi0_clk>;
				status = "disabled";
			};

			i2c1: i2c@f0018000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf0018000 0x4000>;
				interrupts = <19 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(9)>,
				       <&dma0 2 AT91_DMA_CFG_PER_ID(10)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c1>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi1_clk>;
				status = "disabled";
			};

			usart0: serial@f001c000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf001c000 0x100>;
				interrupts = <12 IRQ_TYPE_LEVEL_HIGH 5>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(3)>,
				       <&dma0 2 (AT91_DMA_CFG_PER_ID(4) | AT91_DMA_CFG_FIFOCFG_ASAP)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart0>;
				clocks = <&usart0_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart1: serial@f0020000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf0020000 0x100>;
				interrupts = <13 IRQ_TYPE_LEVEL_HIGH 5>;
				dmas = <&dma0 2 AT91_DMA_CFG_PER_ID(5)>,
				       <&dma0 2 (AT91_DMA_CFG_PER_ID(6) | AT91_DMA_CFG_FIFOCFG_ASAP)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart1>;
				clocks = <&usart1_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			uart0: serial@f0024000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf0024000 0x100>;
				interrupts = <16 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_uart0>;
				clocks = <&uart0_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			pwm0: pwm@f002c000 {
				compatible = "atmel,sama5d3-pwm";
				reg = <0xf002c000 0x300>;
				interrupts = <28 IRQ_TYPE_LEVEL_HIGH 4>;
				#pwm-cells = <3>;
				clocks = <&pwm_clk>;
				status = "disabled";
			};

			isi: isi@f0034000 {
				compatible = "atmel,at91sam9g45-isi";
				reg = <0xf0034000 0x4000>;
				interrupts = <37 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_isi_data_0_7>;
				clocks = <&isi_clk>;
				clock-names = "isi_clk";
				status = "disabled";
			};

			sfr: sfr@f0038000 {
				compatible = "atmel,sama5d3-sfr", "syscon";
				reg = <0xf0038000 0x60>;
			};

			mmc1: mmc@f8000000 {
				compatible = "atmel,hsmci";
				reg = <0xf8000000 0x600>;
				interrupts = <22 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(0)>;
				dma-names = "rxtx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mmc1_clk_cmd_dat0 &pinctrl_mmc1_dat1_3>;
				status = "disabled";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci1_clk>;
				clock-names = "mci_clk";
			};

			spi1: spi@f8008000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xf8008000 0x100>;
				interrupts = <25 IRQ_TYPE_LEVEL_HIGH 3>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(15)>,
				       <&dma1 2 AT91_DMA_CFG_PER_ID(16)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi1>;
				clocks = <&spi1_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			ssc1: ssc@f800c000 {
				compatible = "atmel,at91sam9g45-ssc";
				reg = <0xf800c000 0x4000>;
				interrupts = <39 IRQ_TYPE_LEVEL_HIGH 4>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(3)>,
				       <&dma1 2 AT91_DMA_CFG_PER_ID(4)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc1_tx &pinctrl_ssc1_rx>;
				clocks = <&ssc1_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			adc0: adc@f8018000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91sam9x5-adc";
				reg = <0xf8018000 0x100>;
				interrupts = <29 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <
					&pinctrl_adc0_adtrg
					&pinctrl_adc0_ad0
					&pinctrl_adc0_ad1
					&pinctrl_adc0_ad2
					&pinctrl_adc0_ad3
					&pinctrl_adc0_ad4
					&pinctrl_adc0_ad5
					&pinctrl_adc0_ad6
					&pinctrl_adc0_ad7
					&pinctrl_adc0_ad8
					&pinctrl_adc0_ad9
					&pinctrl_adc0_ad10
					&pinctrl_adc0_ad11
					>;
				clocks = <&adc_clk>,
					 <&adc_op_clk>;
				clock-names = "adc_clk", "adc_op_clk";
				atmel,adc-channels-used = <0xfff>;
				atmel,adc-startup-time = <40>;
				atmel,adc-use-external-triggers;
				atmel,adc-vref = <3000>;
				atmel,adc-res = <10 12>;
				atmel,adc-sample-hold-time = <11>;
				atmel,adc-res-names = "lowres", "highres";
				status = "disabled";

				trigger@0 {
					reg = <0>;
					trigger-name = "external-rising";
					trigger-value = <0x1>;
					trigger-external;
				};
				trigger@1 {
					reg = <1>;
					trigger-name = "external-falling";
					trigger-value = <0x2>;
					trigger-external;
				};
				trigger@2 {
					reg = <2>;
					trigger-name = "external-any";
					trigger-value = <0x3>;
					trigger-external;
				};
				trigger@3 {
					reg = <3>;
					trigger-name = "continuous";
					trigger-value = <0x6>;
				};
			};

			i2c2: i2c@f801c000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf801c000 0x4000>;
				interrupts = <20 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(11)>,
				       <&dma1 2 AT91_DMA_CFG_PER_ID(12)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c2>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi2_clk>;
				status = "disabled";
			};

			usart2: serial@f8020000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8020000 0x100>;
				interrupts = <14 IRQ_TYPE_LEVEL_HIGH 5>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(7)>,
				       <&dma1 2 (AT91_DMA_CFG_PER_ID(8) | AT91_DMA_CFG_FIFOCFG_ASAP)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart2>;
				clocks = <&usart2_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart3: serial@f8024000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8024000 0x100>;
				interrupts = <15 IRQ_TYPE_LEVEL_HIGH 5>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(9)>,
				       <&dma1 2 (AT91_DMA_CFG_PER_ID(10) | AT91_DMA_CFG_FIFOCFG_ASAP)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart3>;
				clocks = <&usart3_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			sha@f8034000 {
				compatible = "atmel,at91sam9g46-sha";
				reg = <0xf8034000 0x100>;
				interrupts = <42 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(17)>;
				dma-names = "tx";
				clocks = <&sha_clk>;
				clock-names = "sha_clk";
			};

			aes@f8038000 {
				compatible = "atmel,at91sam9g46-aes";
				reg = <0xf8038000 0x100>;
				interrupts = <43 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(18)>,
				       <&dma1 2 AT91_DMA_CFG_PER_ID(19)>;
				dma-names = "tx", "rx";
				clocks = <&aes_clk>;
				clock-names = "aes_clk";
			};

			tdes@f803c000 {
				compatible = "atmel,at91sam9g46-tdes";
				reg = <0xf803c000 0x100>;
				interrupts = <44 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(20)>,
				       <&dma1 2 AT91_DMA_CFG_PER_ID(21)>;
				dma-names = "tx", "rx";
				clocks = <&tdes_clk>;
				clock-names = "tdes_clk";
			};

			trng@f8040000 {
				compatible = "atmel,at91sam9g45-trng";
				reg = <0xf8040000 0x100>;
				interrupts = <45 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&trng_clk>;
			};

			dma0: dma-controller@ffffe600 {
				compatible = "atmel,at91sam9g45-dma";
				reg = <0xffffe600 0x200>;
				interrupts = <30 IRQ_TYPE_LEVEL_HIGH 0>;
				#dma-cells = <2>;
				clocks = <&dma0_clk>;
				clock-names = "dma_clk";
			};

			dma1: dma-controller@ffffe800 {
				compatible = "atmel,at91sam9g45-dma";
				reg = <0xffffe800 0x200>;
				interrupts = <31 IRQ_TYPE_LEVEL_HIGH 0>;
				#dma-cells = <2>;
				clocks = <&dma1_clk>;
				clock-names = "dma_clk";
			};

			ramc0: ramc@ffffea00 {
				compatible = "atmel,sama5d3-ddramc";
				reg = <0xffffea00 0x200>;
				clocks = <&ddrck>, <&mpddr_clk>;
				clock-names = "ddrck", "mpddr";
			};

			dbgu: serial@ffffee00 {
				compatible = "atmel,at91sam9260-dbgu", "atmel,at91sam9260-usart";
				reg = <0xffffee00 0x200>;
				interrupts = <2 IRQ_TYPE_LEVEL_HIGH 7>;
				dmas = <&dma1 2 AT91_DMA_CFG_PER_ID(13)>,
				       <&dma1 2 (AT91_DMA_CFG_PER_ID(14) | AT91_DMA_CFG_FIFOCFG_ASAP)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_dbgu>;
				clocks = <&dbgu_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			aic: interrupt-controller@fffff000 {
				#interrupt-cells = <3>;
				compatible = "atmel,sama5d3-aic";
				interrupt-controller;
				reg = <0xfffff000 0x200>;
				atmel,external-irqs = <47>;
			};

			pinctrl@fffff200 {
				bootph-all;
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "atmel,sama5d3-pinctrl", "atmel,at91sam9x5-pinctrl", "simple-bus";
				ranges = <0xfffff200 0xfffff200 0xa00>;
				atmel,mux-mask = <
					/*   A          B          C  */
					0xffffffff 0xc0fc0000 0xc0ff0000	/* pioA */
					0xffffffff 0x0ff8ffff 0x00000000	/* pioB */
					0xffffffff 0xbc00f1ff 0x7c00fc00	/* pioC */
					0xffffffff 0xc001c0e0 0x0001c1e0	/* pioD */
					0xffffffff 0xbf9f8000 0x18000000	/* pioE */
					>;

				/* shared pinctrl settings */
				adc0 {
					pinctrl_adc0_adtrg: adc0_adtrg {
						atmel,pins =
							<AT91_PIOD 19 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD19 periph A ADTRG */
					};
					pinctrl_adc0_ad0: adc0_ad0 {
						atmel,pins =
							<AT91_PIOD 20 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD20 periph A AD0 */
					};
					pinctrl_adc0_ad1: adc0_ad1 {
						atmel,pins =
							<AT91_PIOD 21 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD21 periph A AD1 */
					};
					pinctrl_adc0_ad2: adc0_ad2 {
						atmel,pins =
							<AT91_PIOD 22 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD22 periph A AD2 */
					};
					pinctrl_adc0_ad3: adc0_ad3 {
						atmel,pins =
							<AT91_PIOD 23 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD23 periph A AD3 */
					};
					pinctrl_adc0_ad4: adc0_ad4 {
						atmel,pins =
							<AT91_PIOD 24 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD24 periph A AD4 */
					};
					pinctrl_adc0_ad5: adc0_ad5 {
						atmel,pins =
							<AT91_PIOD 25 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD25 periph A AD5 */
					};
					pinctrl_adc0_ad6: adc0_ad6 {
						atmel,pins =
							<AT91_PIOD 26 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD26 periph A AD6 */
					};
					pinctrl_adc0_ad7: adc0_ad7 {
						atmel,pins =
							<AT91_PIOD 27 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD27 periph A AD7 */
					};
					pinctrl_adc0_ad8: adc0_ad8 {
						atmel,pins =
							<AT91_PIOD 28 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD28 periph A AD8 */
					};
					pinctrl_adc0_ad9: adc0_ad9 {
						atmel,pins =
							<AT91_PIOD 29 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD29 periph A AD9 */
					};
					pinctrl_adc0_ad10: adc0_ad10 {
						atmel,pins =
							<AT91_PIOD 30 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD30 periph A AD10, conflicts with PCK0 */
					};
					pinctrl_adc0_ad11: adc0_ad11 {
						atmel,pins =
							<AT91_PIOD 31 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD31 periph A AD11, conflicts with PCK1 */
					};
				};

				dbgu {
					bootph-all;
					pinctrl_dbgu: dbgu-0 {
						bootph-all;
						atmel,pins =
							<AT91_PIOB 30 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB30 periph A */
							 AT91_PIOB 31 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PB31 periph A with pullup */
					};
				};

				i2c0 {
					pinctrl_i2c0: i2c0-0 {
						atmel,pins =
							<AT91_PIOA 30 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA30 periph A TWD0 pin, conflicts with URXD1, ISI_VSYNC */
							 AT91_PIOA 31 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA31 periph A TWCK0 pin, conflicts with UTXD1, ISI_HSYNC */
					};
				};

				i2c1 {
					pinctrl_i2c1: i2c1-0 {
						atmel,pins =
							<AT91_PIOC 26 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PC26 periph B TWD1 pin, conflicts with SPI1_NPCS1, ISI_D11 */
							 AT91_PIOC 27 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PC27 periph B TWCK1 pin, conflicts with SPI1_NPCS2, ISI_D10 */
					};
				};

				i2c2 {
					pinctrl_i2c2: i2c2-0 {
						atmel,pins =
							<AT91_PIOA 18 AT91_PERIPH_B AT91_PINCTRL_NONE	/* TWD2 pin, conflicts with LCDDAT18, ISI_D2 */
							 AT91_PIOA 19 AT91_PERIPH_B AT91_PINCTRL_NONE>; /* TWCK2 pin, conflicts with LCDDAT19, ISI_D3 */
					};
				};

				isi {
					pinctrl_isi_data_0_7: isi-0-data-0-7 {
						atmel,pins =
							<AT91_PIOA 16 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA16 periph C ISI_D0, conflicts with LCDDAT16 */
							 AT91_PIOA 17 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA17 periph C ISI_D1, conflicts with LCDDAT17 */
							 AT91_PIOA 18 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA18 periph C ISI_D2, conflicts with LCDDAT18, TWD2 */
							 AT91_PIOA 19 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA19 periph C ISI_D3, conflicts with LCDDAT19, TWCK2 */
							 AT91_PIOA 20 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA20 periph C ISI_D4, conflicts with LCDDAT20, PWMH0 */
							 AT91_PIOA 21 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA21 periph C ISI_D5, conflicts with LCDDAT21, PWML0 */
							 AT91_PIOA 22 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA22 periph C ISI_D6, conflicts with LCDDAT22, PWMH1 */
							 AT91_PIOA 23 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA23 periph C ISI_D7, conflicts with LCDDAT23, PWML1 */
							 AT91_PIOC 30 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC30 periph C ISI_PCK, conflicts with UTXD0 */
							 AT91_PIOA 31 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PA31 periph C ISI_HSYNC, conflicts with TWCK0, UTXD1 */
							 AT91_PIOA 30 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PA30 periph C ISI_VSYNC, conflicts with TWD0, URXD1 */
					};

					pinctrl_isi_data_8_9: isi-0-data-8-9 {
						atmel,pins =
							<AT91_PIOC 29 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC29 periph C ISI_PD8, conflicts with URXD0, PWMFI2 */
							 AT91_PIOC 28 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC28 periph C ISI_PD9, conflicts with SPI1_NPCS3, PWMFI0 */
					};

					pinctrl_isi_data_10_11: isi-0-data-10-11 {
						atmel,pins =
							<AT91_PIOC 27 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC27 periph C ISI_PD10, conflicts with SPI1_NPCS2, TWCK1 */
							 AT91_PIOC 26 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC26 periph C ISI_PD11, conflicts with SPI1_NPCS1, TWD1 */
					};
				};

				mmc0 {
					bootph-all;
					pinctrl_mmc0_clk_cmd_dat0: mmc0_clk_cmd_dat0 {
						bootph-all;
						atmel,pins =
							<AT91_PIOD 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD9 periph A MCI0_CK */
							 AT91_PIOD 0 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD0 periph A MCI0_CDA with pullup */
							 AT91_PIOD 1 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PD1 periph A MCI0_DA0 with pullup */
					};
					pinctrl_mmc0_dat1_3: mmc0_dat1_3 {
						bootph-all;
						atmel,pins =
							<AT91_PIOD 2 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD2 periph A MCI0_DA1 with pullup */
							 AT91_PIOD 3 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD3 periph A MCI0_DA2 with pullup */
							 AT91_PIOD 4 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PD4 periph A MCI0_DA3 with pullup */
					};
					pinctrl_mmc0_dat4_7: mmc0_dat4_7 {
						bootph-all;
						atmel,pins =
							<AT91_PIOD 5 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD5 periph A MCI0_DA4 with pullup, conflicts with TIOA0, PWMH2 */
							 AT91_PIOD 6 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD6 periph A MCI0_DA5 with pullup, conflicts with TIOB0, PWML2 */
							 AT91_PIOD 7 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PD7 periph A MCI0_DA6 with pullup, conlicts with TCLK0, PWMH3 */
							 AT91_PIOD 8 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PD8 periph A MCI0_DA7 with pullup, conflicts with PWML3 */
					};
				};

				mmc1 {
					bootph-all;
					pinctrl_mmc1_clk_cmd_dat0: mmc1_clk_cmd_dat0 {
						bootph-all;
						atmel,pins =
							<AT91_PIOB 24 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB24 periph A MCI1_CK, conflicts with GRX5 */
							 AT91_PIOB 19 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB19 periph A MCI1_CDA with pullup, conflicts with GTX4 */
							 AT91_PIOB 20 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PB20 periph A MCI1_DA0 with pullup, conflicts with GTX5 */
					};
					pinctrl_mmc1_dat1_3: mmc1_dat1_3 {
						bootph-all;
						atmel,pins =
							<AT91_PIOB 21 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB21 periph A MCI1_DA1 with pullup, conflicts with GTX6 */
							 AT91_PIOB 22 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB22 periph A MCI1_DA2 with pullup, conflicts with GTX7 */
							 AT91_PIOB 23 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PB23 periph A MCI1_DA3 with pullup, conflicts with GRX4 */
					};
				};

				nand0 {
					pinctrl_nand0_ale_cle: nand0_ale_cle-0 {
						atmel,pins =
							<AT91_PIOE 21 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PE21 periph A with pullup */
							 AT91_PIOE 22 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PE22 periph A with pullup */
					};
				};

				pwm0 {
					pinctrl_pwm0_pwmh0_0: pwm0_pwmh0-0 {
						atmel,pins =
							<AT91_PIOA 20 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with ISI_D4 and LCDDAT20 */
					};
					pinctrl_pwm0_pwmh0_1: pwm0_pwmh0-1 {
						atmel,pins =
							<AT91_PIOB 0 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GTX0 */
					};
					pinctrl_pwm0_pwml0_0: pwm0_pwml0-0 {
						atmel,pins =
							<AT91_PIOA 21 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with ISI_D5 and LCDDAT21 */
					};
					pinctrl_pwm0_pwml0_1: pwm0_pwml0-1 {
						atmel,pins =
							<AT91_PIOB 1 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GTX1 */
					};

					pinctrl_pwm0_pwmh1_0: pwm0_pwmh1-0 {
						atmel,pins =
							<AT91_PIOA 22 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with ISI_D6 and LCDDAT22 */
					};
					pinctrl_pwm0_pwmh1_1: pwm0_pwmh1-1 {
						atmel,pins =
							<AT91_PIOB 4 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GRX0 */
					};
					pinctrl_pwm0_pwmh1_2: pwm0_pwmh1-2 {
						atmel,pins =
							<AT91_PIOB 27 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* conflicts with G125CKO and RTS1 */
					};
					pinctrl_pwm0_pwml1_0: pwm0_pwml1-0 {
						atmel,pins =
							<AT91_PIOA 23 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with ISI_D7 and LCDDAT23 */
					};
					pinctrl_pwm0_pwml1_1: pwm0_pwml1-1 {
						atmel,pins =
							<AT91_PIOB 5 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GRX1 */
					};
					pinctrl_pwm0_pwml1_2: pwm0_pwml1-2 {
						atmel,pins =
							<AT91_PIOE 31 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with IRQ */
					};

					pinctrl_pwm0_pwmh2_0: pwm0_pwmh2-0 {
						atmel,pins =
							<AT91_PIOB 8 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GTXCK */
					};
					pinctrl_pwm0_pwmh2_1: pwm0_pwmh2-1 {
						atmel,pins =
							<AT91_PIOD 5 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* conflicts with MCI0_DA4 and TIOA0 */
					};
					pinctrl_pwm0_pwml2_0: pwm0_pwml2-0 {
						atmel,pins =
							<AT91_PIOB 9 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GTXEN */
					};
					pinctrl_pwm0_pwml2_1: pwm0_pwml2-1 {
						atmel,pins =
							<AT91_PIOD 6 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* conflicts with MCI0_DA5 and TIOB0 */
					};

					pinctrl_pwm0_pwmh3_0: pwm0_pwmh3-0 {
						atmel,pins =
							<AT91_PIOB 12 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GRXDV */
					};
					pinctrl_pwm0_pwmh3_1: pwm0_pwmh3-1 {
						atmel,pins =
							<AT91_PIOD 7 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* conflicts with MCI0_DA6 and TCLK0 */
					};
					pinctrl_pwm0_pwml3_0: pwm0_pwml3-0 {
						atmel,pins =
							<AT91_PIOB 13 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* conflicts with GRXER */
					};
					pinctrl_pwm0_pwml3_1: pwm0_pwml3-1 {
						atmel,pins =
							<AT91_PIOD 8 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* conflicts with MCI0_DA7 */
					};
				};

				spi0 {
					bootph-all;
					pinctrl_spi0: spi0-0 {
						bootph-all;
						atmel,pins =
							<AT91_PIOD 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD10 periph A SPI0_MISO pin */
							 AT91_PIOD 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD11 periph A SPI0_MOSI pin */
							 AT91_PIOD 12 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD12 periph A SPI0_SPCK pin */
					};
				};

				spi1 {
					bootph-all;
					pinctrl_spi1: spi1-0 {
						bootph-all;
						atmel,pins =
							<AT91_PIOC 22 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC22 periph A SPI1_MISO pin */
							 AT91_PIOC 23 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC23 periph A SPI1_MOSI pin */
							 AT91_PIOC 24 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PC24 periph A SPI1_SPCK pin */
					};
				};

				ssc0 {
					pinctrl_ssc0_tx: ssc0_tx {
						atmel,pins =
							<AT91_PIOC 16 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC16 periph A TK0 */
							 AT91_PIOC 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC17 periph A TF0 */
							 AT91_PIOC 18 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PC18 periph A TD0 */
					};

					pinctrl_ssc0_rx: ssc0_rx {
						atmel,pins =
							<AT91_PIOC 19 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC19 periph A RK0 */
							 AT91_PIOC 20 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PC20 periph A RF0 */
							 AT91_PIOC 21 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PC21 periph A RD0 */
					};
				};

				ssc1 {
					pinctrl_ssc1_tx: ssc1_tx {
						atmel,pins =
							<AT91_PIOB 2 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB2 periph B TK1, conflicts with GTX2 */
							 AT91_PIOB 3 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB3 periph B TF1, conflicts with GTX3 */
							 AT91_PIOB 6 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB6 periph B TD1, conflicts with TD1 */
					};

					pinctrl_ssc1_rx: ssc1_rx {
						atmel,pins =
							<AT91_PIOB 7 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB7 periph B RK1, conflicts with EREFCK */
							 AT91_PIOB 10 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB10 periph B RF1, conflicts with GTXER */
							 AT91_PIOB 11 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB11 periph B RD1, conflicts with GRXCK */
					};
				};

				uart0 {
					pinctrl_uart0: uart0-0 {
						atmel,pins =
							<AT91_PIOC 29 AT91_PERIPH_A AT91_PINCTRL_NONE	/* conflicts with PWMFI2, ISI_D8 */
							 AT91_PIOC 30 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* conflicts with ISI_PCK */
					};
				};

				uart1 {
					pinctrl_uart1: uart1-0 {
						atmel,pins =
							<AT91_PIOA 30 AT91_PERIPH_B AT91_PINCTRL_NONE	/* conflicts with TWD0, ISI_VSYNC */
							 AT91_PIOA 31 AT91_PERIPH_B AT91_PINCTRL_PULL_UP>;	/* conflicts with TWCK0, ISI_HSYNC */
					};
				};

				usart0 {
					pinctrl_usart0: usart0-0 {
						atmel,pins =
							<AT91_PIOD 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD17 periph A */
							 AT91_PIOD 18 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PD18 periph A with pullup */
					};

					pinctrl_usart0_rts_cts: usart0_rts_cts-0 {
						atmel,pins =
							<AT91_PIOD 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD15 periph A, conflicts with SPI0_NPCS2, CANTX0 */
							 AT91_PIOD 16 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD16 periph A, conflicts with SPI0_NPCS3, PWMFI3 */
					};
				};

				usart1 {
					pinctrl_usart1: usart1-0 {
						atmel,pins =
							<AT91_PIOB 28 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB28 periph A */
							 AT91_PIOB 29 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PB29 periph A with pullup */
					};

					pinctrl_usart1_rts_cts: usart1_rts_cts-0 {
						atmel,pins =
							<AT91_PIOB 26 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB26 periph A, conflicts with GRX7 */
							 AT91_PIOB 27 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB27 periph A, conflicts with G125CKO */
					};
				};

				usart2 {
					pinctrl_usart2: usart2-0 {
						atmel,pins =
							<AT91_PIOE 25 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PE25 periph B, conflicts with A25 */
							 AT91_PIOE 26 AT91_PERIPH_B AT91_PINCTRL_PULL_UP>;	/* PE26 periph B with pullup, conflicts NCS0 */
					};

					pinctrl_usart2_rts_cts: usart2_rts_cts-0 {
						atmel,pins =
							<AT91_PIOE 23 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PE23 periph B, conflicts with A23 */
							 AT91_PIOE 24 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PE24 periph B, conflicts with A24 */
					};
				};

				usart3 {
					pinctrl_usart3: usart3-0 {
						atmel,pins =
							<AT91_PIOE 18 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PE18 periph B, conflicts with A18 */
							 AT91_PIOE 19 AT91_PERIPH_B AT91_PINCTRL_PULL_UP>;	/* PE19 periph B with pullup, conflicts with A19 */
					};

					pinctrl_usart3_rts_cts: usart3_rts_cts-0 {
						atmel,pins =
							<AT91_PIOE 16 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PE16 periph B, conflicts with A16 */
							 AT91_PIOE 17 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PE17 periph B, conflicts with A17 */
					};
				};

				pioA: gpio@fffff200 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff200 0x100>;
					interrupts = <6 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioA_clk>;
					bootph-all;
				};

				pioB: gpio@fffff400 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff400 0x100>;
					interrupts = <7 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioB_clk>;
					bootph-all;
				};

				pioC: gpio@fffff600 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff600 0x100>;
					interrupts = <8 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioC_clk>;
					bootph-all;
				};

				pioD: gpio@fffff800 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff800 0x100>;
					interrupts = <9 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioD_clk>;
					bootph-all;
				};

				pioE: gpio@fffffa00 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffffa00 0x100>;
					interrupts = <10 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioE_clk>;
					bootph-all;
				};
			};

			pmc: pmc@fffffc00 {
				compatible = "atmel,sama5d3-pmc", "syscon";
				reg = <0xfffffc00 0x120>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				interrupt-controller;
				#address-cells = <1>;
				#size-cells = <0>;
				#interrupt-cells = <1>;
				bootph-all;

				main_rc_osc: main_rc_osc {
					compatible = "atmel,at91sam9x5-clk-main-rc-osc";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_MOSCRCS>;
					clock-frequency = <12000000>;
					clock-accuracy = <50000000>;
				};

				main_osc: main_osc {
					compatible = "atmel,at91rm9200-clk-main-osc";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_MOSCS>;
					clocks = <&main_xtal>;
				};

				main: mainck {
					compatible = "atmel,at91sam9x5-clk-main";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_MOSCSELS>;
					clocks = <&main_rc_osc &main_osc>;
				};

				plla: pllack@0 {
					compatible = "atmel,sama5d3-clk-pll";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_LOCKA>;
					clocks = <&main>;
					reg = <0>;
					atmel,clk-input-range = <8000000 50000000>;
					#atmel,pll-clk-output-range-cells = <4>;
					atmel,pll-clk-output-ranges = <400000000 1000000000 0 0>;
				};

				plladiv: plladivck {
					compatible = "atmel,at91sam9x5-clk-plldiv";
					#clock-cells = <0>;
					clocks = <&plla>;
				};

				utmi: utmick {
					compatible = "atmel,at91sam9x5-clk-utmi";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_LOCKU>;
					clocks = <&main>;
					regmap-sfr = <&sfr>;
					bootph-all;
				};

				mck: masterck {
					compatible = "atmel,at91sam9x5-clk-master";
					#clock-cells = <0>;
					interrupt-parent = <&pmc>;
					interrupts = <AT91_PMC_MCKRDY>;
					clocks = <&clk32k>, <&main>, <&plladiv>, <&utmi>;
					atmel,clk-output-range = <0 166000000>;
					atmel,clk-divisors = <1 2 4 3>;
					bootph-all;
				};

				usb: usbck {
					compatible = "atmel,at91sam9x5-clk-usb";
					#clock-cells = <0>;
					clocks = <&plladiv>, <&utmi>;
				};

				prog: progck {
					compatible = "atmel,at91sam9x5-clk-programmable";
					#address-cells = <1>;
					#size-cells = <0>;
					interrupt-parent = <&pmc>;
					clocks = <&clk32k>, <&main>, <&plladiv>, <&utmi>, <&mck>;

					prog0: progck@0 {
						#clock-cells = <0>;
						reg = <0>;
						interrupts = <AT91_PMC_PCKRDY(0)>;
					};

					prog1: progck@1 {
						#clock-cells = <0>;
						reg = <1>;
						interrupts = <AT91_PMC_PCKRDY(1)>;
					};

					prog2: progck@2 {
						#clock-cells = <0>;
						reg = <2>;
						interrupts = <AT91_PMC_PCKRDY(2)>;
					};
				};

				smd: smdclk {
					compatible = "atmel,at91sam9x5-clk-smd";
					#clock-cells = <0>;
					clocks = <&plladiv>, <&utmi>;
				};

				systemck {
					compatible = "atmel,at91rm9200-clk-system";
					#address-cells = <1>;
					#size-cells = <0>;

					ddrck: ddrck@2 {
						#clock-cells = <0>;
						reg = <2>;
						clocks = <&mck>;
					};

					smdck: smdck@4 {
						#clock-cells = <0>;
						reg = <4>;
						clocks = <&smd>;
					};

					uhpck: uhpck@6 {
						#clock-cells = <0>;
						reg = <6>;
						clocks = <&usb>;
					};

					udpck: udpck@7 {
						#clock-cells = <0>;
						reg = <7>;
						clocks = <&usb>;
					};

					pck0: pck@8 {
						#clock-cells = <0>;
						reg = <8>;
						clocks = <&prog0>;
					};

					pck1: pck@9 {
						#clock-cells = <0>;
						reg = <9>;
						clocks = <&prog1>;
					};

					pck2: pck@10 {
						#clock-cells = <0>;
						reg = <10>;
						clocks = <&prog2>;
					};
				};

				periphck {
					compatible = "atmel,at91sam9x5-clk-peripheral";
					#address-cells = <1>;
					#size-cells = <0>;
					clocks = <&mck>;
					bootph-all;

					dbgu_clk: dbgu_clk@2 {
						bootph-all;
						#clock-cells = <0>;
						reg = <2>;
					};

					hsmc_clk: hsmc_clk@5 {
						#clock-cells = <0>;
						reg = <5>;
					};

					pioA_clk: pioA_clk@6 {
						bootph-all;
						#clock-cells = <0>;
						reg = <6>;
					};

					pioB_clk: pioB_clk@7 {
						bootph-all;
						#clock-cells = <0>;
						reg = <7>;
					};

					pioC_clk: pioC_clk@8 {
						bootph-all;
						#clock-cells = <0>;
						reg = <8>;
					};

					pioD_clk: pioD_clk@9 {
						bootph-all;
						#clock-cells = <0>;
						reg = <9>;
					};

					pioE_clk: pioE_clk@10 {
						bootph-all;
						#clock-cells = <0>;
						reg = <10>;
					};

					usart0_clk: usart0_clk@12 {
						#clock-cells = <0>;
						reg = <12>;
						atmel,clk-output-range = <0 66000000>;
					};

					usart1_clk: usart1_clk@13 {
						#clock-cells = <0>;
						reg = <13>;
						atmel,clk-output-range = <0 66000000>;
					};

					usart2_clk: usart2_clk@14 {
						#clock-cells = <0>;
						reg = <14>;
						atmel,clk-output-range = <0 66000000>;
					};

					usart3_clk: usart3_clk@15 {
						#clock-cells = <0>;
						reg = <15>;
						atmel,clk-output-range = <0 66000000>;
					};

					uart0_clk: uart0_clk@16 {
						#clock-cells = <0>;
						reg = <16>;
						atmel,clk-output-range = <0 66000000>;
					};

					twi0_clk: twi0_clk@18 {
						reg = <18>;
						#clock-cells = <0>;
						atmel,clk-output-range = <0 16625000>;
					};

					twi1_clk: twi1_clk@19 {
						#clock-cells = <0>;
						reg = <19>;
						atmel,clk-output-range = <0 16625000>;
					};

					twi2_clk: twi2_clk@20 {
						#clock-cells = <0>;
						reg = <20>;
						atmel,clk-output-range = <0 16625000>;
					};

					mci0_clk: mci0_clk@21 {
						bootph-all;
						#clock-cells = <0>;
						reg = <21>;
					};

					mci1_clk: mci1_clk@22 {
						bootph-all;
						#clock-cells = <0>;
						reg = <22>;
					};

					spi0_clk: spi0_clk@24 {
						bootph-all;
						#clock-cells = <0>;
						reg = <24>;
						atmel,clk-output-range = <0 133000000>;
					};

					spi1_clk: spi1_clk@25 {
						bootph-all;
						#clock-cells = <0>;
						reg = <25>;
						atmel,clk-output-range = <0 133000000>;
					};

					tcb0_clk: tcb0_clk@26 {
						#clock-cells = <0>;
						reg = <26>;
						atmel,clk-output-range = <0 133000000>;
					};

					pwm_clk: pwm_clk@28 {
						#clock-cells = <0>;
						reg = <28>;
					};

					adc_clk: adc_clk@29 {
						#clock-cells = <0>;
						reg = <29>;
						atmel,clk-output-range = <0 66000000>;
					};

					dma0_clk: dma0_clk@30 {
						#clock-cells = <0>;
						reg = <30>;
					};

					dma1_clk: dma1_clk@31 {
						#clock-cells = <0>;
						reg = <31>;
					};

					uhphs_clk: uhphs_clk@32 {
						#clock-cells = <0>;
						reg = <32>;
					};

					udphs_clk: udphs_clk@33 {
						#clock-cells = <0>;
						reg = <33>;
					};

					isi_clk: isi_clk@37 {
						#clock-cells = <0>;
						reg = <37>;
					};

					ssc0_clk: ssc0_clk@38 {
						#clock-cells = <0>;
						reg = <38>;
						atmel,clk-output-range = <0 66000000>;
					};

					ssc1_clk: ssc1_clk@39 {
						#clock-cells = <0>;
						reg = <39>;
						atmel,clk-output-range = <0 66000000>;
					};

					sha_clk: sha_clk@42 {
						#clock-cells = <0>;
						reg = <42>;
					};

					aes_clk: aes_clk@43 {
						#clock-cells = <0>;
						reg = <43>;
					};

					tdes_clk: tdes_clk@44 {
						#clock-cells = <0>;
						reg = <44>;
					};

					trng_clk: trng_clk@45 {
						#clock-cells = <0>;
						reg = <45>;
					};

					fuse_clk: fuse_clk@48 {
						#clock-cells = <0>;
						reg = <48>;
					};

					mpddr_clk: mpddr_clk@49 {
						#clock-cells = <0>;
						reg = <49>;
					};
				};
			};

			rstc@fffffe00 {
				compatible = "atmel,sama5d3-rstc", "atmel,at91sam9g45-rstc";
				reg = <0xfffffe00 0x10>;
				clocks = <&clk32k>;
			};

			shutdown-controller@fffffe10 {
				compatible = "atmel,at91sam9x5-shdwc";
				reg = <0xfffffe10 0x10>;
				clocks = <&clk32k>;
			};

			pit: timer@fffffe30 {
				compatible = "atmel,at91sam9260-pit";
				reg = <0xfffffe30 0xf>;
				interrupts = <3 IRQ_TYPE_LEVEL_HIGH 5>;
				clocks = <&mck>;
				bootph-all;
			};

			watchdog@fffffe40 {
				compatible = "atmel,at91sam9260-wdt";
				reg = <0xfffffe40 0x10>;
				interrupts = <4 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&clk32k>;
				atmel,watchdog-type = "hardware";
				atmel,reset-type = "all";
				atmel,dbg-halt;
				status = "disabled";
			};

			sckc@fffffe50 {
				compatible = "atmel,at91sam9x5-sckc";
				reg = <0xfffffe50 0x4>;

				slow_rc_osc: slow_rc_osc {
					compatible = "atmel,at91sam9x5-clk-slow-rc-osc";
					#clock-cells = <0>;
					clock-frequency = <32768>;
					clock-accuracy = <50000000>;
					atmel,startup-time-usec = <75>;
				};

				slow_osc: slow_osc {
					compatible = "atmel,at91sam9x5-clk-slow-osc";
					#clock-cells = <0>;
					clocks = <&slow_xtal>;
					atmel,startup-time-usec = <1200000>;
				};

				clk32k: slowck {
					compatible = "atmel,at91sam9x5-clk-slow";
					#clock-cells = <0>;
					clocks = <&slow_rc_osc &slow_osc>;
				};
			};

			rtc@fffffeb0 {
				compatible = "atmel,at91rm9200-rtc";
				reg = <0xfffffeb0 0x30>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&clk32k>;
			};
		};

		usb0: gadget@00500000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "atmel,sama5d3-udc";
			reg = <0x00500000 0x100000
			       0xf8030000 0x4000>;
			interrupts = <33 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&udphs_clk>, <&utmi>;
			clock-names = "pclk", "hclk";
			status = "disabled";

			ep0: endpoint@0 {
				reg = <0>;
				atmel,fifo-size = <64>;
				atmel,nb-banks = <1>;
			};

			ep1: endpoint@1 {
				reg = <1>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <3>;
				atmel,can-dma;
				atmel,can-isoc;
			};

			ep2: endpoint@2 {
				reg = <2>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <3>;
				atmel,can-dma;
				atmel,can-isoc;
			};

			ep3: endpoint@3 {
				reg = <3>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
				atmel,can-dma;
			};

			ep4: endpoint@4 {
				reg = <4>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
				atmel,can-dma;
			};

			ep5: endpoint@5 {
				reg = <5>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
				atmel,can-dma;
			};

			ep6: endpoint@6 {
				reg = <6>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
				atmel,can-dma;
			};

			ep7i: endpoint@7 {
				reg = <7>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
				atmel,can-dma;
			};

			ep8: endpoint@8 {
				reg = <8>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep9: endpoint@9 {
				reg = <9>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep10: endpoint@a {
				reg = <10>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep11: endpoint@b {
				reg = <11>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep12: endpoint@c {
				reg = <12>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep13: endpoint@d {
				reg = <13>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep14: endpoint@e {
				reg = <14>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};

			ep15: endpoint@f {
				reg = <15>;
				atmel,fifo-size = <1024>;
				atmel,nb-banks = <2>;
			};
		};

		usb1: ohci@00600000 {
			compatible = "atmel,at91rm9200-ohci", "usb-ohci";
			reg = <0x00600000 0x100000>;
			interrupts = <32 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&uhphs_clk>, <&uhphs_clk>, <&uhpck>;
			clock-names = "ohci_clk", "hclk", "uhpck";
			status = "disabled";
		};

		usb2: ehci@00700000 {
			compatible = "atmel,at91sam9g45-ehci", "usb-ehci";
			reg = <0x00700000 0x100000>;
			interrupts = <32 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&utmi>, <&uhphs_clk>;
			clock-names = "usb_clk", "ehci_clk";
			status = "disabled";
		};

		nand0: nand@60000000 {
			compatible = "atmel,at91rm9200-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			reg = <	0x60000000 0x01000000	/* EBI CS3 */
				0xffffc070 0x00000490	/* SMC PMECC regs */
				0xffffc500 0x00000100	/* SMC PMECC Error Location regs */
				0x00110000 0x00018000	/* ROM code */
				>;
			interrupts = <5 IRQ_TYPE_LEVEL_HIGH 6>;
			atmel,nand-addr-offset = <21>;
			atmel,nand-cmd-offset = <22>;
			atmel,nand-has-dma;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand0_ale_cle>;
			atmel,pmecc-lookup-table-offset = <0x0 0x8000>;
			status = "disabled";

			nfc@70000000 {
				compatible = "atmel,sama5d3-nfc";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <
					0x70000000 0x08000000	/* NFC Command Registers */
					0xffffc000 0x00000070	/* NFC HSMC regs */
					0x00200000 0x00100000	/* NFC SRAM banks */
					>;
				clocks = <&hsmc_clk>;
			};
		};
	};

	onewire_tm: onewire {
		compatible = "w1-gpio";
		status = "disabled";
	};
};
