// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2017 Antony Antony <antony@phenome.org>
// Copyright (C) 2016 ARM Ltd.

/dts-v1/;
#include "sun50i-h5.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/pinctrl/sun4i-a10.h>

/ {
	model = "FriendlyARM NanoPi NEO Plus2";
	compatible = "friendlyarm,nanopi-neo-plus2", "allwinner,sun50i-h5";

	aliases {
		ethernet0 = &emac;
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "nanopi:green:pwr";
			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led-1 {
			label = "nanopi:red:status";
			gpios = <&pio 0 20 GPIO_ACTIVE_HIGH>;
		};
	};

	reg_gmac_3v3: gmac-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "gmac-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <100000>;
		enable-active-high;
		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
		vin-supply = <&reg_vcc3v3>;
	};

	reg_gmac_2v5: gmac-2v5 {
		/* 2V5 supply for GMAC PHY IO */
		compatible = "regulator-fixed";
		regulator-name = "gmac-2v5";
		regulator-min-microvolt = <2500000>;
		regulator-max-microvolt = <2500000>;
		regulator-always-on;
		vin-supply = <&reg_vcc3v3>;
	};

	reg_vcc5v: regulator-vcc5v {
		/* board 5V supply from micro USB or pin headers */
		compatible = "regulator-fixed";
		regulator-name = "vcc-5v";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
	};

	reg_vcc3v3: vcc3v3 {
		/* board 3V3 supply by SY8089A */
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		vin-supply = <&reg_vcc5v>;
	};

	vdd_cpux: gpio-regulator {
		/* cpu voltage regulator MP2143DJ */
		compatible = "regulator-gpio";
		regulator-name = "vdd-cpux";
		regulator-type = "voltage";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1300000>;
		regulator-ramp-delay = <50>; /* 4ms */
		gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>;
		gpios-states = <0x1>;
		states = <1100000 0>, <1300000 1>;
		vin-supply = <&reg_vcc5v>;
	};

	wifi_pwrseq: pwrseq {
		compatible = "mmc-pwrseq-simple";
		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
		post-power-on-delay-ms = <200>;
	};
};

&codec {
	allwinner,audio-routing =
		"Line Out", "LINEOUT",
		"MIC1", "Mic",
		"Mic",  "MBIAS";
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci3 {
	status = "okay";
};

&emac {
	pinctrl-names = "default";
	pinctrl-0 = <&emac_rgmii_pins>;
	phy-supply = <&reg_gmac_3v3>;
	phy-handle = <&ext_rgmii_phy>;
	phy-mode = "rgmii-id";
	status = "okay";
};

&external_mdio {
	ext_rgmii_phy: ethernet-phy@7 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <7>;
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
	disable-wp;
	status = "okay";
};

&mmc1 {
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc3v3>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	brcmf: wifi@1 {
		reg = <1>;
		compatible = "brcm,bcm4329-fmac";
	};
};

&mmc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc2_8bit_pins>;
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <8>;
	non-removable;
	cap-mmc-hw-reset;
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci3 {
	status = "okay";
};

&pio {
	vcc-pa-supply = <&reg_vcc3v3>;
	vcc-pc-supply = <&reg_vcc3v3>;
	vcc-pd-supply = <&reg_gmac_2v5>;
	vcc-pf-supply = <&reg_vcc3v3>;
	vcc-pg-supply = <&reg_vcc3v3>;
};

&r_pio {
	vcc-pl-supply = <&reg_vcc3v3>;
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pa_pins>;
	status = "okay";
};

&usb_otg {
	dr_mode = "host";
	status = "okay";
};

&usbphy {
	/* USB Type-A ports' VBUS is always on */
	status = "okay";
};
