// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2015 Phytec Messtechnik GmbH
 * Author: Teresa Remmet <t.remmet@phytec.de>
 */

/ {
	model = "Phytec AM335x phyBOARD-WEGA";
	compatible = "phytec,am335x-wega", "phytec,am335x-phycore-som", "ti,am33xx";

	sound: sound_iface {
		compatible = "ti,da830-evm-audio";
	};

	vcc3v3: fixedregulator1 {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
	};
};

/* Audio */
&am33xx_pinmux {
	mcasp0_pins: pinmux_mcasp0 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_MCASP0_AHCLKX, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_ACLKX, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_FSX, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_AXR0, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_AXR1, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
		>;
	};
};

&i2c0 {
	tlv320aic3007: tlv320aic3007@18 {
		compatible = "ti,tlv320aic3007";
		reg = <0x18>;
		AVDD-supply = <&vcc3v3>;
		IOVDD-supply = <&vcc3v3>;
		DRVDD-supply = <&vcc3v3>;
		DVDD-supply = <&vdig1_reg>;
		status = "okay";
	};
};

&mcasp0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mcasp0_pins>;
	op-mode = <0>; /* DAVINCI_MCASP_IIS_MODE */
	tdm-slots = <2>;
	serial-dir = <
		2 1 0 0 /* # 0: INACTIVE, 1: TX, 2: RX */
	>;
	tx-num-evt = <16>;
	rt-num-evt = <16>;
	status = "okay";
};

&sound {
	ti,model = "AM335x-Wega";
	ti,audio-codec = <&tlv320aic3007>;
	ti,mcasp-controller = <&mcasp0>;
	ti,audio-routing =
		"Line Out",		"LLOUT",
		"Line Out",		"RLOUT",
		"LINE1L",		"Line In",
		"LINE1R",		"Line In";
	clocks = <&mcasp0_fck>;
	clock-names = "mclk";
	status = "okay";
};

/* CAN Busses */
&am33xx_pinmux {
	dcan1_pins: pinmux_dcan1 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART0_CTSN, PIN_OUTPUT_PULLUP, MUX_MODE2) /* uart0_ctsn.d_can1_tx */
			AM33XX_PADCONF(AM335X_PIN_UART0_RTSN, PIN_INPUT_PULLUP, MUX_MODE2) /* uart0_rtsn.d_can1_rx */
		>;
	};
};

&dcan1 {
	pinctrl-names = "default";
	pinctrl-0 = <&dcan1_pins>;
	status = "okay";
};

/* Ethernet */
&am33xx_pinmux {
	ethernet1_pins: pinmux_ethernet1 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_A0, PIN_OUTPUT, MUX_MODE1)		/* gpmc_a0.mii2_txen */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A1, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a1.mii2_rxdv */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A2, PIN_OUTPUT, MUX_MODE1)		/* gpmc_a2.mii2_txd3 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A3, PIN_OUTPUT, MUX_MODE1)		/* gpmc_a3.mii2_txd2 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A4, PIN_OUTPUT, MUX_MODE1)		/* gpmc_a4.mii2_txd1 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A5, PIN_OUTPUT, MUX_MODE1)		/* gpmc_a5.mii2_txd0 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A6, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a6.mii2_txclk */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A7, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a7.mii2_rxclk */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A8, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a8.mii2_rxd3 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A9, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a9.mii2_rxd2 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A10, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a10.mii2_rxd1 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_A11, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_a11.mii2_rxd0 */
			AM33XX_PADCONF(AM335X_PIN_GPMC_WPN, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_wpn.mii2_rxerr */
			AM33XX_PADCONF(AM335X_PIN_GPMC_BEN1, PIN_INPUT_PULLDOWN, MUX_MODE1)	/* gpmc_ben1.mii2_col */
		>;
	};
};

&cpsw_emac1 {
	phy-handle = <&phy1>;
	phy-mode = "mii";
	dual_emac_res_vlan = <2>;
};

&davinci_mdio {
	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&mac {
	slaves = <2>;
	pinctrl-names = "default";
	pinctrl-0 = <&ethernet0_pins &ethernet1_pins>;
	dual_emac = <1>;
};

/* MMC */
&am33xx_pinmux {
	mmc1_pins: pinmux_mmc1 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_MMC0_DAT3, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MMC0_DAT2, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MMC0_DAT1, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MMC0_DAT0, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MMC0_CLK, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MMC0_CMD, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_SPI0_CS1, PIN_INPUT_PULLUP, MUX_MODE7)	/* spi0_cs1.mmc0_sdcd */
		>;
	};
};

&mmc1 {
	vmmc-supply = <&vcc3v3>;
	bus-width = <4>;
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	cd-gpios = <&gpio0 6 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

/* Power */
&vdig1_reg {
	regulator-boot-on;
	regulator-always-on;
};

/* UARTs */
&am33xx_pinmux {
	uart0_pins: pinmux_uart0 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART0_RXD, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART0_TXD, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
		>;
	};

	uart1_pins: pinmux_uart1_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART1_RXD, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_TXD, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_CTSN, PIN_INPUT, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_RTSN, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
		>;
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;
	status = "okay";
};

/* USB */
&cppi41dma {
	status = "okay";
};

&usb_ctrl_mod {
	status = "okay";
};

&usb {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb0_phy {
	status = "okay";
};

&usb1 {
	dr_mode = "host";
	status = "okay";
};

&usb1_phy {
	status = "okay";
};
