// SPDX-License-Identifier: GPL-2.0+
/*
 * Copyright (C) 2017 Álvaro Fernández Rojas <noltari@gmail.com>
 */

#include <dt-bindings/clock/bcm6358-clock.h>
#include <dt-bindings/dma/bcm6358-dma.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/reset/bcm6358-reset.h>
#include "skeleton.dtsi"

/ {
	compatible = "brcm,bcm6358";

	aliases {
		spi0 = &spi;
	};

	cpus {
		reg = <0xfffe0000 0x4>;
		#address-cells = <1>;
		#size-cells = <0>;
		bootph-all;

		cpu@0 {
			compatible = "brcm,bcm6358-cpu", "mips,mips4Kc";
			device_type = "cpu";
			reg = <0>;
			bootph-all;
		};

		cpu@1 {
			compatible = "brcm,bcm6358-cpu", "mips,mips4Kc";
			device_type = "cpu";
			reg = <1>;
			bootph-all;
		};
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		bootph-all;

		periph_osc: periph-osc {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <50000000>;
			bootph-all;
		};

		periph_clk: periph-clk {
			compatible = "brcm,bcm6345-clk";
			reg = <0xfffe0004 0x4>;
			#clock-cells = <1>;
		};
	};

	pflash: nor@1e000000 {
		compatible = "cfi-flash";
		reg = <0x1e000000 0x2000000>;
		bank-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		status = "disabled";
	};

	ubus {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		bootph-all;

		pll_cntl: syscon@fffe0008 {
			compatible = "syscon";
			reg = <0xfffe0008 0x4>;
		};

		syscon-reboot {
			compatible = "syscon-reboot";
			regmap = <&pll_cntl>;
			offset = <0x0>;
			mask = <0x1>;
		};

		periph_rst: reset-controller@fffe0034 {
			compatible = "brcm,bcm6345-reset";
			reg = <0xfffe0034 0x4>;
			#reset-cells = <1>;
		};

		wdt: watchdog@fffe005c {
			compatible = "brcm,bcm6345-wdt";
			reg = <0xfffe005c 0xc>;
			clocks = <&periph_osc>;
		};

		wdt-reboot {
			compatible = "wdt-reboot";
			wdt = <&wdt>;
		};

		gpio1: gpio-controller@fffe0080 {
			compatible = "brcm,bcm6345-gpio";
			reg = <0xfffe0080 0x4>, <0xfffe0088 0x4>;
			gpio-controller;
			#gpio-cells = <2>;
			ngpios = <8>;

			status = "disabled";
		};

		gpio0: gpio-controller@fffe0084 {
			compatible = "brcm,bcm6345-gpio";
			reg = <0xfffe0084 0x4>, <0xfffe008c 0x4>;
			gpio-controller;
			#gpio-cells = <2>;

			status = "disabled";
		};

		leds: led-controller@fffe00d0 {
			compatible = "brcm,bcm6358-leds";
			reg = <0xfffe00d0 0x8>;
			#address-cells = <1>;
			#size-cells = <0>;

			status = "disabled";
		};

		uart0: serial@fffe0100 {
			compatible = "brcm,bcm6345-uart";
			reg = <0xfffe0100 0x18>;
			clocks = <&periph_osc>;

			status = "disabled";
		};

		uart1: serial@fffe0120 {
			compatible = "brcm,bcm6345-uart";
			reg = <0xfffe0120 0x18>;
			clocks = <&periph_osc>;

			status = "disabled";
		};

		spi: spi@fffe0800 {
			compatible = "brcm,bcm6358-spi";
			reg = <0xfffe0800 0x70c>;
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&periph_clk BCM6358_CLK_SPI>;
			resets = <&periph_rst BCM6358_RST_SPI>;
			spi-max-frequency = <20000000>;
			num-cs = <4>;

			status = "disabled";
		};

		memory-controller@fffe1200 {
			compatible = "brcm,bcm6358-mc";
			reg = <0xfffe1200 0x4c>;
			bootph-all;
		};

		ehci: usb-controller@fffe1300 {
			compatible = "brcm,bcm6358-ehci", "generic-ehci";
			reg = <0xfffe1300 0x100>;
			phys = <&usbh>;
			big-endian;

			status = "disabled";
		};

		ohci: usb-controller@fffe1400 {
			compatible = "brcm,bcm6358-ohci", "generic-ohci";
			reg = <0xfffe1400 0x100>;
			phys = <&usbh>;
			big-endian;

			status = "disabled";
		};

		usbh: usb-phy@fffe1500 {
			compatible = "brcm,bcm6358-usbh";
			reg = <0xfffe1500 0x28>;
			#phy-cells = <0>;
			resets = <&periph_rst BCM6358_RST_USBH>;

			status = "disabled";
		};

		enet0: ethernet@fffe4000 {
			compatible = "brcm,bcm6348-enet";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xfffe4000 0x2dc>;
			clocks = <&periph_clk BCM6358_CLK_ENET0>;
			dmas = <&iudma BCM6358_DMA_ENET0_RX>,
			       <&iudma BCM6358_DMA_ENET0_TX>;
			dma-names = "rx",
				    "tx";

			status = "disabled";
		};

		enet1: ethernet@fffe4800 {
			compatible = "brcm,bcm6348-enet";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xfffe4800 0x2dc>;
			clocks = <&periph_clk BCM6358_CLK_ENET1>;
			dmas = <&iudma BCM6358_DMA_ENET1_RX>,
			       <&iudma BCM6358_DMA_ENET1_TX>;
			dma-names = "rx",
				    "tx";

			status = "disabled";
		};

		iudma: dma-controller@fffe5000 {
			compatible = "brcm,bcm6348-iudma";
			reg = <0xfffe5000 0x24>,
			      <0xfffe5100 0x80>,
			      <0xfffe5200 0x80>;
			reg-names = "dma",
				    "dma-channels",
				    "dma-sram";
			#dma-cells = <1>;
			dma-channels = <8>;
			clocks = <&periph_clk BCM6358_CLK_EMUSB>,
				 <&periph_clk BCM6358_CLK_USBSU>,
				 <&periph_clk BCM6358_CLK_EPHY>;
			resets = <&periph_rst BCM6358_RST_ENET>,
				 <&periph_rst BCM6358_RST_EPHY>;
		};
	};
};
