// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/*
 * Copyright (c) Toradex
 *
 * https://www.toradex.com/computer-on-modules/aquila-arm-family/nxp-imx95
 */

#include <dt-bindings/net/ti-dp83867.h>
#include "imx95.dtsi"

/ {
	aliases {
		can0 = &flexcan1;
		can1 = &flexcan2;
		can2 = &flexcan3;
		can3 = &flexcan4;
		eeprom0 = &som_eeprom;
		ethernet0 = &enetc_port0;
		i2c0 = &lpi2c3;
		i2c1 = &lpi2c2;
		i2c2 = &i3c2;
		i2c3 = &lpi2c8;
		i2c4 = &lpi2c4;
		i2c6 = &lpi2c5;
		mmc0 = &usdhc1;
		mmc1 = &usdhc2;
		rtc0 = &rtc_i2c;
		rtc1 = &scmi_bbm;
		serial0 = &lpuart3;
		serial1 = &lpuart7;
		serial2 = &lpuart1;
		serial3 = &lpuart2;
		usb0 = &usb3;
		usb1 = &usb2;
	};

	chosen {
		stdout-path = "serial2:115200n8";
	};

	aquila_key_wake: gpio-key-wakeup {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ctrl_wake1_mico>;

		status = "disabled";

		key-wakeup {
			/* Aquila CTRL_WAKE1_MICO# */
			gpios = <&gpio5 11 GPIO_ACTIVE_LOW>;
			label = "Wake Up";
			wakeup-source;
			linux,code = <KEY_WAKEUP>;
		};
	};

	clk_dsi2dp_refclk: clock-dsi2dp-refclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <27000000>;
	};

	clk_dsi2dp_refclk_en: clock-dsi2dp-refclk-en {
		compatible = "gpio-gate-clock";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_ctrl_dp_clk_en>;
		clocks = <&clk_dsi2dp_refclk>;
		#clock-cells = <0>;
		/* CTRL_DP_CLK_EN */
		enable-gpios = <&gpio1 11 GPIO_ACTIVE_HIGH>;
	};

	clk_serdes_eth_ref: clock-serdes-eth-ref {
		compatible = "gpio-gate-clock";
		#clock-cells = <0>;
		/* CTRL_ETH_REF_CLK_STBY */
		enable-gpios = <&som_gpio_expander_0 6 GPIO_ACTIVE_LOW>;
	};

	reg_1p8v: regulator-1p8v {
		compatible = "regulator-fixed";
		regulator-max-microvolt = <1800000>;
		regulator-min-microvolt = <1800000>;
		regulator-name = "On-module +V1.8";
	};

	reg_dp_1p2v: regulator-dp-1p2v {
		compatible = "regulator-fixed";
		/* CTRL_DP_BRIDGE_EN */
		gpios = <&som_gpio_expander_0 7 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-always-on;
		regulator-max-microvolt = <1200000>;
		regulator-min-microvolt = <1200000>;
		regulator-name = "On-module +V1.2_DP";
		vin-supply = <&reg_1p8v>;
	};

	reg_usb1_vbus: regulator-usb1-vbus {
		compatible = "regulator-fixed";
		/* Aquila USB_1_EN */
		gpios = <&som_gpio_expander_0 2 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-name = "USB_1_EN";
	};

	reg_usb2_vbus: regulator-usb2-vbus {
		compatible = "regulator-fixed";
		/* Aquila USB_2_EN */
		gpios = <&som_gpio_expander_0 3 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-name = "USB_2_H_EN";
	};

	reg_usdhc2_vmmc: regulator-usdhc2-vmmc {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_sd1_pwr_en>;
		/* Aquila SD_1_PWR_EN */
		gpios = <&gpio3 7 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		off-on-delay-us = <100000>;
		regulator-max-microvolt = <3300000>;
		regulator-min-microvolt = <3300000>;
		regulator-name = "SD_1_PWR_EN";
		startup-delay-us = <20000>;
	};

	reg_usdhc2_vqmmc: regulator-usdhc2-vqmmc {
		compatible = "regulator-gpio";
		/* PMIC_SD_1_VSEL */
		gpios = <&som_gpio_expander_1 9 GPIO_ACTIVE_HIGH>;
		regulator-max-microvolt = <3300000>;
		regulator-min-microvolt = <1800000>;
		regulator-name = "PMIC_SD_1_VSEL";
		states = <1800000 0x1>,
			 <3300000 0x0>;
	};

	remoteproc-cm7 {
		compatible = "fsl,imx95-cm7";
		mboxes = <&mu7 0 1 &mu7 1 1 &mu7 3 1>;
		mbox-names = "tx", "rx", "rxdb";
		memory-region = <&vdevbuffer>, <&vdev0vring0>, <&vdev0vring1>,
				<&vdev1vring0>, <&vdev1vring1>, <&rsc_table>, <&m7_reserved>;
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		linux_cma: linux,cma {
			compatible = "shared-dma-pool";
			reusable;
			size = <0 0x3c000000>;
			alloc-ranges = <0 0x80000000 0 0x7f000000>;
			linux,cma-default;
		};

		m7_reserved: memory@80000000 {
			reg = <0 0x80000000 0 0x1000000>;
			no-map;
		};

		rsc_table: rsc-table@88220000 {
			reg = <0 0x88220000 0 0x1000>;
			no-map;
		};

		vdev0vring0: vdev0vring0@88000000 {
			reg = <0 0x88000000 0 0x8000>;
			no-map;
		};

		vdev0vring1: vdev0vring1@88008000 {
			reg = <0 0x88008000 0 0x8000>;
			no-map;
		};

		vdev1vring0: vdev1vring0@88010000 {
			reg = <0 0x88010000 0 0x8000>;
			no-map;
		};

		vdev1vring1: vdev1vring1@88018000 {
			reg = <0 0x88018000 0 0x8000>;
			no-map;
		};

		vdevbuffer: vdevbuffer@88020000 {
			compatible = "shared-dma-pool";
			reg = <0 0x88020000 0 0x100000>;
			no-map;
		};
	};
};

/* Aquila ADC_[1-4] */
&adc1 {
	vref-supply = <&reg_1p8v>;
};

/* Aquila ETH_1 */
&enetc_port0 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enetc0>;
	phy-handle = <&ethphy1>;
	phy-mode = "rgmii-id";
};

/* Aquila CAN_1 */
&flexcan1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan1>;
};

/* Aquila CAN_2 */
&flexcan2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan2>;
};

/* Aquila CAN_3 */
&flexcan3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan3>;
};

/* Aquila CAN_4 */
&flexcan4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan4>;
};

/* Aquila QSPI_1 */
&flexspi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexspi1_8bit>,
		    <&pinctrl_qspi_cs1>;
};

&gpio1 {
	gpio-line-names = "", /* 0 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "AQUILA_C24", /* 10 */
			  "",
			  "AQUILA_B17",
			  "CTRL_GPIO_EXP_INT#",
			  "AQUILA_B18";

	status = "okay";
};

&gpio2 {
	gpio-line-names = "", /* 0 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "AQUILA_B42",
			  "",
			  "AQUILA_B43";
};

&gpio3 {
	gpio-line-names = "", /* 0 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "", /* 10 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "AQUILA_A11",
			  "", /* 20 */
			  "AQUILA_B57",
			  "AQUILA_B19";
};

&gpio4 {
	gpio-line-names = "", /* 0 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "", /* 10 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "AQUILA_C22",
			  "AQUILA_C21",
			  "AQUILA_C20",
			  "", /* 20 */
			  "",
			  "",
			  "AQUILA_C23",
			  "AQUILA_D23",
			  "AQUILA_D24",
			  "",
			  "AQUILA_D25";
};

&gpio5 {
	gpio-line-names = "", /* 0 */
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "",
			  "", /* 10 */
			  "",
			  "",
			  "AQUILA_B44",
			  "AQUILA_B45";
};

/* Aquila I2C_2 */
&i3c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i3c2>;
	i2c-scl-hz = <100000>;
};

/* Aquila I2C_1 */
&lpi2c2 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_lpi2c2>;
	pinctrl-1 = <&pinctrl_lpi2c2_gpio>;
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <100000>;
	scl-gpios = <&gpio1 2 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio1 3 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

/* On-module I2C - I2C_SOM */
&lpi2c3 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_lpi2c3>, <&pinctrl_ctrl_gpio_exp_int>;
	pinctrl-1 = <&pinctrl_lpi2c3_gpio>, <&pinctrl_ctrl_gpio_exp_int>;
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <400000>;
	scl-gpios = <&gpio2 29 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio2 28 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;

	status = "okay";

	som_gpio_expander_0: gpio@20 {
		compatible = "nxp,pcal6408";
		reg = <0x20>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-line-names =
			"AQUILA_C38", /* 0 */
			"PCIE_2_RESET#",
			"AQUILA_B77",
			"USB_2_H_EN",
			"BT_DISABLE#",
			"WIFI_DISABLE#",
			"CTRL_ETH_REF_CLK_STBY",
			"CTRL_DP_BRIDGE_EN";
	};

	som_gpio_expander_1: gpio@21 {
		compatible = "nxp,pcal6416";
		reg = <0x21>;
		#interrupt-cells = <2>;
		interrupt-controller;
		interrupt-parent = <&gpio1>;
		interrupts = <13 IRQ_TYPE_LEVEL_LOW>;
		#gpio-cells = <2>;
		gpio-controller;
		gpio-line-names =
			"AQUILA_C1", /* 0 */
			"AQUILA_C2",
			"AQUILA_C3",
			"AQUILA_C4",
			"AQUILA_C36",
			"AQUILA_B74",
			"AQUILA_B75",
			"USB_2_H_OC#",
			"AQUILA_B81",
			"PMIC_SD_1_VSEL",
			"ETH_1_INT#", /* 10 */
			"CTRL_TPM_INT#",
			"SPI_2_CS2_TPM",
			"PCIE_WAKE_WIFI#",
			"WIFI_WAKE_BT",
			"WIFI_WAKEUP_HOST";
	};

	som_dsi2dp_bridge: bridge@2c {
		compatible = "ti,sn65dsi86";
		reg = <0x2c>;
		clocks = <&clk_dsi2dp_refclk_en>;
		clock-names = "refclk";
		vcc-supply = <&reg_dp_1p2v>;
		vcca-supply = <&reg_dp_1p2v>;
		vccio-supply = <&reg_1p8v>;
		vpll-supply = <&reg_1p8v>;

		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				dsi2dp_in: endpoint {
				};
			};

			port@1 {
				reg = <1>;

				dsi2dp_out: endpoint {
					data-lanes = <3 2 1 0>;
				};
			};
		};
	};

	rtc_i2c: rtc@32 {
		compatible = "epson,rx8130";
		reg = <0x32>;
	};

	temperature-sensor@48 {
		compatible = "ti,tmp1075";
		reg = <0x48>;
	};

	som_eeprom: eeprom@50 {
		compatible = "st,24c02", "atmel,24c02";
		reg = <0x50>;
		pagesize = <16>;
	};
};

/* Aquila I2C_4_CSI1 */
&lpi2c4 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_lpi2c4>;
	pinctrl-1 = <&pinctrl_lpi2c4_gpio>;
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <100000>;
	scl-gpios = <&gpio2 31 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio2 30 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

/* Aquila I2C_6 */
&lpi2c5 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_lpi2c5>;
	pinctrl-1 = <&pinctrl_lpi2c5_gpio>;
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <100000>;
	scl-gpios = <&gpio2 23 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio2 22 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

/* Aquila I2C_3_DSI1/I2C_5_CSI2 */
&lpi2c8 {
	pinctrl-names = "default", "gpio";
	pinctrl-0 = <&pinctrl_lpi2c8>;
	pinctrl-1 = <&pinctrl_lpi2c8_gpio>;
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <100000>;
	scl-gpios = <&gpio2 13 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
	sda-gpios = <&gpio2 12 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
};

/* Aquila SPI_2 */
&lpspi4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_lpspi4>;
	cs-gpios = <&gpio2 18 GPIO_ACTIVE_LOW>,
		   <&som_gpio_expander_1 12 GPIO_ACTIVE_LOW>;

	status = "okay";

	som_tpm: tpm@1 {
		compatible = "infineon,slb9670", "tcg,tpm_tis-spi";
		reg = <0x1>;
		interrupt-parent = <&som_gpio_expander_1>;
		interrupts = <11 IRQ_TYPE_EDGE_FALLING>;
		/*
		 * Maximum TPM-supported speed is 18.5 MHz, limited to 12 MHz
		 * here as lpspi4's per-clock (2x the max speed) is 24 MHz.
		 */
		spi-max-frequency = <12000000>;
	};
};

/* Aquila SPI_1 */
&lpspi6 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_lpspi6>;
	cs-gpios = <&gpio2 0 GPIO_ACTIVE_LOW>;
};

/* Aquila UART_3, used as the Linux Console */
&lpuart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
};

/* Aquila UART_4 */
&lpuart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
};

/* Aquila UART_1 */
&lpuart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	uart-has-rtscts;
};

/* Aquila UART_2 */
&lpuart7 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart7>;
	uart-has-rtscts;
};

&mu7 {
	status = "okay";
};

/* Aquila ETH_2_XGMII_MDIO, shared between all ethernet ports */
&netc_emdio {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_emdio>;

	status = "okay";

	ethphy1: ethernet-phy@1 {
		reg = <1>;
		interrupt-parent = <&som_gpio_expander_1>;
		interrupts = <10 IRQ_TYPE_EDGE_FALLING>;
		ti,rx-internal-delay = <DP83867_RGMIIDCTL_2_00_NS>;
		ti,tx-internal-delay = <DP83867_RGMIIDCTL_2_00_NS>;
	};
};

&netcmix_blk_ctrl {
	status = "okay";
};

&netc_blk_ctrl {
	status = "okay";
};

&netc_timer {
	status = "okay";
};

/* Aquila PCIE_1 */
&pcie0 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pcie0>;
	reset-gpios = <&som_gpio_expander_0 0 GPIO_ACTIVE_LOW>;
};

/* On-module Wi-Fi or Aquila PCIE_2 */
&pcie1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pcie1>;
	reset-gpios = <&som_gpio_expander_0 1 GPIO_ACTIVE_LOW>;

	status = "okay";
};

/* Aquila I2S_1 */
&sai2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_sai2>;
	assigned-clocks = <&scmi_clk IMX95_CLK_AUDIOPLL1_VCO>,
			  <&scmi_clk IMX95_CLK_AUDIOPLL2_VCO>,
			  <&scmi_clk IMX95_CLK_AUDIOPLL1>,
			  <&scmi_clk IMX95_CLK_AUDIOPLL2>,
			  <&scmi_clk IMX95_CLK_SAI2>;
	assigned-clock-parents = <0>, <0>, <0>, <0>,
				 <&scmi_clk IMX95_CLK_AUDIOPLL1>;
	assigned-clock-rates = <3932160000>,
			       <3612672000>, <393216000>,
			       <361267200>, <12288000>;
	#sound-dai-cells = <0>;
	fsl,sai-mclk-direction-output;
};

&scmi_bbm {
	linux,code = <KEY_POWER>;
};

&thermal_zones {
	/* PF09 Main PMIC */
	pf09-thermal {
		polling-delay = <2000>;
		polling-delay-passive = <250>;
		thermal-sensors = <&scmi_sensor 2>;

		trips {
			trip0 {
				hysteresis = <2000>;
				temperature = <155000>;
				type = "critical";
			};
		};
	};

	/* PF53 VDD_ARM PMIC */
	pf53-arm-thermal {
		polling-delay = <2000>;
		polling-delay-passive = <250>;
		thermal-sensors = <&scmi_sensor 4>;

		trips {
			trip0 {
				hysteresis = <2000>;
				temperature = <155000>;
				type = "critical";
			};
		};
	};

	/* PF53 VDD_SOC PMIC */
	pf53-soc-thermal {
		polling-delay = <2000>;
		polling-delay-passive = <250>;
		thermal-sensors = <&scmi_sensor 3>;

		trips {
			trip0 {
				hysteresis = <2000>;
				temperature = <155000>;
				type = "critical";
			};
		};
	};
};

/* Aquila PWM_1 */
&tpm3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>;
};

/* Aquila PWM_2 */
&tpm6 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm2>;
};

/* Aquila PWM_3_DSI and PWM_4_DP */
&tpm5 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm3_dsi>, <&pinctrl_pwm4_dp>;
};

/* Aquila USB_2, optional Bluetooth USB */
&usb2 {
	dr_mode = "host";
	vbus-supply = <&reg_usb2_vbus>;
};

/* Aquila USB_1 */
&usb3 {
	fsl,disable-port-power-control;
};

&usb3_dwc3 {
	dr_mode = "otg";
	adp-disable;
	hnp-disable;
	srp-disable;
	usb-role-switch;
};

&usb3_phy {
	vbus-supply = <&reg_usb1_vbus>;
};

/* On-module eMMC */
&usdhc1 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz";
	pinctrl-0 = <&pinctrl_usdhc1>;
	pinctrl-1 = <&pinctrl_usdhc1>;
	pinctrl-2 = <&pinctrl_usdhc1_200mhz>;
	bus-width = <8>;
	non-removable;
	no-sdio;
	no-sd;

	status = "okay";
};

/* Aquila SD_1 */
&usdhc2 {
	pinctrl-names = "default", "state_100mhz", "state_200mhz", "sleep";
	pinctrl-0 = <&pinctrl_usdhc2>, <&pinctrl_sd1_cd_gpio>;
	pinctrl-1 = <&pinctrl_usdhc2>, <&pinctrl_sd1_cd_gpio>;
	pinctrl-2 = <&pinctrl_usdhc2_200mhz>,<&pinctrl_sd1_cd_gpio>;
	pinctrl-3 = <&pinctrl_usdhc2_sleep>, <&pinctrl_sd1_cd_gpio>;
	cd-gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
	vmmc-supply = <&reg_usdhc2_vmmc>;
	vqmmc-supply = <&reg_usdhc2_vqmmc>;
};

&wdog3 {
	fsl,ext-reset-output;

	status = "okay";
};

&scmi_iomuxc {
	/* Aquila CTRL_WAKE1_MICO# */
	pinctrl_ctrl_wake1_mico: ctrlwake1micogrp {
		fsl,pins = <IMX95_PAD_XSPI1_SS1_B__GPIO5_IO_BIT11	0x31e>; /* Aquila D6 */
	};

	pinctrl_ctrl_dp_clk_en: dpclkengrp {
		fsl,pins = <IMX95_PAD_SAI1_TXFS__AONMIX_TOP_GPIO1_IO_BIT11	0x11e>; /* CTRL_DP_CLK_EN */
	};

	/* Aquila ETH_2_XGMII_MDIO */
	pinctrl_emdio: emdiogrp {
		fsl,pins = <IMX95_PAD_ENET2_MDC__NETCMIX_TOP_NETC_MDC	0x57e>, /* Aquila B90 */
			   <IMX95_PAD_ENET2_MDIO__NETCMIX_TOP_NETC_MDIO	0x97e>; /* Aquila B89 */
	};

	/* Aquila ETH_1 */
	pinctrl_enetc0: enetc0grp {
		fsl,pins = <IMX95_PAD_ENET1_TX_CTL__NETCMIX_TOP_ETH0_RGMII_TX_CTL	0x57e>, /* ENET1_TX_CTL */
			   <IMX95_PAD_ENET1_TXC__NETCMIX_TOP_ETH0_RGMII_TX_CLK		0x58e>, /* ENET1_TXC    */
			   <IMX95_PAD_ENET1_TD0__NETCMIX_TOP_ETH0_RGMII_TD0		0x50e>, /* ENET1_TDO    */
			   <IMX95_PAD_ENET1_TD1__NETCMIX_TOP_ETH0_RGMII_TD1		0x50e>, /* ENET1_TD1    */
			   <IMX95_PAD_ENET1_TD2__NETCMIX_TOP_ETH0_RGMII_TD2		0x50e>, /* ENET1_TD2    */
			   <IMX95_PAD_ENET1_TD3__NETCMIX_TOP_ETH0_RGMII_TD3		0x50e>, /* ENET1_TD3    */
			   <IMX95_PAD_ENET1_RX_CTL__NETCMIX_TOP_ETH0_RGMII_RX_CTL	0x57e>, /* ENET1_RX_CTL */
			   <IMX95_PAD_ENET1_RXC__NETCMIX_TOP_ETH0_RGMII_RX_CLK		0x58e>, /* ENET1_RXC    */
			   <IMX95_PAD_ENET1_RD0__NETCMIX_TOP_ETH0_RGMII_RD0		0x57e>, /* ENET1_RD0    */
			   <IMX95_PAD_ENET1_RD1__NETCMIX_TOP_ETH0_RGMII_RD1		0x57e>, /* ENET1_RD1    */
			   <IMX95_PAD_ENET1_RD2__NETCMIX_TOP_ETH0_RGMII_RD2		0x57e>, /* ENET1_RD2    */
			   <IMX95_PAD_ENET1_RD3__NETCMIX_TOP_ETH0_RGMII_RD3		0x57e>; /* ENET1_RD3    */
	};

	/* Aquila CAN_1 */
	pinctrl_flexcan1: flexcan1grp {
		fsl,pins = <IMX95_PAD_PDM_CLK__AONMIX_TOP_CAN1_TX		0x39e>, /* Aquila B48 */
			   <IMX95_PAD_PDM_BIT_STREAM0__AONMIX_TOP_CAN1_RX	0x39e>; /* Aquila B49 */
	};

	/* Aquila CAN_2 */
	pinctrl_flexcan2: flexcan2grp {
		fsl,pins = <IMX95_PAD_GPIO_IO25__CAN2_TX	0x39e>, /* Aquila B50 */
			   <IMX95_PAD_GPIO_IO27__CAN2_RX	0x39e>; /* Aquila B51 */
	};

	/* Aquila CAN_3 */
	pinctrl_flexcan3: flexcan3grp {
		fsl,pins = <IMX95_PAD_CCM_CLKO3__CAN3_TX	0x39e>, /* Aquila B53 */
			   <IMX95_PAD_CCM_CLKO4__CAN3_RX	0x39e>; /* Aquila B54 */
	};

	/* Aquila CAN_4 */
	pinctrl_flexcan4: flexcan4grp {
		fsl,pins = <IMX95_PAD_GPIO_IO04__CAN4_TX	0x39e>, /* Aquila B55 */
			   <IMX95_PAD_GPIO_IO05__CAN4_RX	0x39e>; /* Aquila B56 */
	};

	/* Aquila QSPI_1 (4 bit) */
	pinctrl_flexspi1_4bit: flexspi14bitgrp {
		fsl,pins = <IMX95_PAD_XSPI1_SCLK__FLEXSPI1_A_SCLK	0x3fe>, /* Aquila B65 */
			   <IMX95_PAD_XSPI1_DATA0__FLEXSPI1_A_DATA_BIT0	0x3fe>, /* Aquila B68 */
			   <IMX95_PAD_XSPI1_DATA1__FLEXSPI1_A_DATA_BIT1	0x3fe>, /* Aquila B67 */
			   <IMX95_PAD_XSPI1_DATA2__FLEXSPI1_A_DATA_BIT2	0x3fe>, /* Aquila B61 */
			   <IMX95_PAD_XSPI1_DATA3__FLEXSPI1_A_DATA_BIT3	0x3fe>, /* Aquila B60 */
			   <IMX95_PAD_XSPI1_DQS__FLEXSPI1_A_DQS		0x3fe>; /* Aquila B63 */
	};

	/* Aquila QSPI_1 (8 bit) */
	pinctrl_flexspi1_8bit: flexspi18bitgrp {
		fsl,pins = <IMX95_PAD_XSPI1_SCLK__FLEXSPI1_A_SCLK	0x3fe>, /* Aquila B65 */
			   <IMX95_PAD_XSPI1_DATA0__FLEXSPI1_A_DATA_BIT0	0x3fe>, /* Aquila B68 */
			   <IMX95_PAD_XSPI1_DATA1__FLEXSPI1_A_DATA_BIT1	0x3fe>, /* Aquila B67 */
			   <IMX95_PAD_XSPI1_DATA2__FLEXSPI1_A_DATA_BIT2	0x3fe>, /* Aquila B61 */
			   <IMX95_PAD_XSPI1_DATA3__FLEXSPI1_A_DATA_BIT3	0x3fe>, /* Aquila B60 */
			   <IMX95_PAD_XSPI1_DATA4__FLEXSPI1_A_DATA_BIT4	0x3fe>, /* Aquila B70 */
			   <IMX95_PAD_XSPI1_DATA5__FLEXSPI1_A_DATA_BIT5	0x3fe>, /* Aquila B71 */
			   <IMX95_PAD_XSPI1_DATA6__FLEXSPI1_A_DATA_BIT6	0x3fe>, /* Aquila B72 */
			   <IMX95_PAD_XSPI1_DATA7__FLEXSPI1_A_DATA_BIT7	0x3fe>, /* Aquila B73 */
			   <IMX95_PAD_XSPI1_DQS__FLEXSPI1_A_DQS		0x3fe>; /* Aquila B63 */
	};

	/* Aquila GPIO_01 */
	pinctrl_gpio_1: gpio1grp {
		fsl,pins = <IMX95_PAD_ENET2_RD0__GPIO4_IO_BIT24	0x31e>; /* Aquila D23 */
	};

	/* Aquila GPIO_02 */
	pinctrl_gpio_2: gpio2grp {
		fsl,pins = <IMX95_PAD_ENET2_RD1__GPIO4_IO_BIT25	0x31e>; /* Aquila D24 */
	};

	/* Aquila GPIO_03 */
	pinctrl_gpio_3: gpio3grp {
		fsl,pins = <IMX95_PAD_ENET2_RD3__GPIO4_IO_BIT27	0x31e>; /* Aquila D25 */
	};

	/* Aquila GPIO_04 */
	pinctrl_gpio_4: gpio4grp {
		fsl,pins = <IMX95_PAD_ENET2_TD0__GPIO4_IO_BIT19	0x31e>; /* Aquila C20 */
	};

	/* Aquila GPIO_05 */
	pinctrl_gpio_5: gpio5grp {
		fsl,pins = <IMX95_PAD_ENET2_TD1__GPIO4_IO_BIT18	0x31e>; /* Aquila C21 */
	};

	/* Aquila GPIO_06 */
	pinctrl_gpio_6: gpio6grp {
		fsl,pins = <IMX95_PAD_ENET2_TD2__GPIO4_IO_BIT17	0x31e>; /* Aquila C22 */
	};

	/* Aquila GPIO_07 */
	pinctrl_gpio_7: gpio7grp {
		fsl,pins = <IMX95_PAD_ENET2_RXC__GPIO4_IO_BIT23	0x31e>; /* Aquila C23 */
	};

	/* Aquila GPIO_08 */
	pinctrl_gpio_8: gpio8grp {
		fsl,pins = <IMX95_PAD_PDM_BIT_STREAM1__AONMIX_TOP_GPIO1_IO_BIT10	0x31e>; /* Aquila C24 */
	};

	/* Aquila GPIO_09_CSI_1 */
	pinctrl_gpio_9_csi_1: gpio9csi1grp {
		fsl,pins = <IMX95_PAD_SAI1_TXC__AONMIX_TOP_GPIO1_IO_BIT12	0x31e>; /* Aquila B17 */
	};

	/* Aquila GPIO_10_CSI_1 */
	pinctrl_gpio_10_csi_1: gpio10csi1grp {
		fsl,pins = <IMX95_PAD_SAI1_RXD0__AONMIX_TOP_GPIO1_IO_BIT14	0x31e>; /* Aquila B18 */
	};

	/* Aquila GPIO_11_CSI_1 */
	pinctrl_gpio_11_csi_1: gpio11csi1grp {
		fsl,pins = <IMX95_PAD_SD2_VSELECT__GPIO3_IO_BIT19	0x31e>; /* Aquila A11*/
	};

	/* Aquila GPIO_12_CSI_1 */
	pinctrl_gpio_12_csi_1: gpio12csi1grp {
		fsl,pins = <IMX95_PAD_SD3_DATA0__GPIO3_IO_BIT22	0x31e>; /* Aquila B19 */
	};

	/* Aquila GPIO_17_DSI_1 */
	pinctrl_gpio_17_dsi_1: gpio17dsi1grp {
		fsl,pins = <IMX95_PAD_GPIO_IO07__GPIO2_IO_BIT7	0x31e>; /* Aquila B42 */
	};

	/* Aquila GPIO_18_DSI_1 */
	pinctrl_gpio_18_dsi_1: gpio18dsi1grp {
		fsl,pins = <IMX95_PAD_GPIO_IO09__GPIO2_IO_BIT9	0x31e>; /* Aquila B43 */
	};

	/* Aquila GPIO_19_DSI_1 */
	pinctrl_gpio_19_dsi_1: gpio19dsi1grp {
		fsl,pins = <IMX95_PAD_GPIO_IO33__GPIO5_IO_BIT13	0x31e>; /* Aquila B44 */
	};

	/* Aquila GPIO_20_DSI_1 */
	pinctrl_gpio_20_dsi_1: gpio20dsi1grp {
		fsl,pins = <IMX95_PAD_GPIO_IO34__GPIO5_IO_BIT14	0x31e>; /* Aquila B45 */
	};

	/* Aquila GPIO_21_DP */
	pinctrl_gpio_21_dp: gpio21dpgrp {
		fsl,pins = <IMX95_PAD_SD3_CMD__GPIO3_IO_BIT21	0x31e>; /* Aquila B57 */
	};

	pinctrl_ctrl_gpio_exp_int: gpioexpintgrp {
		fsl,pins = <IMX95_PAD_SAI1_TXD0__AONMIX_TOP_GPIO1_IO_BIT13	0x31e>; /* CTRL_GPIO_EXP_INT# */
	};

	/* Aquila I2C_2 */
	pinctrl_i3c2: i3c2cgrp {
		fsl,pins = <IMX95_PAD_ENET1_MDC__I3C2_SCL	0x40001186>, /* Aquila C17 */
			   <IMX95_PAD_ENET1_MDIO__I3C2_SDA	0x40001186>; /* Aquila C16 */
	};

	/* Aquila I2C_1 as GPIOs */
	pinctrl_lpi2c2_gpio: lpi2c2gpiogrp {
		fsl,pins = <IMX95_PAD_I2C2_SCL__AONMIX_TOP_GPIO1_IO_BIT2	0x40001b9e>, /* Aquila D8 */
			   <IMX95_PAD_I2C2_SDA__AONMIX_TOP_GPIO1_IO_BIT3	0x40001b9e>; /* Aquila D7 */
	};

	/* Aquila I2C_1 */
	pinctrl_lpi2c2: lpi2c2grp {
		fsl,pins = <IMX95_PAD_I2C2_SCL__AONMIX_TOP_LPI2C2_SCL	0x40001b9e>, /* Aquila D8 */
			   <IMX95_PAD_I2C2_SDA__AONMIX_TOP_LPI2C2_SDA	0x40001b9e>; /* Aquila D7 */
	};

	/* On-module I2C as GPIOs */
	pinctrl_lpi2c3_gpio: lpi2c3gpiogrp {
		fsl,pins = <IMX95_PAD_GPIO_IO28__GPIO2_IO_BIT28	0x40001b9e>, /* I2C_SOM_SDA */
			   <IMX95_PAD_GPIO_IO29__GPIO2_IO_BIT29	0x40001b9e>; /* I2C_SOM_SCL */
	};

	/* On-module I2C */
	pinctrl_lpi2c3: lpi2c3grp {
		fsl,pins = <IMX95_PAD_GPIO_IO28__LPI2C3_SDA	0x40001b9e>, /* I2C_SOM_SDA */
			   <IMX95_PAD_GPIO_IO29__LPI2C3_SCL	0x40001b9e>; /* I2C_SOM_SCL */
	};

	/* Aquila I2C_4_CSI1 as GPIO */
	pinctrl_lpi2c4_gpio: lpi2c4gpiogrp {
		fsl,pins = <IMX95_PAD_GPIO_IO30__GPIO2_IO_BIT30	0x40001b9e>, /* Aquila A12 */
			   <IMX95_PAD_GPIO_IO31__GPIO2_IO_BIT31	0x40001b9e>; /* Aquila A13 */
	};

	/* Aquila I2C_4_CSI1 */
	pinctrl_lpi2c4: lpi2c4grp {
		fsl,pins = <IMX95_PAD_GPIO_IO30__LPI2C4_SDA	0x40001b9e>, /* Aquila A12 */
			   <IMX95_PAD_GPIO_IO31__LPI2C4_SCL	0x40001b9e>; /* Aquila A13 */
	};

	/* Aquila I2C_6 as GPIO */
	pinctrl_lpi2c5_gpio: lpi2c5gpiogrp {
		fsl,pins = <IMX95_PAD_GPIO_IO22__GPIO2_IO_BIT22	0x40001b9e>, /* Aquila C18 */
			   <IMX95_PAD_GPIO_IO23__GPIO2_IO_BIT23	0x40001b9e>; /* Aquila C19 */
	};

	/* Aquila I2C_6 */
	pinctrl_lpi2c5: lpi2c5grp {
		fsl,pins = <IMX95_PAD_GPIO_IO22__LPI2C5_SDA	0x40001b9e>, /* Aquila C18 */
			   <IMX95_PAD_GPIO_IO23__LPI2C5_SCL	0x40001b9e>; /* Aquila C19 */
	};

	/* Aquila I2C_3_DSI1/I2C_5_CSI2 as GPIO */
	pinctrl_lpi2c8_gpio: lpi2c8gpiogrp {
		fsl,pins = <IMX95_PAD_GPIO_IO12__GPIO2_IO_BIT12	0x40001b9e>, /* Aquila C5/B40 */
			   <IMX95_PAD_GPIO_IO13__GPIO2_IO_BIT13	0x40001b9e>; /* Aquila C6/B41 */
	};

	/* Aquila I2C_3_DSI1/I2C_5_CSI2 */
	pinctrl_lpi2c8: lpi2c8grp {
		fsl,pins = <IMX95_PAD_GPIO_IO12__LPI2C8_SDA	0x40001b9e>, /* Aquila C5/B40 */
			   <IMX95_PAD_GPIO_IO13__LPI2C8_SCL	0x40001b9e>; /* Aquila C6/B41 */
	};

	/* Aquila SPI_2 */
	pinctrl_lpspi4: lpspi4grp {
		fsl,pins = <IMX95_PAD_GPIO_IO18__GPIO2_IO_BIT18	0x3fe>, /* Aquila D16 */
			   <IMX95_PAD_GPIO_IO19__LPSPI4_SIN	0x3fe>, /* Aquila D15 */
			   <IMX95_PAD_GPIO_IO20__LPSPI4_SOUT	0x3fe>, /* Aquila D17 */
			   <IMX95_PAD_GPIO_IO21__LPSPI4_SCK	0x3fe>; /* Aquila D14 */
	};

	/* Aquila SPI_1 */
	pinctrl_lpspi6: lpspi6grp {
		fsl,pins = <IMX95_PAD_GPIO_IO00__GPIO2_IO_BIT0	0x3fe>, /* Aquila D9 */
			   <IMX95_PAD_GPIO_IO01__LPSPI6_SIN	0x3fe>, /* Aquila D10 */
			   <IMX95_PAD_GPIO_IO02__LPSPI6_SOUT	0x3fe>, /* Aquila D11 */
			   <IMX95_PAD_GPIO_IO03__LPSPI6_SCK	0x3fe>; /* Aquila D12 */
	};

	/* Aquila PCIE_1 */
	pinctrl_pcie0: pcie0grp {
		fsl,pins = <IMX95_PAD_GPIO_IO32__HSIOMIX_TOP_PCIE1_CLKREQ_B	0x40001b1e>; /* Aquila C37 */
	};

	/* Aquila PCIE_2 */
	pinctrl_pcie1: pcie1grp {
		fsl,pins = <IMX95_PAD_GPIO_IO35__HSIOMIX_TOP_PCIE2_CLKREQ_B	0x40001b1e>; /* Aquila C34 */
	};

	/* Aquila QSPI_1_CS1# */
	pinctrl_qspi_cs1: qspics1grp {
		fsl,pins = <IMX95_PAD_XSPI1_SS0_B__FLEXSPI1_A_SS0_B	0x3fe>; /* Aquila B66 */
	};

	/* Aquila QSPI_1_CS2# as GPIO */
	pinctrl_qspi_cs2_gpio: qspics2gpiogrp {
		fsl,pins = <IMX95_PAD_CCM_CLKO2__GPIO3_IO_BIT27	0x3fe>; /* Aquila B62 */
	};

	/* Aquila I2S_1 */
	pinctrl_sai2: sai2grp {
		fsl,pins = <IMX95_PAD_ENET2_TX_CTL__NETCMIX_TOP_SAI2_TX_SYNC		0x11e>, /* Aquila B21 */
			   <IMX95_PAD_ENET2_TXC__NETCMIX_TOP_SAI2_TX_BCLK		0x11e>, /* Aquila B20 */
			   <IMX95_PAD_ENET2_TD3__NETCMIX_TOP_SAI2_RX_DATA_BIT0		0x11e>, /* Aquila B23 */
			   <IMX95_PAD_ENET2_RX_CTL__NETCMIX_TOP_SAI2_TX_DATA_BIT0	0x11e>; /* Aquila B22 */
	};

	pinctrl_sai2_mclk: sai2mclkgrp {
		fsl,pins = <IMX95_PAD_ENET2_RD2__NETCMIX_TOP_SAI2_MCLK	0x31e>; /* Aquila B24 */
	};

	/* Aquila SD_1_CD# as GPIO */
	pinctrl_sd1_cd_gpio: sd1cdgpiogrp {
		fsl,pins = <IMX95_PAD_SD2_CD_B__GPIO3_IO_BIT0	0x1100>; /* Aquila A1 */
	};

	/* Aquila SD_1_PWR_EN */
	pinctrl_sd1_pwr_en: sd1pwrengpiogrp {
		fsl,pins = <IMX95_PAD_SD2_RESET_B__GPIO3_IO_BIT7	0x11e>; /* Aquila A6 */
	};

	/* Aquila PWM_1 */
	pinctrl_pwm1: tpm3ch3grp {
		fsl,pins = <IMX95_PAD_GPIO_IO24__TPM3_CH3	0x11e>; /* Aquila C25 */
	};

	/* Aquila PWM_3_DSI as GPIO */
	pinctrl_pwm3_dsi_gpio: tpm5ch0gpiogrp {
		fsl,pins = <IMX95_PAD_GPIO_IO06__GPIO2_IO_BIT6	0x11e>; /* Aquila B46 */
	};

	/* Aquila PWM_3_DSI */
	pinctrl_pwm3_dsi: tpm5ch0grp {
		fsl,pins = <IMX95_PAD_GPIO_IO06__TPM5_CH0	0x11e>; /* Aquila B46 */
	};

	/* Aquila PWM_4_DP */
	pinctrl_pwm4_dp: tpm5ch3grp {
		fsl,pins = <IMX95_PAD_GPIO_IO26__TPM5_CH3	0x11e>; /* Aquila B58 */
	};

	/* Aquila PWM_2 */
	pinctrl_pwm2: tpm6ch0grp {
		fsl,pins = <IMX95_PAD_GPIO_IO08__TPM6_CH0	0x11e>; /* Aquila C26 */
	};

	/* Aquila UART_3 */
	pinctrl_uart1: uart1grp {
		fsl,pins = <IMX95_PAD_UART1_TXD__AONMIX_TOP_LPUART1_TX	0x31e>, /* Aquila D20 */
			   <IMX95_PAD_UART1_RXD__AONMIX_TOP_LPUART1_RX	0x31e>; /* Aquila D19 */
	};

	/* Aquila UART_4 */
	pinctrl_uart2: uart2grp {
		fsl,pins = <IMX95_PAD_UART2_TXD__AONMIX_TOP_LPUART2_TX	0x31e>, /* Aquila D22 */
			   <IMX95_PAD_UART2_RXD__AONMIX_TOP_LPUART2_RX	0x31e>; /* Aquila D21 */
	};

	/* Aquila UART_1 */
	pinctrl_uart3: uart3grp {
		fsl,pins = <IMX95_PAD_GPIO_IO14__LPUART3_TX	0x31e>, /* Aquila B37 */
			   <IMX95_PAD_GPIO_IO15__LPUART3_RX	0x31e>, /* Aquila B35 */
			   <IMX95_PAD_GPIO_IO16__LPUART3_CTS_B	0x31e>, /* Aquila B36 */
			   <IMX95_PAD_GPIO_IO17__LPUART3_RTS_B	0x31e>; /* Aquila B38 */
	};

	/* Aquila UART_2 */
	pinctrl_uart7: uart7grp {
		fsl,pins = <IMX95_PAD_GPIO_IO36__LPUART7_TX	0x31e>, /* Aquila B33 */
			   <IMX95_PAD_GPIO_IO37__LPUART7_RX	0x31e>, /* Aquila B31 */
			   <IMX95_PAD_GPIO_IO10__LPUART7_CTS_B	0x31e>, /* Aquila B32 */
			   <IMX95_PAD_GPIO_IO11__LPUART7_RTS_B	0x31e>; /* Aquila B34 */
	};

	/* On-module eMMC */
	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <IMX95_PAD_SD1_CLK__USDHC1_CLK	0x158e>, /* eMMC_CLK    */
			   <IMX95_PAD_SD1_CMD__USDHC1_CMD	0x138e>, /* eMMC_CMD    */
			   <IMX95_PAD_SD1_DATA0__USDHC1_DATA0	0x138e>, /* eMMC_DATA0  */
			   <IMX95_PAD_SD1_DATA1__USDHC1_DATA1	0x138e>, /* eMMC_DATA1  */
			   <IMX95_PAD_SD1_DATA2__USDHC1_DATA2	0x138e>, /* eMMC_DATA2  */
			   <IMX95_PAD_SD1_DATA3__USDHC1_DATA3	0x138e>, /* eMMC_DATA3  */
			   <IMX95_PAD_SD1_DATA4__USDHC1_DATA4	0x138e>, /* eMMC_DATA4  */
			   <IMX95_PAD_SD1_DATA5__USDHC1_DATA5	0x138e>, /* eMMC_DATA5  */
			   <IMX95_PAD_SD1_DATA6__USDHC1_DATA6	0x138e>, /* eMMC_DATA6  */
			   <IMX95_PAD_SD1_DATA7__USDHC1_DATA7	0x138e>, /* eMMC_DATA7  */
			   <IMX95_PAD_SD1_STROBE__USDHC1_STROBE	0x158e>; /* eMMC_STROBE */
	};

	pinctrl_usdhc1_200mhz: usdhc1-200mhzgrp {
		fsl,pins = <IMX95_PAD_SD1_CLK__USDHC1_CLK	0x15fe>, /* eMMC_CLK    */
			   <IMX95_PAD_SD1_CMD__USDHC1_CMD	0x13fe>, /* eMMC_CMD    */
			   <IMX95_PAD_SD1_DATA0__USDHC1_DATA0	0x13fe>, /* eMMC_DATA0  */
			   <IMX95_PAD_SD1_DATA1__USDHC1_DATA1	0x13fe>, /* eMMC_DATA1  */
			   <IMX95_PAD_SD1_DATA2__USDHC1_DATA2	0x13fe>, /* eMMC_DATA2  */
			   <IMX95_PAD_SD1_DATA3__USDHC1_DATA3	0x13fe>, /* eMMC_DATA3  */
			   <IMX95_PAD_SD1_DATA4__USDHC1_DATA4	0x13fe>, /* eMMC_DATA4  */
			   <IMX95_PAD_SD1_DATA5__USDHC1_DATA5	0x13fe>, /* eMMC_DATA5  */
			   <IMX95_PAD_SD1_DATA6__USDHC1_DATA6	0x13fe>, /* eMMC_DATA6  */
			   <IMX95_PAD_SD1_DATA7__USDHC1_DATA7	0x13fe>, /* eMMC_DATA7  */
			   <IMX95_PAD_SD1_STROBE__USDHC1_STROBE	0x15fe>; /* eMMC_STROBE */
	};

	/* Aquila SD_1 */
	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <IMX95_PAD_SD2_CLK__USDHC2_CLK	0x158e>, /* Aquila A5  */
			   <IMX95_PAD_SD2_CMD__USDHC2_CMD	0x138e>, /* Aquila A7  */
			   <IMX95_PAD_SD2_DATA0__USDHC2_DATA0	0x138e>, /* Aquila A3  */
			   <IMX95_PAD_SD2_DATA1__USDHC2_DATA1	0x138e>, /* Aquila A2  */
			   <IMX95_PAD_SD2_DATA2__USDHC2_DATA2	0x138e>, /* Aquila A10 */
			   <IMX95_PAD_SD2_DATA3__USDHC2_DATA3	0x138e>; /* Aquila A8  */
	};

	pinctrl_usdhc2_200mhz: usdhc2-200mhzgrp {
		fsl,pins = <IMX95_PAD_SD2_CLK__USDHC2_CLK	0x15fe>, /* Aquila A5  */
			   <IMX95_PAD_SD2_CMD__USDHC2_CMD	0x13fe>, /* Aquila A7  */
			   <IMX95_PAD_SD2_DATA0__USDHC2_DATA0	0x13fe>, /* Aquila A3  */
			   <IMX95_PAD_SD2_DATA1__USDHC2_DATA1	0x13fe>, /* Aquila A2  */
			   <IMX95_PAD_SD2_DATA2__USDHC2_DATA2	0x13fe>, /* Aquila A10 */
			   <IMX95_PAD_SD2_DATA3__USDHC2_DATA3	0x13fe>; /* Aquila A8  */
	};

	pinctrl_usdhc2_sleep: usdhc2-sleepgrp {
		fsl,pins = <IMX95_PAD_SD2_CLK__USDHC2_CLK	0x400>, /* Aquila A5  */
			   <IMX95_PAD_SD2_CMD__USDHC2_CMD	0x400>, /* Aquila A7  */
			   <IMX95_PAD_SD2_DATA0__USDHC2_DATA0	0x400>, /* Aquila A3  */
			   <IMX95_PAD_SD2_DATA1__USDHC2_DATA1	0x400>, /* Aquila A2  */
			   <IMX95_PAD_SD2_DATA2__USDHC2_DATA2	0x400>, /* Aquila A10 */
			   <IMX95_PAD_SD2_DATA3__USDHC2_DATA3	0x400>; /* Aquila A8  */
	};
};
