// SPDX-License-Identifier: GPL-2.0

#include <dt-bindings/input/input.h>
#include "tegra30.dtsi"

/ {
	chosen {
		stdout-path = &uarta;
	};

	aliases {
		i2c0 = &pwr_i2c;

		mmc0 = &sdmmc4;	/* eMMC */

		rtc0 = &pmic;
		rtc1 = "/rtc@7000e000";

		usb0 = &usb1;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x40000000>;
	};

	host1x@50000000 {
		dc@54200000 {
			nvidia,180-rotation;
			rgb {
				status = "okay";

				nvidia,panel = <&panel>;
			};
		};
	};

	gpio@6000d000 {
		volume-buttons-hog {
			gpio-hog;
			gpios = <TEGRA_GPIO(R, 0) GPIO_ACTIVE_HIGH>,
				<TEGRA_GPIO(Q, 0) GPIO_ACTIVE_HIGH>;
			output-low;
		};
	};

	bsev@6001b000 {
		status = "okay";
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			clk_32k_out_pa0 {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,function = "blink";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart3_cts_n_pa1 {
				nvidia,pins = "uart3_cts_n_pa1",
						"uart3_rxd_pw7";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap2_fs_pa2 {
				nvidia,pins = "dap2_fs_pa2",
						"dap2_sclk_pa3",
						"dap2_din_pa4",
						"dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_clk_pa6 {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_cmd_pa7 {
				nvidia,pins = "sdmmc3_cmd_pa7",
						"sdmmc3_dat3_pb4",
						"sdmmc3_dat2_pb5",
						"sdmmc3_dat1_pb6",
						"sdmmc3_dat0_pb7",
						"sdmmc3_dat4_pd1",
						"sdmmc3_dat6_pd3",
						"sdmmc3_dat7_pd4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi_a17_pb0 {
				nvidia,pins = "gmi_a17_pb0",
						"gmi_a18_pb1";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			lcd_pwr0_pb2 {
				nvidia,pins = "lcd_pwr0_pb2",
						"lcd_pwr1_pc1",
						"lcd_m1_pw1";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd_pclk_pb3 {
				nvidia,pins = "lcd_pclk_pb3",
						"lcd_d0_pe0",
						"lcd_d1_pe1",
						"lcd_d2_pe2",
						"lcd_d3_pe3",
						"lcd_d4_pe4",
						"lcd_d5_pe5",
						"lcd_d6_pe6",
						"lcd_d7_pe7",
						"lcd_d8_pf0",
						"lcd_d9_pf1",
						"lcd_d10_pf2",
						"lcd_d11_pf3",
						"lcd_d12_pf4",
						"lcd_d13_pf5",
						"lcd_d14_pf6",
						"lcd_d15_pf7",
						"lcd_de_pj1",
						"lcd_hsync_pj3",
						"lcd_vsync_pj4",
						"lcd_d16_pm0",
						"lcd_d17_pm1",
						"lcd_d18_pm2",
						"lcd_d19_pm3",
						"lcd_d20_pm4",
						"lcd_d21_pm5",
						"lcd_d22_pm6",
						"lcd_d23_pm7",
						"lcd_cs0_n_pn4",
						"lcd_sdout_pn5",
						"lcd_dc0_pn6",
						"lcd_cs1_n_pw0",
						"lcd_sdin_pz2",
						"lcd_sck_pz4";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uart3_rts_n_pc0 {
				nvidia,pins = "uart3_rts_n_pc0",
						"uart3_txd_pw6";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_txd_pc2 {
				nvidia,pins = "uart2_txd_pc2",
						"uart2_rts_n_pj6";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			uart2_rxd_pc3 {
				nvidia,pins = "uart2_rxd_pc3",
						"uart2_cts_n_pj5";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gen1_i2c_scl_pc4 {
				nvidia,pins = "gen1_i2c_scl_pc4",
						"gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			gmi_wp_n_pc7 {
				nvidia,pins = "gmi_wp_n_pc7",
						"gmi_wait_pi7",
						"gmi_cs4_n_pk2",
						"gmi_cs3_n_pk4";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad12_ph4 {
				nvidia,pins = "gmi_ad12_ph4",
						"gmi_cs0_n_pj0",
						"gmi_cs1_n_pj2",
						"gmi_cs2_n_pk3";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc3_dat5_pd0 {
				nvidia,pins = "sdmmc3_dat5_pd0";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad0_pg0 {
				nvidia,pins = "gmi_ad0_pg0",
						"gmi_ad1_pg1",
						"gmi_ad14_ph6",
						"pu1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad2_pg2 {
				nvidia,pins = "gmi_ad2_pg2",
						"gmi_ad3_pg3",
						"gmi_ad6_pg6",
						"gmi_ad7_pg7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad4_pg4 {
				nvidia,pins = "gmi_ad4_pg4",
						"gmi_ad5_pg5";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi_ad8_ph0 {
				nvidia,pins = "gmi_ad8_ph0";
				nvidia,function = "pwm0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad9_ph1 {
				nvidia,pins = "gmi_ad9_ph1";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad10_ph2 {
				nvidia,pins = "gmi_ad10_ph2";
				nvidia,function = "pwm2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad11_ph3 {
				nvidia,pins = "gmi_ad11_ph3";
				nvidia,function = "pwm3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad13_ph5 {
				nvidia,pins = "gmi_ad13_ph5",
						"gmi_wr_n_pi0",
						"gmi_oe_n_pi1",
						"gmi_adv_n_pk0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_ad15_ph7 {
				nvidia,pins = "gmi_ad15_ph7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_dqs_pi2 {
				nvidia,pins = "gmi_dqs_pi2",
						"pu2",
						"pv1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi_rst_n_pi4 {
				nvidia,pins = "gmi_rst_n_pi4";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_iordy_pi5 {
				nvidia,pins = "gmi_iordy_pi5";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gmi_cs7_n_pi6 {
				nvidia,pins = "gmi_cs7_n_pi6",
						"gmi_clk_pk1";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gmi_a16_pj7 {
				nvidia,pins = "gmi_a16_pj7",
						"gmi_a19_pk7";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_out_pk5 {
				nvidia,pins = "spdif_out_pk5";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spdif_in_pk6 {
				nvidia,pins = "spdif_in_pk6";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap1_fs_pn0 {
				nvidia,pins = "dap1_fs_pn0",
						"dap1_din_pn1",
						"dap1_dout_pn2",
						"dap1_sclk_pn3";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			hdmi_int_pn7 {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,function = "hdmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_data7_po0 {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ulpi_data3_po4 {
				nvidia,pins = "ulpi_data3_po4";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap3_fs_pp0 {
				nvidia,pins = "dap3_fs_pp0";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			dap4_fs_pp4 {
				nvidia,pins = "dap4_fs_pp4",
						"dap4_din_pp5",
						"dap4_dout_pp6",
						"dap4_sclk_pp7";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col0_pq0 {
				nvidia,pins = "kb_col0_pq0",
						"kb_col1_pq1",
						"kb_row1_pr1";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_col2_pq2 {
				nvidia,pins = "kb_col2_pq2",
						"kb_col3_pq3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_col4_pq4 {
				nvidia,pins = "kb_col4_pq4",
						"kb_col5_pq5",
						"kb_col7_pq7",
						"kb_row2_pr2",
						"kb_row4_pr4",
						"kb_row5_pr5",
						"kb_row14_ps6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			kb_row0_pr0 {
				nvidia,pins = "kb_row0_pr0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row6_pr6 {
				nvidia,pins = "kb_row6_pr6",
						"kb_row8_ps0",
						"kb_row9_ps1",
						"kb_row10_ps2";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			kb_row11_ps3 {
				nvidia,pins = "kb_row11_ps3",
						"kb_row12_ps4";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			gen2_i2c_scl_pt5 {
				nvidia,pins = "gen2_i2c_scl_pt5",
						"gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_cmd_pt7 {
				nvidia,pins = "sdmmc4_cmd_pt7",
						"sdmmc4_dat0_paa0",
						"sdmmc4_dat1_paa1",
						"sdmmc4_dat2_paa2",
						"sdmmc4_dat3_paa3",
						"sdmmc4_dat4_paa4",
						"sdmmc4_dat5_paa5",
						"sdmmc4_dat6_paa6",
						"sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pu0 {
				nvidia,pins = "pu0",
						"pu6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			jtag_rtck_pu7 {
				nvidia,pins = "jtag_rtck_pu7";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pv0 {
				nvidia,pins = "pv0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ddc_scl_pv4 {
				nvidia,pins = "ddc_scl_pv4",
						"ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			crt_hsync_pv6 {
				nvidia,pins = "crt_hsync_pv6",
						"crt_vsync_pv7";
				nvidia,function = "crt";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			spi2_cs1_n_pw2 {
				nvidia,pins = "spi2_cs1_n_pw2",
						"spi2_miso_px1",
						"spi2_sck_px2";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk1_out_pw4 {
				nvidia,pins = "clk1_out_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2_out_pw5 {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "extperiph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			spi2_cs0_n_px3 {
				nvidia,pins = "spi2_cs0_n_px3";
				nvidia,function = "spi6";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			spi1_mosi_px4 {
				nvidia,pins = "spi1_mosi_px4",
						"spi1_cs0_n_px6";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ulpi_clk_py0 {
				nvidia,pins = "ulpi_clk_py0",
						"ulpi_dir_py1";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sdmmc1_dat3_py4 {
				nvidia,pins = "sdmmc1_dat3_py4",
						"sdmmc1_dat2_py5",
						"sdmmc1_dat1_py6",
						"sdmmc1_dat0_py7",
						"sdmmc1_cmd_pz1";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_clk_pz0 {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			lcd_wr_n_pz3 {
				nvidia,pins = "lcd_wr_n_pz3";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sys_clk_req_pz5 {
				nvidia,pins = "sys_clk_req_pz5";
				nvidia,function = "sysclk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pwr_i2c_scl_pz6 {
				nvidia,pins = "pwr_i2c_scl_pz6",
						"pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pbb0 {
				nvidia,pins = "pbb0",
						"pcc1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			cam_i2c_scl_pbb1 {
				nvidia,pins = "cam_i2c_scl_pbb1",
						"cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
			};
			pbb3 {
				nvidia,pins = "pbb3";
				nvidia,function = "vgp3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb4 {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb5 {
				nvidia,pins = "pbb5";
				nvidia,function = "vgp5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb6 {
				nvidia,pins = "pbb6";
				nvidia,function = "vgp6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pbb7 {
				nvidia,pins = "pbb7",
						"pcc2";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			cam_mclk_pcc0 {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_rst_n_pcc3 {
				nvidia,pins = "sdmmc4_rst_n_pcc3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_clk_pcc4 {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk2_req_pcc5 {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			pex_l2_rst_n_pcc6 {
				nvidia,pins = "pex_l2_rst_n_pcc6",
						"pex_l2_clkreq_n_pcc7";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pex_wake_n_pdd3 {
				nvidia,pins = "pex_wake_n_pdd3",
						"pex_l2_prsnt_n_pdd7";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			clk3_out_pee0 {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			clk1_req_pee2 {
				nvidia,pins = "clk1_req_pee2";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			hdmi_cec_pee3 {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_DISABLE>;
			};
			owr {
				nvidia,pins = "owr";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			drive_dap1 {
				nvidia,pins = "drive_dap1",
						"drive_dap2",
						"drive_dbg",
						"drive_at5",
						"drive_gme",
						"drive_ddc",
						"drive_ao1",
						"drive_uart3";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};
			drive_sdio1 {
				nvidia,pins = "drive_sdio1",
						"drive_sdio3";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <46>;
				nvidia,pull-up-strength = <42>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FAST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FAST>;
			};
			drive_gma {
				nvidia,pins = "drive_gma",
						"drive_gmb",
						"drive_gmc",
						"drive_gmd";
				nvidia,pull-down-strength = <9>;
				nvidia,pull-up-strength = <9>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
			};
		};
	};

	uarta: serial@70006000 {
		status = "okay";
	};

	pwm: pwm@7000a000 {
		status = "okay";
	};

	pwr_i2c: i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;
	};

	sdmmc4: mmc@78000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;

		vmmc-supply = <&vcore_emmc>;
		vqmmc-supply = <&vdd_1v8_vio>;
	};

	usb1: usb@7d000000 {
		status = "okay";
		dr_mode = "otg";
	};

	usb-phy@7d000000 {
		status = "okay";
		nvidia,hssync-start-delay = <0>;
		nvidia,xcvr-lsfslew = <2>;
		nvidia,xcvr-lsrslew = <2>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";

		enable-gpios = <&gpio TEGRA_GPIO(H, 2) GPIO_ACTIVE_HIGH>;
		power-supply = <&vdd_5v0_bl>;
		pwms = <&pwm 0 50000>;

		brightness-levels = <1 35 70 105 140 175 210 255>;
		default-brightness-level = <5>;
	};

	/* PMIC has a built-in 32KHz oscillator which is used by PMC */
	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "pmic-oscillator";
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(V, 0) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_ENTER>;
		};

		key-volume-up {
			label = "Volume Up";
			gpios = <&gpio TEGRA_GPIO(Q, 2) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_UP>;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio TEGRA_GPIO(Q, 3) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_DOWN>;
		};

		switch-hall-sensor {
			label = "Lid";
			gpios = <&gpio TEGRA_GPIO(S, 6) GPIO_ACTIVE_LOW>;
			linux,code = <SW_LID>;
		};
	};

	panel: panel {
		compatible = "simple-panel";

		power-supply = <&vdd_pnl_reg>;
		enable-gpios = <&gpio TEGRA_GPIO(N, 6) GPIO_ACTIVE_HIGH>;

		backlight = <&backlight>;

		display-timings {
			timing@0 {
				/* 1280x800@60Hz */
				clock-frequency = <68000000>;

				hactive = <800>;
				hfront-porch = <24>;
				hback-porch = <32>;
				hsync-len = <24>;

				vactive = <1280>;
				vfront-porch = <5>;
				vback-porch = <32>;
				vsync-len = <1>;
			};
		};
	};

	vdd_pnl_reg: regulator-pnl {
		compatible = "regulator-fixed";
		regulator-name = "vdd_panel";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio TEGRA_GPIO(W, 1) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vdd_5v0_bl: regulator-bl {
		compatible = "regulator-fixed";
		regulator-name = "vdd_5v0_bl";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(H, 3) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};
